CONSOLIDATED CHECKLIST C5
	Part 5 of 5 parts

	Standards for Owners and Operators of Hazardous Waste Treatment,
	Storage, and Disposal Facilities
	40 CFR Part 264, Subparts CC-EE, as of December 31, 2002
	
Note: Consolidated Checklist C5 is divided into five separate documents/computer files solely for ease of handling its printed and electronic versions.  Consolidated Checklist C5 remains one checklist; States must adopt all five portions simultaneously to correctly use this Consolidated Checklist.  Note, the prenotes and endnotes associated with each part have been placed with the part to which they apply.

Note: No final rules affecting 40 CFR Part 264, Subparts CC‑EE were promulgated between June 30, 2002 and December 31, 2002, therefore, this Consolidated Checklist corresponds to 40 CFR Part 264, Subparts CC‑EE as published on July 1, 2002.

	
FEDERAL REQUIREMENTS	
CHECKLIST
REFERENCE	
FEDERAL RCRA CITATION	
ANALOGOUS STATE CITATION	
STATE ANALOG IS:	
					
EQUIV-ALENT	
LESS
STRIN-
GENT	
MORE STRIN-GENT	
BROADER IN SCOPE	

PART 264 - STANDARDS FOR OWNERS AND OPERATORS OF HAZARDOUS WASTE TREATMENT, STORAGE, AND DISPOSAL FACILITIES	

SUBPART CC - AIR EMISSIONS STANDARDS FOR TANKS,
SURFACE IMPOUNDMENTS, AND CONTAINERS	

APPLICABILITY	

264, Subpart CC requirements apply to owners/operators of all facilities that treat, store, or dispose of hazardous waste in tanks, surface impoundments, or containers except as in 264.1 & 264.1080(b)	
154	
264.1080(a)	

	

	
264, Subpart CC requirements do not apply to the following waste management units at the facility:	
154	
264.1080(b)	

	

	
waste management unit that holds hazardous waste placed in it before December 6, 1996 & to which none is added on or after December 6, 1996	
154,163	
264.1080(b)(1)	

	

	
container with design capacity of less than or equal to 0.1 m3	
154	
264.1080(b)(2)	

	

	
tank to which an owner/operator has stopped adding hazardous waste & has begun implementing or completed closure  pursuant to plan	
154	
264.1080(b)(3)	

	

	
surface impoundment in which owner/operator has stopped adding hazardous waste & has begun implementing or completed closure pursuant to plan	
154	
264.1080(b)(4)	

	

	
waste management unit used solely for on-site treatment or storage of hazardous waste placed in the unit as a result of remedial activities	
154,177	
264.1080(b)(5)	

	

	
waste management unit used solely for management of radioactive mixed waste	
154	
264.1080(b)(6)	

	

	
hazardous waste management unit equipped with & operating air emission controls in accordance with Clean Air Act; a tank for which air emission control includes an enclosure must comply with 264.1084(i), except as in 264.1082(c)(5)	
154	
264.1080(b)(7)	

	

	
tank with process vent as defined in 264.1031	
154	
264.1080(b)(8)	

	

	
for owners/operators of a facility subject to 264, Subpart CC who have received a final permit before December 6, 1996, 264, Subpart CC requirements are incorporated into a permit when reissued or reviewed; until such date owner/operator is subject to 265, Subpart CC requirements	
154,163	
264.1080(c)	

	

	
administrative stay of subpart CC requirements, with exception of 264.1089(i), for tanks or containers used to manage hazardous waste from organic  peroxide manufacturing & associated laboratory operations when owner/operator meets the specified conditions	
154	
264.1080(d)	

	

		
154	
264.1080(d)(1)	

	

		
154	
264.1080(d)(2)	

	

		
154	
264.1080(d)(3)	

	

	
DEFINITIONS	

264, Subpart CC terms have meanings given them in 265.1081, the Act, & Parts 260-266	
154	
264.1081	

	

	
STANDARDS:  GENERAL	

264.1082 applies to management of hazardous waste in tanks, surface impoundments, & containers subject to 264, Subpart CC	
154	
264.1082(a)	

	

	
owner or operator shall control air pollutant emissions from hazardous waste management unit in accordance with 264.1084 - 264.1087, except as in 264.1082(c)	
154,163	
264.1082(b)	

	

	
tank, surface impoundment, or container is exempt from standards specified in 264.1084- 264.1087, provided that it is:	
154	
264.1082(c)	

	

	
tank, surface impoundment, or container for which entering hazardous waste has average VO concentration at point of origination of less than 500ppmw; how VO concentration is determined; frequency of reviews and updates	
154	
264.1082(c)(1)	

	

	
tank, surface impoundment, or container for which the organic content of the hazardous waste entering the waste management unit is reduced by organic destruction or removal that achieves any of the following conditions:	
154	
264.1082(c)(2)	

	

	
process that removes or destroys organics to level such that average VO concentration at the point of treatment < the exit concentration limit established for the process; how average VO concentration is determined	
154	
264.1082(c)(2)(i)	

	

	
process that removes or destroys organics to a level such that organic reduction efficiency $ 95% & average VO concentration at point of treatment is < 100 ppmw; how organic reduction efficiency and average VO concentration are determined	
154	
264.1082(c)(2)(ii)	

	

	
process that removes or destroys organics to level such that actual organic mass removal rate $ required organic mass removal rate established for the process; how required organic mass removal rate & actual organic mass removal rate are determined	
154	
264.1082(c)(2)(iii)	

	

	
biological process that destroys or degrades organics contained in hazardous waste such that either of following conditions is met:	
154	
264.1082(c)(2)(iv)	

	

	
organic reduction efficiency for process $95 %& organic biodegradation efficiency$ 95 %; how organic reduction efficiency & biodegradation efficiency are determined	
154	
264.1082(c)(2)(iv)(A)	

	

	
total actual organic  mass biodegradation rate for hazardous waste treated by the process $ required organic mass removal rate; how organic mass removal rate & actual mass biodegradation rate are determined	
154	
264.1082(c)(2)(iv)(B)	

	

	
process that removes or destroys organics contained in hazardous waste & meets all of the specified conditions	
154	
264.1082(c)(2)(v)	

	

		
154	
264.1082(c)(2)(v)(A)	

	

		
154	
264.1082(c)(2)(v)(B)	

	

		
154	
264.1082(c)(2)(v)(C)	

	

	
process that removes or destroys organics in hazardous waste to specified levels; specified levels to be determined using procedures in 264.1083(a)&(b)	
154	
264.1082(c)(2)(vi)	

	

	
hazardous waste incinerator for which the owner or operator has either:	
154	
264.1082(c)(2)(vii)	

	

	
been issued a final permit under part 270 which implements part 264, subpart O; or	
154	
264.1082(c)(2)(vii)(A)	

	

	
has designed & operates the incinerator in accordance with interim status requirements of part 265, subpart O	
154	
264.1082(c)(2)(vii)(B)	

	

	
boiler or industrial furnace for which owner/operator has either:	
154	
264.1082(c)(2)(viii)	

	

	
been issued a final permit under part 270 which implements part 266, subpart H; or	
154	
264.1082(c)(2)(viii)(A)	

	

	
designed & operates boiler or furnace in accordance with interim status requirements of 266, subpart H	
154	
264.1082(c)(2)(viii)(B)	

	

	
for determining performance of organic destruction process, owner/operator shall account for VO concentrations below detection limit by using following:	
154	
264.1082(c)(2)(ix)	

	

	
if Method 25D in part 60, appendix A is used, 2 of blank value determined in the method at section 4.4 of Method 25D, appendix A, or a value of 25 ppmw, whichever is less	
154,163	
264.1082(c)(2)(ix)(A)	

	

	
if other analytical method used, one-half sum of limits of detection established for each organic constituent in waste that has Henry=s law constant value at least 0.1 Y/X at 25 degrees Celsius	
154,163	
264.1082(c)(2)(ix)(B)	

	

	
tank or surface impoundment used for biological treatment of hazardous waste in accordance with 264.1082(c)(2)(iv)	
154,163	
264.1082(c)(3)	

	

	
tank, surface impoundment, or container for which hazardous waste placed in unit that either:	
154	
264.1082(c)(4)	

	

	
meets numerical concentration limits for organic constituents in 268.40; or	
154	
264.1082(c)(4)(i)	

	

	
organic hazardous constituents in waste have been treated as in 268.42(a), or have been removed or destroyed by equivalent method pursuant to 268.42(b)	
154,163	
264.1082(c)(4)(ii)	

	

	
tank used for bulk feed of hazardous waste to an incinerator & all of following are met:	
154	
264.1082(c)(5)	

	

	
tank is inside enclosure vented to control device designed & operated in accordance with part 61, subpart FF for facility generating $ 10 megagrams of benzene per year	
154	
264.1082(c)(5)(i)	

	

	
tank's enclosure & control device installed & began operation prior to November 25, 1996 &	
154	
264.1082(c)(5)(ii)	

	

	
enclosure designed & operated in accordance with 52.741, appendix B; allowance for openings; verification as specified in ' 5.0	
154	
264.1082(c)(5)(iii)	

	

	
Regional Administrator may perform, or request the owner or operator perform, waste determination for hazardous waste managed in a tank, surface impoundment, or container exempt from using air emission controls under 264.1082 as follows:	
154	
264.1082(d)	

	

	
waste determination for average VO concentration of hazardous waste at point of waste origination shall be performed using direct measurement in accordance with 264.1083(a) requirements; how  determination will be performed	
154	
264.1082(d)(1)	

	

	
in performing waste determination pursuant to 264.1082(d)(1), sample preparation shall be conducted as follows:	
154	
264.1082(d)(2)	

	

	
in accordance with method used by owner/operator, except as specified by 264.1082(d)(2)(ii)	
154	
264.1082(d)(2)(i)	

	

	
if Regional Administrator determines owner/ operator's methods inappropriate, then may choose appropriate one	
154	
264.1082(d)(2)(ii)	

	

	
when owner/ operator performs waste determination, Regional Administrator may have an authorized representative observe sampling 	
154	
264.1082(d)(3)	

	

	
if results of waste determination performed or requested by Regional Administrator do not agree with results of waste determination performed by owner/operator, then results of waste determination performed under 264.1082(d)(1) shall be used	
154	
264.1082(d)(4)	

	

	
if averaging period of greater than 1 hour used to determine average VO concentration of hazardous waste at point of origination, Regional Administrator can establish 264, Subpart CC compliance by performing or requesting that owner/operator perform a waste determination based on samples collected within 1-hour period as specified	
154	
264.1082(d)(5)	

	

		
154	
264.1082(d)(5)(i)	

	

		
154	
264.1082(d)(5)(ii)	

	

		
154	
264.1082(d)(5)(iii)	

	

	
WASTE DETERMINATION PROCEDURES	

waste determination procedure to determine average VO concentration of hazardous waste at point of origination	
154	
264.1083(a)	

	

	
average VO concentration at point of waste origination shall be determined for each hazardous waste placed in a unit  exempted under 264.1082(c)(1) from using air emission controls in accordance with 264.1084-1087	
154	
264.1083(a)(1)	

	

	
average VO concentration of waste stream shall be determined before first time material in hazardous waste stream is placed in unit exempted under 264.1082(c)(1) from using air emission controls,  thereafter concentration shall be determined for each averaging period that hazardous waste is managed in unit; and	
177	
264.1083(a)(1)(i)	

	

	
perform new determination when changes to generating source are likely to cause concentration to increase to level equal to or greater than limit specified in 264.1082	
177	
264.1083(a)(1)(ii)	

	

	
for waste determination that is required by 264.1083(a)(1), average VO concentration at point of waste origination shall be determined in accordance with 265.1084(a)(2)-(4)	
154,163	
264.1083(a)(2)	

	

	
waste determination procedures for treated hazardous waste	
154	
264.1083(b)	

	

	
owner/operator shall perform applicable waste determination for each treated hazardous waste placed in units exempted under 264.1082(c)(2)(i) through 264.1082(c)(2)(vi) from using air emission controls in accordance with 264.1084-1087	
154,163	
264.1083(b)(1)	

	

	
average VO concentration of waste stream shall be determined before first time material in treated waste stream is placed in exempt unit, thereafter update determination information at least once every 12 months; and	
177	
264.1083(b)(1)(i)	

	

	
perform new determination when process generating or treating waste stream changes are likely to cause concentration to increase such that 264.1082(c)(2) treatment conditions are not achieved	
177	
264.1083(b)(1)(ii)	

	

	
the waste determination for a treated hazardous waste shall be performed in accordance with 265.1084(b)(2)-(9)	
154	
264.1083(b)(2)	

	

	
procedure to determine maximum organic vapor pressure of hazardous waste in a tank	
154	
264.1083(c)	

	

	
an owner/operator shall determine maximum organic vapor pressure for each hazardous waste placed in a  tank using Tank Level 1 controls in accordance with 264.1084(c)	
154	
264.1083(c)(1)	

	

	
maximum organic vapor pressure of hazardous waste may be determined in accordance with 265.1084(c)(2)-(4)	
154	
264.1083(c)(2)	

	

	
procedure for determining no detectable organic emissions shall be conducted in accordance with 265.1084(d)	
154	
264.1083(d)	

	

	
STANDARDS:  TANKS	

provisions of 264.1084 apply to control of air pollutant emissions from tanks for which 264.1082(b) references the use of 264.1084 for such air emission control	
154	
264.1084(a)	

	

	
owner/operator shall control air pollutant emissions from each tank subject to 264.1084 in  accordance with the following:	
154	
264.1084(b)	

	

	
requirements for a tank that manages hazardous waste & meets the conditions in 264.1084(b)(1)(i)-(iii)	
154	
264.1084(b)(1)	

	

	
hazardous waste in the tank has maximum organic vapor pressure less than limit for tank's capacity category as specified	
154	
264.1084(b)(1)(i)	

	

		
154	
264.1084(b)(1)(i)(A)	

	

		
154	
264.1084(b)(1)(i)(B)	

	

		
154	
264.1084(b)(1)(i)(C)	

	

	
hazardous waste in the tank is not heated by owner/operator to temperature at which maximum organic vapor pressure is determined to comply with 264.1084(b)(1)(i)	
154	
264.1084(b)(1)(ii)	

	

	
hazardous waste in tank is not treated by owner/operator using waste stabilization process, as in 265.1081	
154	
264.1084(b)(1)(iii)	

	

	
requirements for tanks that do not meet 264.1084(b)(1)(i)-(iii)	
154	
264.1084(b)(2)	

	

	
owners/operators controlling air pollutant emissions from tank using Tank Level 1 controls meet requirements in 264.1084(c)(1)-(c)(4) 	
154	
264.1084(c)	

	

	
owner/operator to determine maximum organic vapor pressure for hazardous waste in tank using Tank Level 1 controls before placing waste in tank; maximum organic vapor pressure to be determined using 264.1083(c); when  determinations shall be performed	
154	
264.1084(c)(1)	

	

	
tank shall be equipped with fixed roof designed to meet the following:	
154	
264.1084(c)(2)	

	

	
fixed roof & its closure devices shall form continuous barrier over surface of hazardous waste in the tank; what is a fixed roof	
154	
264.1084(c)(2)(i)	

	

	
installed without visible cracks, holes, gaps, or open spaces between joints/edges	
154	
264.1084(c)(2)(ii)	

	

	
openings and any manifold system associated with  fixed roof shall be equipped with a closure device or connected by a closed-vent system	
154,163	
264.1084(c)(2)(iii)	

	

		
154	
264.1084(c)(2)(iii)(A)	

	

		
154,163	
264.1084(c)(2)(iii)(B)	

	

		
163	
264.1084(c)(2)(iii)(B)(1)	

	

		
163	
264.1084(c)(2)(iii)(B)(2)	

	

	
fixed roof & its closure devices shall consist of materials to minimize exposure of hazardous waste to atmosphere, & maintain integrity throughout service life; factors for selecting materials	
154	
264.1084(c)(2)(iv)	

	

	
when hazardous waste is in the tank, fixed roof shall be installed with closure device secured in closed position except:	
154	
264.1084(c)(3)	

	

	
opening of closure devices or removal of fixed roof is allowed to provide access or to remove accumulated sludge	
154	
264.1084(c)(3)(i)	

	

		
154	
264.1084(c)(3)(i)(A)	

	

		
154	
264.1084(c)(3)(i)(B)	

	

	
opening of pressure relief devices which vent to the atmosphere during normal operations to maintain internal pressure; designed to operate with no detectable emissions when closed; remain in closed position when internal pressure is within operating range determined by owner/operator; normal operating conditions	
154	
264.1084(c)(3)(ii)	

	

	
opening of safety device allowed to avoid an unsafe condition	
154	
264.1084(c)(3)(iii)	

	

	
owner/operator shall inspect & monitor air emission control equipment as follows:	
154	
264.1084(c)(4)	

	

	
fixed roof & closure devices to be visually inspected for defects; examples	
154	
264.1084(c)(4)(i)	

	

	
initial inspection of fixed roof & closure devices on or before tank is subject to 264.1084; then at least once a year except under 264.1084(l)	
154	
264.1084(c)(4)(ii)	

	

	
in event of defect, shall be repaired in accordance with 264.1084(k)	
154	
264.1084(c)(4)(iii)	

	

	
owner/operator shall maintain inspection record in accordance with 264.1089(b)	
154	
264.1084(c)(4)(iv)	

	

	
owners/operators controlling air pollutant emissions from a tank using Tank Level 2 controls shall use one of the following:	
154	
264.1084(d)	

	

	
fixed-roof tank equipped with internal floating roof in accordance with 264.1084(e)	
154	
264.1084(d)(1)	

	

	
tank equipped with external floating roof in accordance with 264.1084(f)	
154	
264.1084(d)(2)	

	

	
tank vented through a closed-vent system to control device in accordance with 264.1084(g)	
154	
264.1084(d)(3)	

	

	
pressure tank designed & operated in accordance with 264.1084(h); or	
154	
264.1084(d)(4)	

	

	
tank inside an enclosure vented through a closed-vent system to an enclosed combustion control device in accordance with 264.1084(i) 	
154	
264.1084(d)(5)	

	

	
owner/operator who controls emissions from a tank using a fixed roof with internal floating roof shall meet 264.1084(e)(1)-(3) requirements	
154	
264.1084(e)	

	

	
tank shall be equipped with fixed roof & internal floating roof in accordance with the following:	
154	
264.1084(e)(1)	

	

	
internal floating roof shall be designed to  float on liquid surface except when supported by leg supports	
154	
264.1084(e)(1)(i)	

	

	
internal floating roof shall be equipped with continuous seal that meets specified conditions 	
154	
264.1084(e)(1)(ii)	

	

		
154	
264.1084(e)(1)(ii)(A)	

	

		
154	
264.1084(e)(1)(ii)(B)	

	

	
internal floating roof shall meet listed specifications	
154	
264.1084(e)(1)(iii)	

	

		
154	
264.1084(e)(1)(iii)(A)	

	

		
154	
264.1084(e)(1)(iii)(B)	

	

		
154	
264.1084(e)(1)(iii)(C)	

	

		
154	
264.1084(e)(1)(iii)(D)	

	

		
154	
264.1084(e)(1)(iii)(E)	

	

		
154	
264.1084(e)(1)(iii)(F)	

	

	
owner/operator shall operate the tank in accordance with the following:	
154	
264.1084(e)(2)	

	

	
when floating roof is resting on leg supports, filling, emptying, or refilling shall be continuous & completed as soon as practical	
154	
264.1084(e)(2)(i)	

	

	
automatic bleeder vents to be closed at all times when roof is floating, except when roof is being floated off or landed on leg supports 	
154	
264.1084(e)(2)(ii)	

	

	
prior to filling tank, openings in internal floating roof shall be closed; rim space vents open only when internal floating roof is not floating or when pressure exceeds manufacturer's recommended setting 	
154	
264.1084(e)(2)(iii)	

	

	
owner/operator shall inspect internal floating roof in accordance with the following:	
154	
264.1084(e)(3)	

	

	
floating roof & its closure devices shall be visually inspected for defects which could result in air pollutant emissions; potential defects	
154	
264.1084(e)(3)(i)	

	

	
owner/operator shall inspect internal floating roof components with specified visual inspections except as provided in 264.1084(e)(3)(iii)	
154	
264.1084(e)(3)(ii)	

	

		
154	
264.1084(e)(3)(ii)(A)	

	

		
154	
264.1084(e)(3)(ii)(B)	

	

	
as alternative to 264.1084(e)(3)(ii) inspections for internal floating roof equipped with two continuous seals, owner/operator may perform visual inspection each time tank is emptied & degassed & at least every 5 years	
154	
264.1084(e)(3)(iii)	

	

	
before 264.1084(e)(3)(ii)-(iii) inspections, owner/operator shall notify Regional Administrator in advance to allow for observer during the inspection; & notify Regional Administrator of date & location of inspection	
154	
264.1084(e)(3)(iv)	

	

		
154	
264.1084(e)(3)(iv)(A)	

	

		
154	
264.1084(e)(3)(iv)(B)	

	

	
in event of a defect, it shall be repaired in accordance with 264.1084(k)	
154	
264.1084(e)(3)(v)	

	

	
owner/operator shall maintain inspection record in accordance with 264.1089(b)	
154	
264.1084(e)(3)(vi)	

	

	
safety devices, as defined in 40 CFR 265.1081, may be installed and operated as necessary on tank complying with 264.1084 requirements	
163	
264.1084(e)(4)	

	

	
owner/operator who controls emissions from tank using external floating roof shall meet requirements in 264.1084(f)(1)-(3)	
154	
264.1084(f)	

	

	
owner/operator shall design external floating roof in accordance with the following:	
154	
264.1084(f)(1)	

	

	
external floating roof designed to float on liquid surface except when supported by leg supports	
154	
264.1084(f)(1)(i)	

	

	
floating roof equipped with two continuous seals; the lower seal referred to as primary seal & upper seal as secondary seal	
154	
264.1084(f)(1)(ii)	

	

		
154	
264.1084(f)(1)(ii)(A)	

	

		
154	
264.1084(f)(1)(ii)(B)	

	

	

external floating roof shall meet certain specifications	
154	
264.1084(f)(1)(iii)	

	

		
154	
264.1084(f)(1)(iii)(A)	

	

		
154	
264.1084(f)(1)(iii)(B)	

	

		
154	
264.1084(f)(1)(iii)(C)	

	

		
154	
264.1084(f)(1)(iii)(D)	

	

		
154	
264.1084(f)(1)(iii)(E)	

	

		
154	
264.1084(f)(1)(iii)(F)	

	

		
154	
264.1084(f)(1)(iii)(G)	

	

		
154	
264.1084(f)(1)(iii)(H)	

	

		
154	
264.1084(f)(1)(iii)(I)	

	

	
owner/operator shall operate tank in accordance with the following:	
154	
264.1084(f)(2)	

	

	
when floating roof resting on leg supports, filling, emptying, or refilling shall be continuous & completed as soon as practical	
154	
264.1084(f)(2)(i)	

	

	
except for automatic bleeder vents, rim space vents, roof drains, & leg sleeves, roof openings shall be secured & closed at all times except when closure device must be open for access 	
154	
264.1084(f)(2)(ii)	

	

	
covers on each access hatch & gauge float well shall be bolted or fastened if in closed position 	
154	
264.1084(f)(2)(iii)	

	

	
automatic bleeder vents to be closed at all times when roof floating, except when roof is being floated off or landed on leg supports	
154	
264.1084(f)(2)(iv)	

	

	
rim space vents shall be open only when roof is being floated off the leg supports or when pressure beneath rim seal exceeds manufacturer's recommended setting	
154	
264.1084(f)(2)(v)	

	

	
cap on end of unslotted guide poles shall be closed at all times except when measuring liquid level or collecting samples	
154	
264.1084(f)(2)(vi)	

	

	
cover on each gauge hatch or sample well shall be closed at all times except when hatch or well must be accessed 	
154	
264.1084(f)(2)(vii)	

	

	
both primary & secondary seals shall completely cover annular space between external floating roof & tank wall in continuous fashion except during inspections 	
154	
264.1084(f)(2)(viii)	

	

	
owner/operator shall inspect external floating roof in accordance with the following:	
154	
264.1084(f)(3)	

	

	
owner/operator shall measure external floating roof seal gaps in accordance with specified requirements	
154	
264.1084(f)(3)(i)	

	

		
154	
264.1084(f)(3)(i)(A)	

	

		
154	
264.1084(f)(3)(i)(B)	

	

		
154	
264.1084(f)(3)(i)(C)	

	

		
154	
264.1084(f)(3)(i)(D)	

	

		
154	
264.1084(f)(3)(i)(D)(1)	

	

		
154	
264.1084(f)(3)(i)(D)(2)	

	

		
154	
264.1084(f)(3)(i)(D)(3)	

	

		
154,163	
264.1084(f)(3)(i)(D)(4)	

	

		
154	
264.1084(f)(3)(i)(E)	

	

		
154	
264.1084(f)(3)(i)(F)	

	

	
owner/operator shall visually inspect external floating roof in accordance with specified requirements	
154	
264.1084(f)(3)(ii)	

	

		
154	
264.1084(f)(3)(ii)(A)	

	

		
154	
264.1084(f)(3)(ii)(B)	

	

		
154	
264.1084(f)(3)(ii)(B)	

	

		
154	
264.1084(f)(3)(ii)(C)	

	

		
154	
264.1084(f)(3)(ii)(D)	

	

	
prior to 264.1084(f)(3)(i) or (ii) inspections, owner/operator shall notify Regional Administrator in advance to allow for observer present during inspection; & notify of date & location of inspection	
154,163	
264.1084(f)(3)(iii)	

	

		
154	
264.1084(f)(3)(iii)(A)	

	

		
154	
264.1084(f)(3)(iii)(B)	

	

		
154	
264.1084(f)(3)(iii)(C)	

	

	
safety devices, as defined in 40 CFR 265.1081, may be installed and operated on tank complying with 264.1084(f)	
163	
264.1084(f)(4)	

	

	
owner/operator who controls air pollutant emissions from a tank by venting to a control device shall meet requirements in 264.1084(g)(1)-(3) 	
154	
264.1084(g)	

	

	
tank shall be covered by fixed roof and vented directly to a control device in accordance with the following:	
154	
264.1084(g)(1)	

	

	
fixed roof & closure devices shall form continuous barrier over liquid in tank	
154	
264.1084(g)(1)(i)	

	

	
each opening in fixed roof not vented to control device shall be equipped with closure device; when pressure in vapor headspace < atmospheric pressure; when pressure in vapor headspace $ atmospheric pressure	
154	
264.1084(g)(1)(ii)	

	

	
fixed roof & its closure devices shall be made of suitable materials that will minimize exposure to atmosphere & maintain integrity throughout service life; factors to consider when selecting materials	
154	
264.1084(g)(1)(iii)	

	

	
the closed-vent system & control device shall be designed & operated in accordance with 264.1087	
154	
264.1084(g)(1)(iv)	

	

	
whenever hazardous waste is in the tank, fixed roof shall be installed with closure device secured in closed position except:	
154	
264.1084(g)(2)	

	

	
venting to control device is not required, & opening of closure device or removal of fixed roof is allowed in specified circumstances	
154	
264.1084(g)(2)(i)	

	

		
154	
264.1084(g)(2)(i)(A)	

	

		
154	
264.1084(g)(2)(i)(B)	

	

	
opening of a safety device, as defined in 265.1081, is allowed any time to avoid an unsafe condition	
154	
264.1084(g)(2)(ii)	

	

	
owner/operator shall inspect & monitor air emission control equipment as follows:	
154	
264.1084(g)(3)	

	

	
fixed roof & its closure devices shall be visually inspected for defects; examples	
154	
264.1084(g)(3)(i)	

	

	
closed-vent system & control device shall be inspected & monitored in accordance with 264.1087	
154	
264.1084(g)(3)(ii)	

	

	
perform initial inspection of air emission control equipment on or before tank becomes subject to 264.1084; then at least once a year except under special conditions of 264.1084(l)	
154	
264.1084(g)(3)(iii)	

	

	
in event of defect, it shall be repaired in accordance with 264.1084(k)	
154	
264.1084(g)(3)(iv)	

	

	
owner/operator shall maintain inspection record in accordance with 264.1089(b)	
154	
264.1084(g)(3)(v)	

	

	
owner/operator who controls air pollutant emissions by using a pressure tank shall meet the following:	
154	
264.1084(h)	

	

	
tank shall not be designed to vent to atmosphere as result of compression in vapor headspace during filling	
154	
264.1084(h)(1)	

	

	
tank openings shall be equipped with closure devices that operate with no detectable organic emissions as in 264.1083(d)	
154	
264.1084(h)(2)	

	

	
whenever hazardous waste is in the tank, it shall be operated as a closed system that does not vent to the atmosphere except under either of the following conditions as specified in paragraph (h)(3)(i) or (h)(3)(ii) of this section 	
154,177	
264.1084(h)(3)	

	

	
when opening safety device is required to avoid unsafe condition	
154,177	
264.1084(h)(3)(i)	

	

	
when purging of inerts from tank is required and purge stream is routed to closed-vent system and control device designed & operated according to 264.1087	
177	
264.1084(h)(3)(ii)	

	

	
owner/operator who controls air pollutant emissions by using enclosure vented through a closed-vent system to enclosed combustion control device shall meet requirements in 264.1084(i)(1)-(4) 	
154	
264.1084(i)	

	

	
tank shall be inside enclosure; enclosure shall be designed & operated in accordance with 52.741, appendix B; allowance for openings; perform verification as specified in Section 5.0 	
154	
264.1084(i)(1)	

	

	
enclosure shall be vented through a closed-vent system to enclosed combustion control device designed & operated in accordance with certain standards specified in 264.1087	
154	
264.1084(i)(2)	

	

	
safety devices, defined in 265.1081, may be installed & operated on any enclosure, closed-vent system, or control device used to comply with 264.1084(i)(1)-(2)	
154	
264.1084(i)(3)	

	

	
owner/operator shall inspect & monitor the closed-vent system & control device as specified in 264.1087	
154	
264.1084(i)(4)	

	

	
owner/operator shall transfer hazardous waste to tank subject to 264.1084 in accordance with the following: 	
154	
264.1084(j)	

	

	
transfer of hazardous waste, except as in 264.1084(j)(2), to tank from another tank subject to 264.1084 or from surface impoundment subject to 264.1085 shall use continuous hard-piping or another closed system; individual drain system	
154	
264.1084(j)(1)	

	

	
264.1084(j)(1) requirements do not apply if transferring hazardous waste to tank under following:	
154	
264.1084(j)(2)	

	

	
hazardous waste meets average VO concentration conditions in 264.1082(c)(1) at point of waste origination	
154	
264.1084(j)(2)(i)	

	

	
hazardous waste treated by an organic destruction or removal process to meet 264.1082(c)(2) requirements	
154	
264.1084(j)(2)(ii)	

	

	
hazardous waste meets requirements of 264.1082(c)(4)	
163	
264.1084(j)(2)(iii)	

	

	
owner/operator shall repair each defect detected during inspections performed under 264.1084(c)(4), (e)(3), (f)(3), or (g)(3) as follows:	
154	
264.1084(k)	

	

	
owner/operator shall make first efforts at repair no later than 5 days after detection & repair shall be completed no later than 45 days after detection except as in 264.1084(k)(2)	
154	
264.1084(k)(1)	

	

	
repairs may be delayed beyond 45 days if repair requires emptying or temporary removal from service & no alternative tanks are available; owner/ operator shall repair the defect as soon as tank stops operation; repair shall be completed before resuming operation 	
154	
264.1084(k)(2)	

	

	
after initial inspection & monitoring of cover pursuant to Subpart CC, inspection & monitoring may be at intervals longer than 1 year under the following conditions:	
154	
264.1084(l)	

	

	
if inspecting or monitoring exposes a worker to dangerous, hazardous, or other unsafe conditions, the owner/operator may designate cover as unsafe & comply with the following:  	
154	
264.1084(l)(1)	

	

	
prepare written explanation	
154	
264.1084(l)(1)(i)	

	

	
develop & implement written plan & schedule to inspect & monitor	
154	
264.1084(1)(1)(ii)	

	

	
if tank is buried partially or entirely, owner/operator must inspect & monitor only portions of cover that are located on or above ground	
154	
264.1084(l)(2)	

	

	
STANDARDS:  SURFACE IMPOUNDMENTS	

264.1085 provisions apply to control of air pollutant emissions from surface impoundments for which 264.1082(b) references this section	
154	
264.1085(a)	

	

	
owner/operator shall control air pollutant emissions from surface impoundment by installing & operating either: 	
154	
264.1085(b)	

	

	
floating membrane cover in accordance with 264.1085(c); or	
154	
264.1085(b)(1)	

	

	
cover vented through a closed-vent system to a control device in accordance with 264.1085(d)	
154,163	
264.1085(b)(2)	

	

	
owner/operator who controls emissions from a surface impoundment using a floating membrane cover shall meet requirements in 264.1085(c)(1)-(3) 	
154	
264.1085(c)	

	

	
surface impoundment shall be equipped with floating membrane cover designed to meet the following:	
154	
264.1085(c)(1)	

	

	
designed to float on the liquid surface during normal operations & form a continuous barrier	
154	
264.1085(c)(1)(i)	

	

	
fabricated from synthetic membrane material with certain specifications	
154	
264.1085(c)(1)(ii)	

	

		
154	
264.1085(c)(1)(ii)(A)	

	

		
154	
264.1085(c)(1)(ii)(B)	

	

	
installed without visible cracks, holes, gaps, or open spaces between cover edges or foundation mountings	
154	
264.1085(c)(1)(iii)	

	

	
except as in 264.1085(c)(1)(v), openings in floating membrane cover shall be equipped with a closure device that does not allow for open spaces in the closure device or between the opening & device	
154	
264.1085(c)(1)(iv)	

	

	
floating membrane cover may be equipped with emergency cover drains; drains shall be equipped with slotted membrane fabric cover or flexible fabric sleeve seal	
154	
264.1085(c)(1)(v)	

	

	
closure devices shall consist of materials to minimize exposure of hazardous waste to atmosphere & maintain integrity throughout service life; factors to consider when selecting materials	
154	
264.1085(c)(1)(vi)	

	

	
whenever hazardous waste is in surface impoundment, floating membrane cover shall float on liquid & each closure device in closed position except:	
154	
264.1085(c)(2)	

	

	
opening of closure devices or removal of the cover allowed to provide access to surface impoundment or to remove accumulated sludge	
154	
264.1085(c)(2)(i)	

	

		
154	
264.1085(c)(2)(i)(A)	

	

		
154	
264.1085(c)(2)(i)(B)	

	

	
opening of safety device allowed to avoid an unsafe condition	
154	
264.1085(c)(2)(ii)	

	

	
owner/operator shall inspect floating membrane cover as follows:	
154	
264.1085(c)(3)	

	

	
floating membrane cover & closure devices shall be visually inspected for defects; examples	
154	
264.1085(c)(3)(i)	

	

	
perform initial inspection of floating membrane cover & closure devices on or before surface impoundment is subject to 264.1085; then at least once a year except under 264.1085(g)	
154	
264.1085(c)(3)(ii)	

	

	
in event of defect, it shall be repaired in accordance with 264.1085(f)	
154	
264.1085(c)(3)(iii)	

	

	
owner/operator shall maintain inspection record in accordance with 264.1089(c)	
154	
264.1085(c)(3)(iv)	

	

	
owner/operator who controls air pollutant emissions from a surface impoundment using a cover vented to control device shall meet 264.1085(d)(1)-(3) requirements	
154	
264.1085(d)	

	

	
surface impoundment covered & vented directly to control device in accordance with the following: 	
154	
264.1085(d)(1)	

	

	
cover & closure devices shall form a continuous barrier over liquid in the surface impoundment 	
154	
264.1085(d)(1)(i)	

	

	
openings in the cover not vented to control device equipped with closure device; if pressure in vapor headspace < atmospheric pressure; if pressure in vapor headspace > atmospheric pressure 	
154	
264.1085(d)(1)(ii)	

	

	
cover & closure devices shall be made of suitable materials to minimize exposure to atmosphere & maintain integrity throughout service life; factors to consider when selecting materials 	
154,163	
264.1085(d)(1)(iii)	

	

	
closed-vent system & control device shall be designed & operated in accordance with 264.1087	
154	
264.1085(d)(1)(iv)	

	

	
when hazardous waste is in surface impoundment, cover shall be installed with closure device in closed position except:	
154	
264.1085(d)(2)	

	

	
venting to control device not required, & opening of closure device or removal of cover is allowed in specified circumstances	
154	
264.1085(d)(2)(i)	

	

		
154	
264.1085(d)(2)(i)(A)	

	

		
154,163	
264.1085(d)(2)(i)(B)	

	

	
opening of safety device, as in 265.1081, allowed to avoid an unsafe condition	
154	
264.1085(d)(2)(ii)	

	

	
owner/operator shall inspect & monitor air emission control equipment as follows:	
154	
264.1085(d)(3)	

	

	
surface impoundment cover & closure devices shall be visually inspected for defects; examples	
154	
264.1085(d)(3)(i)	

	

	
closed-vent system & control device shall be inspected & monitored in accordance with 264.1087	
154	
264.1085(d)(3)(ii)	

	

	
initial inspection of air emission control equipment on or before the surface impoundment is subject to 264.1085; then at least once a year except under  264.1085(g)	
154	
264.1085(d)(3)(iii)	

	

	
in event of defect, it shall be repaired in accordance with 264.1085(f)	
154	
264.1085(d)(3)(iv)	

	

	
owner/operator shall maintain inspection record in accordance with 264.1089(c)	
154	
264.1085(d)(3)(v)	

	

	
owner/operator shall transfer hazardous waste to surface impoundment subject to 264.1085 in accordance with:	
154	
264.1085(e)	

	

	
transfer of hazardous waste, except as in 264.1085(e)(2), to surface impoundment from another surface impoundment subject to 264.1085 or from a tank subject to 264.1084 shall use continuous hard-piping or another closed system;  individual drain system	
154	
264.1085(e)(1)	

	

	
264.1085(e)(1) requirements do not apply when transferring a hazardous waste to surface impoundment under the following:	
154	
264.1085(e)(2)	

	

	
hazardous waste meets average VO concentration conditions in 264.1082(c)(1) at point of origination	
154	
264.1085(e)(2)(i)	

	

	
hazardous waste treated by organic destruction or removal process to meet 264.1082(c)(2) requirements	
154	
264.1085(e)(2)(ii)	

	

	
hazardous waste meets requirements of 264.1082(c)(4)	
163	
264.1085(e)(2)(iii)	

	

	
owner/operator repair each defect detected during inspections performed in accordance with 264.1085(c)(3) or (d)(3) as follows:	
154	
264.1085(f)	

	

	
owner/operator shall make first efforts at repair no later than 5 days after detection & repair shall be completed no later than 45 days after detection except as in 264.1085(f)(2) 	
154	
264.1085(f)(1)	

	

	
repairs may be delayed beyond 45 days if require emptying or temporary removal from service & no alternative capacity is available; if so,  owner/operator shall repair defect as soon as process generating hazardous waste in surface impoundment stops operation; repair completed before resuming operation	
154	
264.1085(f)(2)	

	

	
following initial inspection & monitoring of cover as required by Subpart CC, inspection & monitoring at intervals longer than 1 year under following conditions: 	
154	
264.1085(g)	

	

	
written explanation stating why cover is unsafe, if required 	
154	
264.1085(g)(1)	

	

	
develop & implement written plan & schedule to inspect & monitor cover 	
154	
264.1085(g)(2)	

	

	
STANDARDS:  CONTAINERS	

264.1086 applies to control of air pollutant emissions from containers for which 264.1082(b) references this section	
154	
264.1086(a)	

	

	
general requirements 	
154	
264.1086(b)	

	

	
owner/operator shall control air pollutant emissions from each container subject to 264.1086 in accordance with the following:	
154	
264.1086(b)(1)	

	

	
for containers having design capacities greater than 0.1 m3 & less than or equal to 0.46 m3, owner/operator shall control air pollutant emissions in accordance with Container Level 1 standards in 264.1086(c)	
154	
264.1086(b)(1)(i)	

	

	
for containers having design capacities greater than 0.46 m3 not in light material service, owner/ operator shall control air pollutant emissions in accordance with Container Level 1 standards in 264.1086(c)	
154	
264.1086(b)(1)(ii)	

	

	
for containers having design capacities greater than 0.46 m3 in light material service, owner/operator shall control air pollutant emissions in accordance with Container Level 2 standards in 264.1086(d)	
154	
264.1086(b)(1)(iii)	

	

	
when containers with design capacities greater than 0.1 m3 are used for treatment of hazardous waste by waste stabilization process, owner/ operator shall control air pollutant emissions in accordance with Container Level 3 standards in 264.1086(e) 	
154	
264.1086(b)(2)	

	

	
Container Level 1 standards	
154	
264.1086(c)	

	

5	
using Container Level 1 controls is one of the following: 	
154	
264.1086(c)(1)	

	

	
meets applicable U.S. DOT regulations on packaging for transportation as in 264.1086(f)	
154	
264.1086(c)(1)(i)	

	

	
equipped with cover & closure devices that form a continuous barrier over openings such that there are no visible open spaces into the interior	
154	
264.1086(c)(1)(ii)	

	

	
open-top container in which organic-vapor suppressing barrier is used such that no hazardous waste is exposed; example	
154	
264.1086(c)(1)(iii)	

	

	
container used to meet requirements of 264.1086(c)(1)(ii) or (c)(1)(iii) shall be equipped with covers & closure devices composed of materials to minimize exposure of hazardous waste to atmosphere & to maintain equipment integrity; factors to consider in selecting materials	
154,163	
264.1086(c)(2)	

	

	
when using Container Level 1 controls, owner/ operator shall install covers & closure devices, & secure & maintain them in closed position except: 	
154	
264.1086(c)(3)	

	

	
opening of closure device or cover is allowed to add hazardous waste or other material as specified	
154	
264.1086(c)(3)(i)	

	

		
154	
264.1086(c)(3)(i)(A)	

	

		
154	
264.1086(c)(3)(i)(B)	

	

	
opening of closure device or cover is allowed to remove hazardous waste as specified	
154	
264.1086(c)(3)(ii)	

	

		
154	
264.1086(c)(3)(ii)(A)	

	

		
154	
264.1086(c)(3)(ii)(B)	

	

	
opening of closure device or cover is allowed when access needed to perform routine activities other than transfer hazardous waste; examples; after activity, owner/operator shall promptly secure closure device or reinstall cover	
154	
264.1086(c)(3)(iii)	

	

	
opening of pressure relief devices allowed during normal operations to maintain internal pressure in accordance with container design; device shall operate with no detectable organic emissions when closed; settings at which device opens shall allow device to remain in closed position when internal pressure is within operating range; examples	
154	
264.1086(c)(3)(iv)	

	

	
opening of safety device, as defined in 265.1081, is allowed any time conditions require it to avoid an unsafe condition	
154	
264.1086(c)(3)(v)	

	

	
inspect containers & their covers & closure devices as follows:	
154	
264.1086(c)(4)	

	

	
if hazardous waste is present in container when owner/operator first accepts possession & container is not emptied within 24 hours, it shall be visually inspected on or before date that container is accepted at facility; date of acceptance; if a defect is detected, owner/operator repair in accordance with 264.1086(c)(4)(iii)	
154,163	
264.1086(c)(4)(i)	

	

	
if container remains at the facility for 1 year or more, owner/operator shall inspect it & cover & closure devices initially & then, at least every 12 months; if defect is detected, owner/operator repair in accordance with 264.1086(c)(4)(iii)	
154	
264.1086(c)(4)(ii)	

	

	
when a defect is detected, owner/ operator shall make repair no later than 24 hours after detection & complete it no later than 5 days after detection; if repair cannot be completed within 5 days, hazardous waste shall be removed & container not used until repaired	
154	
264.1086(c)(4)(iii)	

	

	
owner/operator shall maintain copy of procedure to determine that containers with 0.46 m3 or greater capacity, are not managing hazardous waste in light material service 	
154	
264.1086(c)(5)	

	

	
Container Level 2 standards	
154	
264.1086(d)	

	

5	
container using Container Level 2 controls is one of the following:	
154	
264.1086(d)(1)	

	

	
meets the applicable U.S. DOT regulations on packaging for transportation as in 264.1086(f)  	
154	
264.1086(d)(1)(i)	

	

	
container that operates with no detectable organic emissions as determined in accordance 264.1086(g)	
154	
264.1086(d)(1)(ii)	

	

	
container that has been demonstrated to be vapor-tight by using part 60, appendix A, Method 27 in accordance with 264.1086(h)	
154	
264.1086(d)(1)(iii)	

	

	
transfer of hazardous waste shall minimize exposure to the atmosphere, to extent practical; examples that meet 264.1086(d)(2) requirements	
154,163	
264.1086(d)(2)	

	

	
owner/operator shall install all covers & closure devices, & secure & maintain in closed position except:	
154	
264.1086(d)(3)	

	

	
opening of closure device or cover is allowed to add hazardous waste or other material as follows	
154	
264.1086(d)(3)(i)	

	

		
154	
264.1086(d)(3)(i)(A)	

	

		
154	
264.1086(d)(3)(i)(B)	

	

	
opening of a closure device or cover is allowed to remove hazardous waste as follows	
154	
264.1086(d)(3)(ii)	

	

		
154	
264.1086(d)(3)(ii)(A)	

	

		
154	
264.1086(d)(3)(ii)(B)	

	

	
opening of closure device or cover is allowed when access is needed to perform routine activities other than transfer; examples; after activity, promptly secure closure device or reinstall cover	
154	
264.1086(d)(3)(iii)	

	

	
opening of pressure relief devices which vent to atmosphere is allowed during normal operations to maintain internal pressure in accordance with container design; device shall operate with no detectable organic emissions when in closed position; settings at which device opens shall allow device to remain in closed position when internal pressure is within operating range; examples	
154	
264.1086(d)(3)(iv)	

	

	
opening of safety device, as defined in 265.1081, is allowed any time conditions require it to avoid an unsafe condition	
154	
264.1086(d)(3)(v)	

	

	
owner/operator shall inspect containers & their covers & closure devices as follows:	
154	
264.1086(d)(4)	

	

	
if hazardous waste is present in container when owner/operator first accepts possession & container is not emptied within 24 hours, it shall be visually inspected on or before date that container accepted at facility; date of acceptance; if defect is detected, owner/operator shall repair in accordance with 264.1086(d)(4)(iii)	
154,163	
264.1086(d)(4)(i)	

	

	
if container remains at the facility for 1 year or more, owner/operator shall inspect it & cover & closure devices initially & then at least every 12 months to check for open spaces into its interior; if defect is detected, owner/ operator shall repair in accordance with 264.1086(d)(4)(iii)	
154	
264.1086(d)(4)(ii)	

	

	
when defect is detected, owner/ operator shall make efforts at repair no later than 24 hours after detections & complete it as soon as possible but no later than 5 days after detection; if repair cannot be completed within 5 days, hazardous waste shall be removed & container shall not be used until repaired	
154	
264.1086(d)(4)(iii)	

	

	
Container Level 3 standards	
154	
264.1086(e)	

	

5	
container using Container Level 3 controls is one of the following:	
154	
264.1086(e)(1)	

	

	
container that is vented through a closed-vent system to control device in accordance with 264.1086(e)(2)(ii)	
154	
264.1086(e)(1)(i)	

	

	
container that is vented inside an enclosure which is exhausted through closed-vent system to control device in accordance with 264.1086(e)(2)(i)-(ii)	
154	
264.1086(e)(1)(ii)	

	

	
owner/operator shall meet the following, as applicable	
154	
264.1086(e)(2)	

	

	
container enclosure shall be designed & operated in accordance with 52.741, appendix B; permanent or temporary openings; verification procedure as in Section 5.0 	
154	
264.1086(e)(2)(i)	

	

	
closed-vent system & control device shall be designed & operated in accordance with 264.1087	
154	
264.1086(e)(2)(ii)	

	

	
safety devices, in 265.1081, may be installed & operated on any container, enclosure, closed-vent system, or control device used to comply with 264.1086(e)(1)	
154	
264.1086(e)(3)	

	

	
owner/operator shall inspect & monitor the closed-vent system & control devices as specified in 264.1087	
154	
264.1086(e)(4)	

	

	
owners/operators shall prepare & maintain records specified in 264.1089(d)	
154	
264.1086(e)(5)	

	

	
transfer of hazardous waste in or out of container using Container Level 3 controls shall be conducted to minimize exposure to atmosphere; examples of acceptable container loading procedures	
177	
264.1086(e)(6)	

	

	
for purpose of 264.1086(c)(1)(i) or (d)(1)(i) compliance, containers shall meet applicable U.S. DOT regulations on packaging for transportation as follows:  	
154	
264.1086(f)	

	

	
meets applicable requirements in 49 CFR part 178 or 49 CFR part 179	
154	
264.1086(f)(1)	

	

	
hazardous waste managed in container in accordance with 49 CFR part 107, subpart B; 49 CFR part 172; 49 CFR part 173; & 49 CFR part 180	
154	
264.1086(f)(2)	

	

	
no exceptions to the 49 CFR part 178 or 179 regulations are allowed except as in 264.1086(f)(4)	
154	
264.1086(f)(3)	

	

	
for lab pack managed in accordance with 49 CFR part 178, owner/operator may comply with the exceptions for combination packaging in 49 CFR 173.12(b)	
154	
264.1086(f)(4)	

	

	
to determine compliance with 264.1086(d)(1)(ii), use procedure specified in 264.1083(d)	
154,163	
264.1086(g)	

	

	
each potential leak interface on container, cover, & closure devices shall be checked; examples	
154	
264.1086(g)(1)	

	

	
test performed when container is filled with material expected to be managed in this container; during test, container cover & closure devices shall be closed 	
154	
264.1086(g)(2)	

	

	
procedure for determining a container to be vapor-tight using Method 27 of part 60, appendix A to comply with 264.1086(d)(1)(iii)	
154	
264.1086(h)	

	

	
test performed in accordance with Method 27 of part 60, appendix A 	
154	
264.1086(h)(1)	

	

	
pressure measurement device shall be used with a precision of "2.5mm water & capable of measuring above that used for vapor pressure tightness	
154	
264.1086(h)(2)	

	

	
if test results indicate container sustains a pressure change less than or equal to 750 Pascals, then it's vapor-tight	
154	
264.1086(h)(3)	

	

	
STANDARDS:  CLOSED-VENT SYSTEMS AND CONTROL DEVICES	

264.1087 applies to closed-vent system & control device installed & operated to control air emissions	
154	
264.1087(a)	

	

	
closed-vent system shall meet the following requirements:	
154	
264.1087(b)	

	

	
route gases, vapors, & fumes to a control device that meets the requirements specified in 264.1087(c)	
154	
264.1087(b)(1)	

	

	
designed & operated in accordance with 264.1033(k)	
154	
264.1087(b)(2)	

	

	
if system includes bypass devices, each device shall be equipped with either flow indicator or seal or locking device; other fittings used for safety purposes are not bypass devices 	
154	
264.1087(b)(3)	

	

	
if flow indicator is used to comply with 264.1087(b)(3), it shall be installed at inlet to bypass line; flow indicator is a device which indicates gas or vapor flow	
154	
264.1087(b)(3)(i)	

	

	
if a seal or locking device is used to comply with 264.1087(b)(3), it shall be placed such that bypass device cannot be opened without breaking the seal or removing the lock; examples; inspect seal or closure mechanism at least once a month 	
154	
264.1087(b)(3)(ii)	

	

	
closed-vent system shall be inspected & monitored by owner/ operator in accordance with 264.1033(l)	
154	
264.1087(b)(4)	

	

	
control device shall meet the following requirements:	
154	
264.1087(c)	

	

	
control device shall be one of the following devices:	
154	
264.1087(c)(1)	

	

	
control device designed & operated to reduce total organic content of inlet vapor stream by at least 95%	
154	
264.1087(c)(1)(i)	

	

	
enclosed combustion device designed & operated in accordance with 264.1033(c)	
154	
264.1087(c)(1)(ii)	

	

	
flare designed & operated in accordance with 264.1033(d)	
154	
264.1087(c)(1)(iii)	

	

	
owner/operator who uses closed-vent system & control device to comply with 264.1087 shall comply with 264.1087(c)(2)(i)-(c)(2)(vi)	
154	
264.1087(c)(2)	

	

	
periods of planned routine maintenance of control device during which 264.1087 (c)(1)(i)-(iii) are not met, shall not exceed 240 hours/year	
154	
264.1087(c)(2)(i)	

	

	
requirements in 264.1087(c)(1)(i)-(iii) do not apply during planned routine maintenance	
154	
264.1087(c)(2)(ii)	

	

	
requirements in 264.1087(c)(1)(i)-(iii) do not apply during control device system malfunction	
154	
264.1087(c)(2)(iii)	

	

	
owner/operator shall demonstrate compliance with 264.1087(c)(2)(i) by recording information in 264.1089(e)(1)(v)	
154	
264.1087(c)(2)(iv)	

	

	
owner/operator shall correct control device system malfunctions as soon as practicable to minimize excess air pollutant emissions	
154	
264.1087(c)(2)(v)	

	

	
owner/operator shall operate closed-vent system such that gases, vapors, or fumes are not vented to control device during maintenance or malfunction except when necessary	
154	
264.1087(c)(2)(vi)	

	

	
owner/operator using a carbon adsorption system shall operate & maintain control device in accordance with the following requirements:	
154	
264.1087(c)(3)	

	

	
following initial startup, all activated carbon shall be replaced with fresh carbon regularly in accordance with 264.1033(g) or (h)	
154	
264.1087(c)(3)(i)	

	

	
all carbon that is hazardous waste and that is removed from control device shall be managed in accordance with 264.1033(n) regardless of average volatile organic concentration of  carbon	
154,163	
264.1087(c)(3)(ii)	

	

	
owner/operator using a control device other than a thermal vapor incinerator, flare, boiler, process heater, condenser, or carbon adsorption system shall operate & maintain in accordance with 264.1033(j)	
154	
264.1087(c)(4)	

	

	
demonstrate that control device achieves performance  requirements of 264.1087(c)(1) as follows:	
154	
264.1087(c)(5)	

	

	
demonstrate, using a performance test as in 264.1087(c)(5)(iii) or design analysis as in 264.1087(c)(5)(iv) for each control device except for the following:	
154	
264.1087(c)(5)(i)	

	

	
a flare	
154	
264.1087(c)(5)(i)(A)	

	

	
boiler or process heater with design input capacity of 44 megawatts or greater	
154	
264.1087(c)(5)(i)(B)	

	

	
boiler or process heater into which the vent stream is introduced with primary fuel	
154	
264.1087(c)(5)(i)(C)	

	

	
boiler or industrial furnace burning hazardous waste for which owner/operator has been issued a final permit and designs and operates unit in accordance with 266, Subpart H	
154	
264.1087(c)(5)(i)(D)	

	

	
boiler or industrial furnace burning hazardous waste for which owner/operator has designed & operates in accordance with requirements of 266, Subpart H	
154	
264.1087(c)(5)(i)(E)	

	

	
owner/operator shall demonstrate the performance of each flare in accordance with 264.1033(e)	
154	
264.1087(c)(5)(ii)	

	

	
for a performance test, owner/operator shall use test methods & procedures in 264.1034(c)(1)-(4)	
154	
264.1087(c)(5)(iii)	

	

	
design analysis shall meet requirements specified in 264.1035(b)(4)(iii)	
154	
264.1087(c)(5)(iv)	

	

	
owner/operator shall demonstrate that carbon adsorption system achieves the 264.1087(c)(1) performance requirements	
154	
264.1087(c)(5)(v)	

	

	
if owner/operator & Regional Administrator do not agree on a demonstration of control device performance using a design analysis, then disagreement shall be resolved using a performance test in accordance with 264.1087(c)(5)(iii); Regional Administrator may choose authorized representative to observe	
154	
264.1087(c)(6)	

	

	
closed-vent system and control device shall be inspected & monitored by owner/operator in accordance with 264.1033(f)(2) & 264.1033(l); readings from each monitoring device inspected at least once each day; any necessary corrective measures immediately implemented	
154,163	
264.1087(c)(7)	

	

	
INSPECTION AND MONITORING REQUIREMENTS	

owner/operator shall inspect & monitor air emission control equipment in accordance with 264.1084-264.1087	
154	
264.1088(a)	

	

	
owner/operator shall develop & implement written plan & schedule to perform inspections & monitoring required by 264.1088(a); shall incorporate plan into facility inspection plan under 264.15	
154	
264.1088(b)	

	

	
RECORDKEEPING REQUIREMENTS	

owners or operator subject to 264, Subpart CC shall record and maintain information specified in 264.1089(b)-(j); with exception, records shall be maintained for at least 3 years; documentation maintained until air emission control equipment is replaced; information required by 264.1089(i)&(j) shall be maintained as long as waste management unit is not using air emission controls in 264.1084-264.1087  	
154,163	
264.1089(a)	

	

	
owner/operator of tank using air emission controls in accordance with 264.1084 shall prepare & maintain records that include: 	
154	
264.1089(b)	

	

	
for tank using air emission controls in accordance with 264.1084, owner/ operator shall record: 	
154	
264.1089(b)(1)	

	

	
tank identification number	
154	
264.1089(b)(1)(i)	

	

	
record for each inspection required by 264.1084 that includes inspection date & other information for defects detected 	
154	
264.1089(b)(1)(ii)	

	

		
154	
264.1089(b)(1)(ii)(A)	

	

		
154,163	
264.1089(b)(1)(ii)(B)	

	

	
owner/operator shall record following information, as applicable to the tank:	
154	
264.1089(b)(2)	

	

	
owner/operator using a fixed roof shall prepare & maintain records for each maximum organic vapor pressure determination in accordance with 264.1084(c); date & time of sample collection, analysis method, & results	
154	
264.1089(b)(2)(i)	

	

	
owner/operator using internal floating roof shall prepare & maintain documentation describing design	
154	
264.1089(b)(2)(ii)	

	

	
owners/operators using external floating roof shall prepare & maintain documentation & records for specified items	
154	
264.1089(b)(2)(iii)	

	

		
154	
264.1089(b)(2)(iii)(A)	

	

		
154	
264.1089(b)(2)(iii)(B)	

	

	
each owner/operator using an enclosure shall prepare & maintain specified records	
154	
264.1089(b)(2)(iv)	

	

		
154	
264.1089(b)(2)(iv)(A)	

	

		
154	
264.1089(b)(2)(iv)(B)	

	

	
owner/operator of a surface impoundment using air emission controls in accordance with 264.1085 shall prepare & maintain records that include: 	
154	
264.1089(c)	

	

	
surface impoundment identification number	
154	
264.1089(c)(1)	

	

	
documentation describing floating membrane cover that includes description of cover design, & certification that it meets specifications in 264.1085(c)	
154	
264.1089(c)(2)	

	

	
record for each inspection required by 264.1085 that includes:	
154	
264.1089(c)(3)	

	

	
date inspection was conducted	
154	
264.1089(c)(3)(i)	

	

	
for each defect detected during inspection: location, description, date & corrective action; if repair delayed, owner/ operator shall record reason & date of expected repair	
154	
264.1089(c)(3)(ii)	

	

	
for a surface impoundment equipped with cover & vented through a closed-vent system to a control device, owner/operator shall prepare & maintain records specified in 264.1089(e)	
154	
264.1089(c)(4)	

	

	
owner/operator of containers using Container Level 3 air emission controls in accordance with 264.1086 shall prepare & maintain records that include: 	
154	
264.1089(d)	

	

	
records for most recent calculations & measurements to verify enclosure meets criteria of a permanent total enclosure as in "Procedure T" 40 CFR 52.741, appendix B	
154	
264.1089(d)(1)	

	

	
records required for closed-vent system & control device in accordance with 264.1089(e)	
154	
264.1089(d)(2)	

	

	
owner/operator using closed-vent system & control device in accordance with 264.1087 shall prepare & maintain records that include: 	
154	
264.1089(e)	

	

	
documentation that includes:	
154	
264.1089(e)(1)	

	

	
certification signed & dated by owner/ operator stating the control device is designed to operate at performance level when operating at capacity 	
154	
264.1089(e)(1)(i)	

	

	
specified design documentation if  design analysis used; include a description of the control device design in accordance with 264.1035(b)(4)(iii) & certification by owner/operator that control equipment meets applicable specifications	
154	
264.1089(e)(1)(ii)	

	

	
performance test plan & all test results, if performance tests are used	
154	
264.1089(e)(1)(iii)	

	

	
information as required by 264.1035 (c)(1)-(2)	
154	
264.1089(e)(1)(iv)	

	

	
owner/operator shall record on semiannual basis, information specified in 264.1089(e)(1)(v)(A)-(B) for planned routine maintenance operations requiring control devices not to meet 264.1087(c)(1)(i)-(iii) requirements	
154	
264.1089(e)(1)(v)	

	

		
154	
264.1089(e)(1)(v)(A)	

	

		
154	
264.1089(e)(1)(v)(B)	

	

	
owner/operator shall record the information specified in 264.1089(e)(1)(vi)(A)-(C) for unexpected control device system malfunctions 	
154	
264.1089(e)(1)(vi)	

	

		
154	
264.1089(e)(1)(vi)(A)	

	

		
154	
264.1089(e)(1)(vi)(B)	

	

		
154	
264.1089(e)(1)(vi)(C)	

	

	
management records of carbon removed from a carbon adsorption system conducted in accordance with 264.1087(c)(3)(ii)	
154	
264.1089(e)(1)(vii)	

	

	
owner/operator of a tank, surface impoundment, or container exempted from standards in accordance with 264.1082(c) shall prepare & maintain following records:	
154	
264.1089(f)	

	

	
if exempted under 264.1082(c)(1) or 264.1082(c)(2)(i)-(vi), owner/operator shall record information used for each waste determination in operating log; if waste sample results used for the determination, date, time, & location shall be recorded in accordance with 264.1083	
154,163	
264.1089(f)(1)	

	

	
if exempted under 264.1082(c)(2)(vii) or (viii), owner/operator shall record ID number for the incinerator, boiler, or industrial furnace in which hazardous waste is treated	
154	
264.1089(f)(2)	

	

	
owner/operator designating a cover as "unsafe to inspect and monitor" shall record in the facility  log: ID numbers, explanations, & inspection plans & schedules	
154	
264.1089(g)	

	

	
owners or operators subject to 264, Subpart CC and to control device standards in 40 CFR Part 60, Subpart VV or 40 CFR 61, Subpart V may demonstrate compliance by documentation pursuant to those subparts to extent that it duplicates that required by 264.1089	
154	
264.1089(h)	

	

	
for tank or container not using air emission controls specified in 264.1084-264.1087 in accordance with 264.1080(d), owner/ operator shall record & maintain the following:	
154	
264.1089(i)	

	

	
list of individual organic peroxide compounds manufactured at the facility that meet 264.1080(d)(1) conditions	
154	
264.1089(i)(1)	

	

	
description of how hazardous waste containing organic peroxide compounds identified in 264.1089(i)(1) are managed in tanks & containers; the description shall include:	
154	
264.1089(i)(2)	

	

	
for tanks, sufficient information provided to describe: facility tank ID number, purpose and placement of the tank in the management train of this hazardous waste, and procedures used to ultimately dispose of hazardous waste	
154	
264.1089(i)(2)(i)	

	

	
for containers, sufficient information provided to describe: facility ID number for each container or group of containers; purpose and placement in the management train of this hazardous waste, and procedures used to ultimately dispose of hazardous waste	
154	
264.1089(i)(2)(ii)	

	

	
why managing the hazardous waste containing organic peroxide compounds identified in 264.1089(i)(1) would create an undue safety hazard if specified air emission controls are installed & operated; include the following information:	
154	
264.1089(i)(3)	

	

	
for tanks, sufficient information to explain how required air emission controls would affect design and facility operating procedures currently used, and why installation of safety devices under Part 264, Subpart CC will not address situations when evacuation is necessary	
154	
264.1089(i)(3)(i)	

	

	
for containers, sufficient information to explain how required air emission controls would affect design and handling procedures currently used, and why installation of safety devices under Part 264, Subpart CC will not address situations in which evacuation is necessary	
154	
264.1089(i)(3)(ii)	

	

	
for each hazardous waste management unit not using air emission controls under 264.1084 through 264.1087 in accordance with 264.1080(b)(7), owner and operator shall record and maintain specified information	
163	
264.1089(j)	

	

		
163	
264.1089(j)(1)						
		
163	
264.1089(j)(2)						

REPORTING REQUIREMENTS	

owner/operator managing hazardous waste in a tank, surface impoundment, or container exempted in accordance with 264.1082(c) shall report each occurrence when there is noncompliance with 264.1082(c)(1) or (2); written report submitted within 15 days; shall contain specified information	
154	
264.1090(a)	

	

	
owner/operator using tank air emission controls in accordance with 264.1084(c) shall report each occurrence when there is noncompliance with 264.1084(b); written report submitted within 15 days; shall contain specified information	
154	
264.1090(b)	

	

	
owner/operator using control device in accordance with 264.1087 shall submit a semiannual written report except as in 264.1090(d); shall describe each occurrence in the past 6 mos. when either:  control device is operated continuously for 24 hours or longer in noncompliance with operating values defined in '264.1035 (c)(4) or flare is operated with visible emissions for 5 minutes or longer in two-hour period, as in '264.1033(d);
report include EPA ID#, facility name & address, explanation, & actions taken; signed & dated	
154	
264.1090(c)	

	

	
report to Regional Administrator is not required for 6-month period during which all control devices are operated such that:	
154	
264.1090(d)	

	

	
during no period of 24 hours or longer did a control device operate continuously in noncompliance with 264.1035(c)(4); &	
154	
264.1090(d)(1)	

	

	
no flare was operated with visible emissions for 5 minutes or longer in a two-hour period, as in 264.1033(d)	
154	
264.1090(d)(2)	

	

	
reserved	
154	
264.1091	

	

	
SUBPART DD - CONTAINMENT BUILDINGS	

APPLICABILITY	

applies to owners/operators storing or treating hazardous waste in units designed and operated under 264.1101; effective February 18, 1993, but may notify Regional Administrator of earlier time; not subject to definition of land disposal in RCRA 3004(k) provided unit:	
109	
264.1100	

	

	
is a completely enclosed, self-supporting structure designed and constructed as specified	
109	
264.1100(a)	

	

	
has a primary barrier designed to withstand movement of personnel, wastes and handling equipment within unit	
109	
264.1100(b)	

	

	
if used to manage liquids:	
109	
264.1100(c)	

	

	
primary barrier designed and constructed to prevent migration of hazardous constituents into barrier	
109	
264.1100(c)(1)	

	

	
liquid collection system to minimize accumulation of liquid on primary barrier	
109	
264.1100(c)(2)	

	

	
secondary containment system to prevent hazardous constituent migration into barrier; leak detection and liquid collection as specified; variance under 264.1101(b)(4)	
109	
264.1100(c)(3)	

	

	
controls to prevent fugitive dust emissions to meet 264.1101(c)(1)(iv) standards	
109	
264.1100(d)	

	

	
designed and operated to ensure containment and prevent tracking of materials from unit by personnel or equipment	
109	
264.1100(e)	

	

	
DESIGN AND OPERATING STANDARDS 	

all containment buildings must comply with following design standards:	
109	
264.1101(a)	

	

	
completely enclosed as specified	
109	
264.1101(a)(1)	

	

	
design and construction of floor, containment walls and secondary containment system; unit of sufficient structural strength to prevent collapse or failure; chemically compatible surfaces; standards for judging structural integrity requirements; when exception for light-weight doors and windows will apply:	
109	
264.1101(a)(2)	

	

	
provide effective barrier against fugitive dust emissions under 264.1101(c)(1)(iv)	
109	
264.1101(a)(2)(i)	

	

	
unit designed and operated so that wastes do not contact openings	
109	
264.1101(a)(2)(ii)	

	

	
no placement of incompatible wastes or treatment reagents that could cause unit or secondary containment system to leak, corrode or otherwise fail	
109	
264.1101(a)(3)	

	

	
must have primary barrier designed to withstand movement of personnel, waste and handling equipment in unit during unit operating life, as appropriate for waste characteristics	
109	
264.1101(a)(4)	

	

	
requirements for hazardous waste containing free liquids or treated with free liquids:	
109	
264.1101(b)	

	

	
primary barrier to prevent migration of hazardous constituents into the barrier	
109	
264.1101(b)(1)	

	

	
liquid collection and removal system to minimize accumulation of liquid on primary barrier:	
109	
264.1101(b)(2)	

	

	
primary barrier sloped to drain liquids to collection system	
109	
264.1101(b)(2)(i)	

	

	
liquids and waste collected and removed to minimize hydraulic head on containment system at earliest practicable time	
109	
264.1101(b)(2)(ii)	

	

	
secondary containment system to prevent hazardous constituent migration into barrier; leak detection and liquid collection as specified	
109	
264.1101(b)(3)	

	

	
what must be installed at a minimum to satisfy leak detection component of secondary containment system	
109	
264.1101(b)(3)(i)	

	

	
constructed with 1% or greater bottom slope	
109	
264.1101(b)(3)(i)  (A)	

	

	
granular, synthetic, or geonet drainage materials as specified	
109	
264.1101(b)(3)(i)  (B)	

	

	
if treatment conducted in building, treatment area designed to prevent releases to other portions of building	
109	
264.1101(b)(3)(ii)	

	

	
secondary containment construction materials specifications; requirements for use of containment building as tank secondary containment system	
109	
264.1101(b)(3)(iii)	

	

	
for existing units other than 90-day generator units, Regional Administrator delay of secondary containment requirement if demonstrated that unit substantially meets Subpart DD standards; for demonstration, owner/operator must:	
109	
264.1101(b)(4)	

	

	
provide written notice by February 18, 1993; what notice must contain	
109	
264.1101(b)(4)(i)	

	

	
respond to Regional Administrator comments within 30 days	
109	
264.1101(b)(4)(ii)	

	

	
if approved, fulfill terms of revised plans	
109	
264.1101(b)(4)(iii)	

	

	
owners and operators of all containment buildings must:	
109	
264.1101(c)	

	

	
use controls and practices to ensure containment of hazardous waste within unit; at a minimum:	
109	
264.1101(c)(1)	

	

	
maintain primary barrier as specified	
109	
264.1101(c)(1)(i)	

	

	
maintain level of stored/treated hazardous waste as specified	
109	
264.1101(c)(1)(ii)	

	

	
take measures to prevent tracking of hazardous waste out of unit; equipment decontamination area; rinsate collection and management	
109	
264.1101(c)(1)(iii)	

	

	
take measures to control fugitive dust emissions; maintain particulate collection devices as specified; when "no visible emissions" must be maintained	
109	
264.1101(c)(1)(iv)	

	

	
certification by qualified registered professional engineer; for units in operation prior to February 18, 1993, certification placed in operating record or on-site files no later than 60 days after date of initial operation; after February 18, 1993, PE certification required prior to operation of unit	
109	
264.1101(c)(2)	

	

	
prompt repairs of unit throughout active life as specified, according to the following procedures:	
109	
264.1101(c)(3)	

	

	
detection of condition that has led to a release; leakage from primary barrier; owner or operator must:	
109	
264.1101(c)(3)(i)	

	

	
enter record of discovery in facility operating record	
109	
264.1101(c)(3)(i)  (A)	

	

	
immediately remove portion of containment building affected by the condition from service	
109	
264.1101(c)(3)(i)  (B)	

	

	
determine steps to be taken for repair, remove leakage from secondary collection system and establish schedule for cleanup and repairs	
109	
264.1101(c)(3)(i)  (C)	

	

	
within 7 days, notify Regional Administrator of condition; within 14 working days, provide written notice to Regional Administrator; what written notice must include	
109	
264.1101(c)(3)(i)  (D)	

	

	
Regional Administrator must review notice, determine extent to which unit must be removed from service during repairs, and notify owner/operator of determination and rationale in writing	
109	
264.1101(c)(3)(ii)	

	

	
written notification to Regional Administrator on completion of repair and cleanup; verification by a qualified, registered professional engineer that repairs and cleanup are in compliance with 264.1101(c)(3)(i)(D) plan	
109	
264.1101(c)(3)(iii)	

	

	
what must be inspected and recorded in facility's operating records, at least once every seven days	
109	
264.1101(c)(4)	

	

	
for containment buildings that contain areas both with and without secondary containment, the owner/operator must:	
109	
264.1101(d)	

	

	
design and operate each area in accordance with 264.1101(a)-(c) requirements	
109	
264.1101(d)(1)	

	

	
take measures to prevent release of liquids or wet materials into areas without secondary containment	
109	
264.1101(d)(2)	

	

	
maintain in facility's operating log a written description of operating procedures used to maintain integrity of areas without secondary containment	
109	
264.1101(d)(3)	

	

	
Regional Administrator waiver of secondary containment requirements; what owner/operator must demonstrate	
109	
264.1101(e)	

	

	
CLOSURE AND POST-CLOSURE CARE	

what must be done at closure; closure plan, closure activities, cost estimates, and financial responsibility must meet all 264 Subpart G & H requirements	
109	
264.1102(a)	

	

	
if 264.1102(a) requirements met and not all contaminated subsoils can be removed or decontaminated, close facility and perform post-closure care as for landfill under 264.310; owner/operator must meet 264 Subpart G & H requirements for landfills	
109	
264.1102(b)	

	

	
reserved	
109	
264.1103-264.1110	

	

	
	SUBPART EE - HAZARDOUS WASTE MUNITIONS AND EXPLOSIVES STORAGE	

APPLICABILITY	

subpart applies to owners and operators who store munitions and explosive hazardous wastes	
156	
264.1200	

	

	
DESIGN AND OPERATING STANDARDS	

storage units must meet following requirements	
156	
264.1201(a)	

	

	
minimize potential for detonation or release	
156	
264.1201(a)(1)	

	

	
provide primary barrier to contain waste	
156	
264.1201(a)(2)	

	

	
if stored outdoors must not be in standing precipitation	
156	
264.1201(a)(3)	

	

	
for liquids, provide secondary containment or vapor detection system	
156	
264.1201(a)(4)	

	

	
provide monitoring and inspection procedures meeting specified requirements	
156	
264.1201(a)(5)	

	

	
hazardous waste military munitions and explosives may be stored in the following	
156	
264.1201(b)	

	

	
earth-covered magazines; requirements for earth-covered magazines	
156	
264.1201(b)(1)	

	

		
156	
264.1201(b)(1)(i)	

	

		
156	
264.1201(b)(1)(ii)	

	

		
156	
264.1201(b)(1)(ii)(A)-(C)	

	

		
156	
264.1201(b)(1)(iii)	

	

	
above-ground magazines must be designed to minimize propagation of explosion	
156	
264.1201(b)(2)	

	

	
outdoor or open storage areas must be designed to minimize propagation of explosion	
156	
264.1201(b)(3)	

	

	
hazardous waste military munitions and explosives must be stored in accordance with Standard Operating Procedure; if procedure serves same purpose as certain Part 264 requirements, they may be used	
156	
264.1201(c)	

	

	
hazardous waste military munitions and explosives must be packaged to ensure safety	
156	
264.1201(d)	

	

	
hazardous waste military munitions and explosives must be inventoried annually	
156	
264.1201(e)	

	

	
hazardous waste military munitions and explosives must be inspected and monitored to ensure safety and no migration	
156	
264.1201(f)	

	

	
CLOSURE AND POST-CLOSURE CARE	

at closure of magazine or unit that stored hazardous waste under Subpart EE, owner/operator must remove or decontaminate residues, components, subsoils, structures and equipment; closure must meet 264 subparts G and H requirements, but may defer as long as munitions or explosives magazine or storage unit	
156	
264.1202(a)	

	

	
if all contaminated subsoils cannot be practicably removed, owner/operator must close facility and perform post-closure as per 264.310	
156	
264.1202(b)	

	

	
APPENDIX I TO PART 264	

RECORDKEEPING INSTRUCTIONS	

instructions for keeping portions of the operating record	
*,131	
Appendix I	

	

	
APPENDIX IV TO PART 264	

COCHRAN'S APPROXIMATION TO THE BEHRENS-FISHER STUDENTS' T-TEST	

instructions for calculation of the t-test	
*	
Appendix IV	

	

	
APPENDIX V TO PART 264	

EXAMPLES OF POTENTIALLY INCOMPATIBLE WASTE	

list of wastes and potential consequences of mixing	
*	
Appendix V	

	

	
APPENDIX VI TO PART 264	

POLITICAL JURISDICTIONS IN WHICH COMPLIANCE WITH '264.18(a) MUST BE DEMONSTRATED	

political jurisdictions by state and city	
*	
Appendix VI	

	

	
APPENDIX IX TO PART 264	

GROUND-WATER MONITORING LIST	

list of substances, suggested test methods, and practical quantitation limits	
40, 158	
Appendix IX