Doc Init;
-
Vol. 60 No.   1 Tuesday, January 3, 1995  p 242
ENVIRONMENTAL PROTECTION AGENCY

40 CFR Part 268

[FRL_5129_2]

Land Disposal Restrictions Phase II_Universal Treatment Standards, and Treatment Standards for Organic Toxicity Characteristic Wastes and Newly Listed Wastes

AGENCY: Environmental Protection Agency (EPA).

ACTION: Final rule; technical amendments.

SUMMARY: On September 19, 1994, EPA published regulations promulgating congressionally_mandated prohibitions on land disposal of certain hazardous wastes. This notice corrects errors and clarifies the language in the preamble and regulation of the September 19, 1994 final rule.

EFFECTIVE DATE: This rule is effective on December 19, 1994.

ADDRESSES: Copies of the rule can be obtained from the RCRA Docket (5305), U.S. Environmental Protection Agency, Room 2616, 401 M Street, S.W., Washington, D.C. 20460. The RCRA Docket is open from 9:00 am to 4:00 pm Monday through Friday, except for federal holidays. The public must make an appointment to review docket materials by calling (202) 260_9327. The public may copy a maximum of 100 pages from any regulatory document at no cost. Additional copies cost $0.15 per page.

FOR FURTHER INFORMATION CONTACT: For general information contact the RCRA Hotline at (800) 424_9346 (toll free) or (703) 920_9810 in the Washington, DC metropolitan area. For technical information contact Doug Heimlich (5302W), Office of Solid Waste, 401 M Street, S.W., Washington, DC 20460, (703) 308_8489.

>>>> Preamble has not been included in this file. <<<<

	For the reasons set out in the preamble, title 40 chapter I of the Code of Federal Regulations is amended to read as follows:

PART 268_LAND DISPOSAL RESTRICTIONS

	1. The authority citation for part 268 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921, and 6924.

Subpart A_General

	2. In § 268.2, paragraph (i) is revised to read as follows:

§ 268.2  Definitions applicable in this part.

*	*	*	*	*

	(i) "Underlying hazardous constituent" means any constituent listed in § 268.48, Table UTS_Universal Treatment Standards, except vanadium and zinc, which can reasonably be expected to be present at the point of generation of the hazardous waste, at a concentration above the constituent_specific UTS treatment standards.

	3. Section 268.7 is amended by revising the introductory text of paragraphs (a)(1) and (d); revising paragraphs (a)(1)(ii); (a)(1)(iv), (a)(1)(v), (a)(2)(i)(B); (a)(3)(vi); (a)(8); (b)(4)(ii); and (d)(1); and by adding paragraphs (a)(1)(vi) and (a)(3)(vii) to read as follows:

§ 268.7  Waste analysis and recordkeeping.

	(a) * * *

	(1) If a generator determines that he is managing a restricted waste under this part and the waste does not meet the applicable treatment standards set forth in subpart D of this part or it exceeds the applicable prohibition levels set forth in § 268.32 or RCRA section 3004(d), with each shipment of waste the generator must notify the treatment or storage facility in writing. The notice must include the following information:

*	*	*	*	*

	(ii) The waste constituents that the treater will monitor, if monitoring will not include all regulated constituents, for wastes F001_F005, F039, D001, D002, D012_D043 and in § 268.32 or RCRA section 3004(d). Generators must also include whether the waste is a nonwastewater or wastewater (as defined in § 268.2 (d) and (f)), and indicate the subcategory of the waste (such as "D003 reactive cyanide"), if applicable;

*	*	*	*	*

	(iv) For hazardous debris, the contaminants subject to treatment as provided by § 268.45(b) and the following statement: "This hazardous debris is subject to the alternative treatment standards of 40 CFR 268.45;"

	(v) The waste analysis data, where available; and,

	(vi) The date the waste is subject to the prohibitions.

	(2) * * *

	(i) * * *

	(B) The waste constituents that the treater will monitor, if monitoring will not include all regulated constituents, for wastes F001_F005, F039, D001, D002, D012_D043 and § 268.32 or RCRA section 3004(d). Generators must also include whether the waste is a nonwastewater or wastewater (as defined in § 268.2 (d) and (f)), and indicate the subcategory of the waste (such as "D003 reactive cyanide"), if applicable;

*	*	*	*	*

	(3) * * *

	(vi) For hazardous debris when using the treatment standards for the contaminating waste(s) in § 268.40: the requirements described in paragraphs (a)(3) (i), (ii), (iii), (iv), and (vii) of this section; and,

	(vii) The date the waste is subject to the prohibitions.

*	*	*	*	*

	(8) If a generator is managing a lab pack that contains none of the wastes specified in appendix IV of part 268, and wishes to use the alternative treatment standard under § 268.42(c), with each shipment of waste the generator must submit a notice to the treatment facility in accordance with paragraph (a)(1) of this section, except that underlying hazardous constituents need not be determined. The generator must also comply with the requirements in paragraphs (a)(5) and (a)(6) of this section and must submit the following certification, which must be signed by an authorized representative:

	I certify under penalty of law that I personally have examined and am familiar with the waste and that the lab pack does not contain any wastes identified at Appendix IV to part 268. I am aware that there are significant penalties for submitting a false certification including possibility of fine or imprisonment.

*	*	*	*	*

	(b) * * *

	(4) * * *

	(ii) The waste constituents to be monitored, if monitoring will not include all regulated constituents, for wastes F001_F005, F039, D001, D002, D012_D043 and in § 268.32 or RCRA section 3004(d). Generators must also include whether the waste is a nonwastewater or wastewater (as defined in § 268.2 (d) and (f), and indicate the subcategory of the waste (such as D003 reactive cyanide), if applicable.
*	*	*	*	*

	(d) Generators or treaters who first claim that hazardous debris is excluded from the definition of hazardous waste under § 261.3(e) of this chapter (i.e., debris treated by an extraction or destruction technology provided by Table 1, § 268.45, and debris that the EPA Regional Administrator (or his designated representative) or State authorized to implement part 268 requirements has determined does not contain hazardous waste) are subject to the following notification and certification requirements:

	(1) A one_time notification, including the following information, must be submitted to the EPA Regional hazardous waste management division director (or his designated representative) or State authorized to implement part 268 requirements, or State authorized to implement part 268 requirements:

*	*	*	*	*

	4. Section 268.9 is amended by revising paragraph (a) and paragraph (d)(2)(i) to read as follows:

§ 268.9  Special rules regarding wastes that exhibit a characteristic.

	(a) The initial generator of a solid waste must determine each EPA Hazardous Waste Number (waste code) applicable to the waste in order to determine the applicable treatment standards under subpart D of this part. For purposes of part 268, the waste will carry the waste code for any applicable listing under 40 CFR 261, subpart D. In addition, the waste will carry one or more of the waste codes under 40 CFR 261, subpart C, where the waste exhibits a characteristic, except in the case when the treatment standard for the waste listed in part 261, subpart D operates in lieu of the treatment standard for the waste under part 261, subpart C, as specified in paragraph (b) of this section. If the generator determines that his waste displays the characteristic of ignitability (D001) (and is not in the High TOC Ignitable Liquids Subcategory or is not treated by CMBST, or RORGS), or the characteristic of corrosivity (D002), and is prohibited under § 268.37; or that his waste displays the characteristic of toxicity (D012_D043), and is prohibited under § 268.38, the generator must determine the underlying hazardous constituents (as defined in § 268.2), in the D001, D002, or D012_D043 wastes.

*	*	*	*	*

	(d) * * *

	(2) * * *

	(i) If treatment removes the characteristic but does not treat underlying hazardous constituents, then the certification found in § 268.7(b)(5)(iv) applies.

*	*	*	*	* 

Subpart D_Treatment Standards

	5. Section 268.40 is amended by revising the table "Treatment Standards for Hazardous Wastes" to read as follows:

§ 268.40  Applicability of Treatment Standards.

*	*	*	*	* 

TREATMENT STANDARDS FOR HAZARDOUS WASTES						
Waste Code	Waste Description and Treatment/Regulatory Subcategory1	REGULATED HAZARDOUS CONSTITUENT		WASTEWATERS	NONWASTEWATERS	
		Common Name	CAS2 Number	Concentration mg/l3; or Technology Code4	Concentration in mg/kg5 unless noted as "mg/l TCLP" or Technology Code	
D001	Ignitable Characteristic Wastes, except for the § 261.21(a)(1) High TOC Subcategory, that are managed in non-CWA/non-CWA-equivalent/non-Class I SDWA systems.	NA	NA	DEACT and meet § 268.48 standards; or RORGS; or CMBST	DEACT and meet § 268.48 standards; or RORGS; or CMBST	
	Ignitable Characteristic Wastes, except for the § 261.21(a)(1) High TOC Subcategory, that are managed in CWA/CWA-equivalent/Class I SDWA systems	NA	NA	DEACT	DEACT	
	High TOC Ignitable Characteristic Liquids Subcategory based on 40 CFR 261.21(a)(1) - Greater than or equal to 10% total organic carbon.
(Note:  This subcategory consists of nonwastewaters only.)	NA	NA	NA	RORGS; or CMBST	
D002	Corrosive Characteristic Wastes that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems.	NA	NA	DEACT
and meet § 268.48 standards	DEACT
and meet § 268.48 standards	
	Corrosive Characteristic Wastes that are managed in CWA, CWA equivalent, or Class I SDWA systems.	NA	NA	DEACT	DEACT	
D002, D004, D005, D006, D007, D008, D009, D010, D011	Radioactive high level wastes generated during the reprocessing of fuel rods.  (Note:  This subcategory consists of nonwastewaters only.)	Corrosivity (pH)	NA	NA	HLVIT	
		Arsenic	7440-38-2	NA	HLVIT	
		Barium	7440-39-3	NA	HLVIT	
		Cadmium	7440-43-9	NA	HLVIT	
		Chromium (Total)	7440-47-3	NA	HLVIT	
		Lead	7439-92-1	NA	HLVIT	
		Mercury	7439-97-6	NA	HLVIT	
		Selenium	7782-49-2	NA	HLVIT	
		Silver	7440-22-4	NA	HLVIT	
D003	Reactive Sulfides Subcategory based on 261.23(a)(5).	NA	NA	DEACT	DEACT	
	Explosives Subcategory based on 261.23(a)(6), (7), and (8).	NA	NA	DEACT	DEACT	
	Other Reactives Subcategory based on 261.23(a)(1).	NA	NA	DEACT	DEACT	
	Water Reactive Subcategory based on 261.23(a)(2), (3), and (4).
(Note:  This subcategory consists of nonwastewaters only.)	NA	NA	NA	DEACT	
	Reactive Cyanides Subcategory based on 261.23(a)(5).	Cyanides (Total)7	57-12-5	Reserved	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
D004	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for arsenic based on the extraction procedure (EP) in SW846 Method 1310.	Arsenic	7440-38-2	5.0	5.0 mg/l EP	
		Arsenic; alternate6 standard for nonwastewaters only.	7440-38-2	NA	5.0 mg/l TCLP	
D005	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for barium based on the extraction procedure (EP) in SW846 Method 1310.	Barium	7440-39-3	100	100 mg/l TCLP	
D006	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for cadmium based on the extraction procedure (EP) in SW846 Method 1310.	Cadmium	7440-43-9	1.0	1.0 mg/l TCLP	
	Cadmium Containing Batteries Subcategory
(Note:  This subcategory consists of nonwastewaters only.)	Cadmium	7440-43-9	NA	RTHRM	
D007	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for chromium based on the extraction procedure (EP) in SW846 Metod 1310.	Chromium (Total)	7440-47-3	5.0	5.0 mg/l TCLP	
D008	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for lead based on the extraction procedure (EP) in SW846 Method 1310.	Lead	7439-92-1	5.0	5.0 mg/l EP	
		Lead; alternate6 standard for nonwastewaters only	7439-92-1	NA	5.0 mg/l TCLP	
	Lead Acid Batteries Subcategory (Note:  This standard only applies to lead acid batteries that are identified as RCRA hazardous wastes and that are not excluded elsewhere from regulation under the land disposal restrictions of 40 CFR 268 or exempted under other EPA regulations (see 40 CFR 266.80).).
(Note:  This subcategory consists of nonwastewaters only.)	Lead	7439-92-1	NA	RLEAD	
	Radioactive Lead Solids Subcategory (Note:  these lead solids include, but are not limited to, all forms of lead shielding and other elemental forms of lead.  These lead solids do not include treatment residuals such as hydroxide sludges, other wastewater treatment residuals, or incinerator ashes that can undergo conventional pozzolanic stabilization, nor do they include organo-lead materials that can be incinerated and stabilized as ash.).
(Note:  This subcategory consists of nonwastewaters only.)	Lead	7439-92-1	NA	MACRO	
D009	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain greater than or equal to 260 mg/kg total mercury that also contain organics and are not incinerator residues.
(High Mercury-Organic Subcategory)	Mercury	7439-97-6	NA	IMERC; OR RMERC	
	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain greater than or equal to 260 mg/kg total mercury that are inorganic, including incinerator residues and residues from RMERC.
(High Mercury-Inorganic Subcategory)	Mercury	7439-97-6	NA	RMERC	
	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain less than 260 mg/kg total mercury.
(Low Mercury Subcategory)	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	All D009 wastewaters.	Mercury	7439-97-6	0.20	NA	
	Elemental mercury contaminated with radioactive materials.
(Note:  This subcategory consists of nonwastewaters only.)	Mercury	7439-97-6	NA	AMLGM	
	Hydraulic oil contaminated with Mercury Radioactive Materials Subcategory.
(Note:  This subcategory consists of nonwastewaters only.)	Mercury	7439-97-6	NA	IMERC	
D010	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for selenium based on the extraction procedure (EP) in SW846 Method 1310.	Selenium	7782-49-2	1.0	5.7 mg/l TCLP	
D011	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for silver based on the extraction procedure (EP) in SW846 Method 1310.	Silver	7440-22-4	5.0	5.0 mg/l TCLP	
D012	Wastes that are TC for Endrin based on the TCLP in SW846 Method 1311.	Endrin	72-20-8	BIODG; or INCIN	0.13
and meet § 268.48 standards	
		Endrin aldehyde	7421-93-4	BIODG; or INCIN	0.13
and meet § 268.48 standards	
D013	Wastes that are TC for Lindane based on the TCLP in SW846 Method 1311.	alpha-BHC	319-84-6	CARBN; or INCIN	0.066
and meet § 268.48 standards	
		beta-BHC	319-85-7	CARBN; or INCIN	0.066
and meet § 268.48 standards	
		delta-BHC	319-86-8	CARBN; or INCIN	0.066
and meet § 268.48 standards	
		gamma-BHC (Lindane)	58-89-9	CARBN; or INCIN	0.066
and meet § 268.48 standards	
D014	Wastes that are TC for Methoxychlor based on the TCLP in SW846 Method 1311.	Methoxychlor	72-43-5	WETOX or INCIN	0.18
and meet § 268.48 standards	
D015	Wastes that are TC for Toxaphene based on the TCLP in SW846 Method 1311.	Toxaphene	8001-35-2	BIODG or INCIN	2.6
and meet § 268.48 standards	
D016	Wastes that are TC for 2,4-D (2,4-Dichlorophenoxyacetic acid) based on the TCLP in SW846 Method 1311.	2,4-D (2,4-Dichlorophenoxyacetic acid)	94-75-7	CHOXD, BIODG, or INCIN	10
and meet § 268.48 standards	
D017	Wastes that are TC for 2,4,5-TP (Silvex) based on the TCLP in SW846 Method 1311.	2,4,5-TP (Silvex)	93-72-1	CHOXD or INCIN	7.9
and meet § 268.48 standards	
D018	Wastes that are TC for Benzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Benzene	71-43-2	0.14
and meet § 268.48 standards	10
and meet § 268.48 standards	
D019	Wastes that are TC for Carbon tetrachloride based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Carbon tetrachloride	56-23-5	0.057
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D020	Wastes that are TC for Chlordane based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Chlordane (alpha and gamma isomers)	57-74-9	0.0033
and meet § 268.48 standards	0.26
and meet § 268.48 standards	
D021	Wastes that are TC for Chlorobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Chlorobenzene	108-90-7	0.057
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D022	Wastes that are TC for Chloroform based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Chloroform	67-66-3	0.046
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D023	Wastes that are TC for o-Cresol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	o-Cresol	95-48-7	0.11
and meet § 268.48 standards	5.6
and meet § 268.48 standards	
D024	Wastes that are TC for m-Cresol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77
and meet § 268.48 standards	5.6
and meet § 268.48 standards	
D025	Wastes that are TC for p-Cresol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77
and meet § 268.48 standards	5.6
and meet § 268.48 standards	
D026	Wastes that are TC for Cresols (Total) based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations)	1319-77-3	0.88
and meet § 268.48 standards	11.2
and meet § 268.48 standards	
D027	Wastes that are TC for p-Dichlorobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	p-Dichlorobenzene (1,4-Dichlorobenzene)	106-46-7	0.090
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D028	Wastes that are TC for 1,2-Dichloroethane based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	1,2-Dichloroethane	107-06-2	0.21
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D029	Wastes that are TC for 1,1-Dichloroethylene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	1,1-Dichloroethylene	75-35-4	0.025
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D030	Wastes that are TC for 2,4-Dinitrotoluene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	2,4-Dinitrotoluene	121-14-2	0.32
and meet § 268.48 standards	140
and meet § 268.48 standards	
D031	Wastes that are TC for Heptachlor based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Heptachlor	76-44-8	0.0012
and meet § 268.48 standards	0.066
and meet § 268.48 standards	
		Heptachlor epoxide	1024-57-3	0.016
and meet § 268.48 standards	0.066
and meet § 268.48 standards	
D032	Wastes that are TC for Hexachlorobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Hexachlorobenzene	118-74-1	0.055
and meet § 268.48 standards	10
and meet § 268.48 standards	
D033	Wastes that are TC for Hexachlorobutadiene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Hexachlorobutadiene	87-68-3	0.055
and meet § 268.48 standards	5.6
and meet § 268.48 standards	
D034	Wastes that are TC for Hexachloroethane based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Hexachloroethane	67-72-1	0.055
and meet § 268.48 standards	30
and meet § 268.48 standards	
D035	Wastes that are TC for Methyl ethyl ketone based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Methyl ethyl ketone	78-93-3	0.28
and meet § 268.48 standards	36
and meet § 268.48 standards	
D036	Wastes that are TC for Nitrobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Nitrobenzene	98-95-3	0.068
and meet § 268.48 standards	14
and meet § 268.48 standards	
D037	Wastes that are TC for Pentachlorophenol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Pentachlorophenol	87-86-5	0.089
and meet § 268.48 standards	7.4
and meet § 268.48 standards	
D038	Wastes that are TC for Pyridine based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Pyridine	110-86-1	0.014
and meet § 268.48 standards	16
and meet § 268.48 standards	
D039	Wastes that are TC for Tetrachloroethylene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Tetrachloroethylene	127-18-4	0.056
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D040	Wastes that are TC for Trichloroethylene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Trichloroethylene	79-01-6	0.054
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
D041	Wastes that are TC for 2,4,5-Trichlorophenol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	2,4,5-Trichlorophenol	95-95-4	0.18
and meet § 268.48 standards	7.4
and meet § 268.48 standards	
D042	Wastes that are TC for 2,4,6-Trichlorophenol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	2,4,6-Trichlorophenol	88-06-2	0.035
and meet § 268.48 standards	7.4
and meet § 268.48 standards	
D043	Wastes that are TC for Vinyl chloride based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Vinyl chloride	75-01-4	0.27
and meet § 268.48 standards	6.0
and meet § 268.48 standards	
F001, F002, F003, F004, & F005	F001, F002, F003, F004 and/or F005 solvent wastes that contain any combination of one or more of the following spent solvents:  acetone, benzene, n-butyl alcohol, carbon disulfide, carbon tetrachloride, chlorinated fluorocarbons, chlorobenzene, o-cresol, m-cresol, p-cresol, cyclohexanone, o-dichlorobenzene, 2-ethoxyethanol, ethyl acetate, ethyl benzene, ethyl ether, isobutyl alcohol, methanol, methylene chloride, methyl ethyl ketone, methyl isobutyl ketone, nitrobenzene, 2-nitropropane, pyridine, tetrachloroethylene, toluene, 1,1,1-trichloroethane, 1,1,2-trichloroethane, 1,1,2-trichloro- 1,2,2-trifluoroethane, trichloroethylene, trichloromonofluoromethane, and/or xylenes (except as specifically noted in other subcategories).  See further details of these listings in § 261.31	Acetone	67-64-1	0.28	160	
		Benzene	71-43-2	0.14	10	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Carbon disulfide	75-15-0	3.8	NA	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chlorobenzene	108-90-7	0.057	6.0	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations)	1319-77-3	0.88	11.2	
		Cyclohexanone	108-94-1	0.36	NA	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		Ethyl acetate	141-78-6	0.34	33	
		Ethyl benzene	100-41-4	0.057	10	
		Ethyl ether	60-29-7	0.12	160	
		Isobutyl alcohol	78-83-1	5.6	170	
		Methanol	67-56-1	5.6	NA	
		Methylene chloride	75-9-2	0.089	30	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Nitrobenzene	98-95-3	0.068	14	
		Pyridine	110-86-1	0.014	16	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		Toluene	108-88-3	0.080	10	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		1,1,2-Trichloro-1,2,2-trifluoroethane	76-13-1	0.057	30	
		Trichloroethylene	79-01-6	0.054	6.0	
		Trichloromonofluoromethane	75-69-4	0.020	30	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
	F003 and/or F005 solvent wastes that contain any combination of one or more of the following three solvents as the only listed F001-5 solvents:  carbon disulfide, cyclohexanone, and/or methanol.  (formerly 268.41(c))	Carbon disulfide	75-15-0	3.8	4.8 mg/l TCLP	
		Cyclohexanone	108-94-1	0.36	0.75 mg/l TCLP	
		Methanol	67-56-1	5.6	0.75 mg/l TCLP	
	F005 solvent waste containing 2-Nitropropane as the only listed F001-5 solvent.	2-Nitropropane	79-46-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
	F005 solvent waste containing 2-Ethoxyethanol as the only listed F001-5 solvent.	2-Ethoxyethanol	110-80-5	BIODG; or INCIN	INCIN	
F006	Wastewater treatment sludges from electroplating operations except from the following processes:  (1) Sulfuric acid anodizing of aluminum; (2) tin plating on carbon steel; (3) zinc plating (segregated basis) on carbon steel; (4) aluminum or zinc-aluminum plating on carbon steel; (5) cleaning/stripping associated with tin, zinc and aluminum plating on carbon steel; and (6) chemical etching and milling of aluminum.	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F007	Spent cyanide plating bath solutions from electroplating operations.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F008	Plating bath residues from the bottom of plating baths from electroplating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F009	Spent stripping and cleaning bath solutions from electroplating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F010	Quenching bath residues from oil baths from metal heat treating operations where cyanides are used in the process.	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	NA	
F011	Spent cyanide solutions from salt bath pot cleaning from metal heat treating operations.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F012	Quenching wastewater treatment sludges from metal heat treating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F019	Wastewater treatment sludges from the chemical conversion coating of aluminum except from zirconium phosphating in aluminum can washing when such phosphating is an exclusive conversion coating process.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
F020, F021, F022, F023, F026	Wastes (except wastewater and spent carbon from hydrogen chloride purification) from the production or manufacturing use (as a reactant, chemical intermediate, or component in a formulating process) of:  (1) tri- or tetrachlorophenol, or of intermediates used to produce their pesticide derivatives, excluding wastes from the production of Hexachlorophene from highly purified 2,4,5-trichlorophenol (F020); (2) pentachlorophenol, or of intermediates used to produce its derivatives (i.e., F021); (3) tetra-, penta-, or hexachlorobenzenes under alkaline conditions (i.e., F022).
Wastes (except wastewater and spent carbon from hydrogen chloride purification) from the production of materials on equipment previously used for the production or manufacturing use (as a reactant, chemical intermediate, or component in a formulating process) of:  (1) tri- or tetrachlorophenols, excluding wastes from equipment used only for the production of Hexachlorophene from highly purified 2,4,5-trichlorophenol (F023); (2) tetra-, penta-, or hexachlorobenzenes under alkaline conditions (i.e., F026).	HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
F027	Discarded unused formulations containing tri-, tetra-, or pentachlorophenol or discarded unused formulations containing compounds derived from these chlorophenols.  (This listing does not include formulations containing hexachlorophene synthesized from prepurified 2,4,5-trichlorophenol as the sole component.).	HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
F028	Residues resulting from the incineration or thermal treatment of soil contaminated with EPA Hazardous Wastes Nos. F020, F021, F023, F026, and F027.	HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
F024	Process wastes, including but not limited to, distillation residues, heavy ends, tars, and reactor clean-out wastes, from the production of certain chlorinated aliphatic hydrocarbons by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.  (This listing does not include wastewaters, wastewater treatment sludges, spent catalysts, and wastes listed in § 261.31 or § 261.32.).	All F024 wastes	NA	INCIN	INCIN	
		2-Chloro-1,3-butadiene	126-99-8	0.057	0.28	
		3-Chloropropylene	107-05-1	0.036	30	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,2-Dichloropropane	78-87-5	0.85	18	
		cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Hexachloroethane	67-72-1	0.055	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
F025	Condensed light ends from the production of certain chlorinated aliphatic hydrocarbons, by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.
F025 - Light Ends Subcategory	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		Methylene chloride	75-9-2	0.089	30	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
	Spent filters and filter aids, and spent desiccant wastes from the production of certain chlorinated aliphatic hydrocarbons, by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.
F025 - Spent Filters/Aids and Desiccants Subcategory	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Methylene chloride	75-9-2	0.089	30	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
F037	Petroleum refinery primary oil/water/solids separation sludge-Any sludge generated from the gravitational separation of oil/water/solids during the storage or treatment of process wastewaters and oily cooling wastewaters from petroleum refineries.  Such sludges include, but are not limited to, those generated in:  oil/water/solids separators; tanks and impoundments; ditches and other conveyances; sumps; and stormwater units receiving dry weather flow.  Sludge generated in stormwater units that do not receive dry weather flow, sludges generated from non-contact once-through cooling waters segregated for treatment from other process or oily cooling waters, sludges generated in agressive biological treatment units as defined in § 261.31(b)(2) (including sludges generated in one or more additional units after wastewaters have been treated in aggressive biological treatment units) and K051 wastes are not included in this listing.	Acenaphthene	83-32-9	0.059	NA	
		Anthracene	120-12-7	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	.032	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
F038	Petroleum refinery secondary (emulsified) oil/water/solids separation sludge and/or float generated from the physical and/or chemical separation of oil/water/solids in process wastewaters and oily cooling wastewaters from petroleum refineries.  Such wastes include, but are not limited to, all sludges and floats generated in:  induced air floatation (IAF) units, tanks and impoundments, and all sludges generated in DAF units.  Sludges generated in stormwater units that do not receive dry weather flow, sludges generated from non-contact once-through cooling waters segregated for treatment from other process or oily cooling waters, sludges and floats generated in aggressive biological treatment units as defined in § 261.31(b)(2) (including sludges and floats generated in one or more additional units after wastewaters have been treated in aggressive biological units) and F037, K048, and K051 are not included in this listing.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
F039	Leachate (liquids that have percolated through land disposed wastes) resulting from the disposal of more than one restricted waste classified as hazardous under subpart D of this part.  (Leachate resulting from the disposal of one or more of the following EPA Hazardous Wastes and no other Hazardous Wastes retains its EPA Hazardous Waste Number(s):  F020, F021, F022, F026, F027, and/or F028.).	Acenaphthylene	208-96-8	0.059	3.4	
		Acenaphthene	83-32-9	0.059	3.4	
		Acetone	67-64-1	0.28	160	
		Acetonitrile	75-05-8	5.6	NA	
		Acetophenone	96-86-2	0.010	9.7	
		2-Acetylaminofluorene	53-96-3	0.059	140	
		Acrolein	107-02-8	0.29	NA	
		Acrylonitrile	107-13-1	0.24	84	
		Aldrin	309-00-2	0.021	0.066	
		4-Aminobiphenyl	92-67-1	0.13	NA	
		Aniline	62-53-3	0.81	14	
		Anthracene	120-12-7	0.059	3.4	
		Aramite	140-57-8	0.36	NA	
		alpha-BHC	319-84-6	0.00014	0.066	
		beta-BHC	319-85-7	0.00014	0.066	
		delta-BHC	319-86-8	0.023	0.066	
		gamma-BHC	58-89-9	0.0017	0.066	
		Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Benzo(g,h,i)perylene	191-24-2	0.0055	1.8	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Bromodichloromethane	75-27-4	0.35	15	
		Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		4-Bromophenyl phenyl ether	101-55-3	0.055	15	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Butyl benzyl phthalate	85-68-7	0.017	28	
		2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	88-85-7	0.066	2.5	
		Carbon disulfide	75-15-0	3.8	NA	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		p-Chloroaniline	106-47-8	0.46	16	
		Chlorobenzene	108-90-7	0.057	6.0	
		Chlorobenzilate	510-15-6	0.10	NA	
		2-Chloro-1,3-butadiene	126-99-8	0.057	NA	
		Chlorodibromomethane	124-48-1	0.057	15	
		Chloroethane	75-00-3	0.27	6.0	
		bis(2-Chloroethoxy)methane	111-91-1	0.036	7.2	
		bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		Chloroform	67-66-3	0.046	6.0	
		bis(2-Chloroisopropyl)ether	39638-32-9	0.055	7.2	
		p-Chloro-m-cresol	59-50-7	0.018	14	
		Chloromethane (Methyl chloride)	74-87-3	0.19	30	
		2-Chloronaphthalene	91-58-7	0.055	5.6	
		2-Chlorophenol	95-57-8	0.044	5.7	
		3-Chloropropylene	107-05-1	0.036	30	
		Chrysene	218-01-9	0.059	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Cyclohexanone	108-94-1	0.36	NA	
		1,2-Dibromo-3-chloropropane	96-12-8	0.11	15	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
		Dibromomethane	74-95-3	0.11	15	
		2,4-D (2,4-Dichlorophenoxyacetic acid)	94-75-7	0.72	10	
		o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
		o,p'-DDE	3424-82-6	0.031	0.087	
		p,p'-DDE	72-55-9	0.031	0.087	
		o,p'-DDT	789-02-6	0.0039	0.087	
		p,p'-DDT	50-29-3	0.0039	0.087	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Dibenz(a,e)pyrene	192-65-4	0.061	NA	
		m-Dichlorobenzene	541-73-1	0.036	6.0	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Dichlorodifluoromethane	75-71-8	0.23	7.2	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		trans-1,2-Dichloroethylene	156-60-5	0.054	30	
		2,4-Dichlorophenol	120-83-2	0.044	14	
		2,6-Dichlorophenol	87-65-0	0.044	14	
		1,2-Dichloropropane	78-87-5	0.85	18	
		cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
		Dieldrin	60-57-1	0.017	0.13	
		Diethyl phthalate	84-66-2	0.20	28	
		2-4-Dimethyl phenol	105-67-9	0.036	14	
		Dimethyl phthalate	131-11-3	0.047	28	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		1,4-Dinitrobenzene	100-25-4	0.32	2.3	
		4,6-Dinitro-o-cresol	534-52-1	0.28	160	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		2,4-Dinitrotoluene	121-14-2	0.32	140	
		2,6-Dinitrotoluene	606-20-2	0.55	28	
		Di-n-octyl phthalate	117-84-0	0.017	28	
		Di-n-propylnitrosamine	621-64-7	0.40	14	
		1,4-Dioxane	123-91-1	NA	170	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine)	122-39-4	0.92	13	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine)	86-30-6	0.92	NA	
		1,2-Diphenylhydrazine	122-66-7	0.087	NA	
		Disulfoton	298-04-4	0.017	6.2	
		Endosulfan I	939-98-8	0.023	0.066	
		Endosulfan II	33213-6-5	0.029	0.13	
		Endosulfan sulfate	1-31-07-8	0.029	0.13	
		Endrin	72-20-8	0.0028	0.13	
		Endrin aldehyde	7421-93-4	0.025	0.13	
		Ethyl acetate	141-78-6	0.34	33	
		Ethyl cyanide (Propanenitrile)	107-12-0	0.24	360	
		Ethyl benzene	100-41-4	0.057	10	
		Ethyl ether	60-29-7	0.12	160	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Ethyl methacrylate	97-63-2	0.14	160	
		Ethylene oxide	75-21-8	0.12	NA	
		Famphur	52-85-7	0.017	15	
		Fluoranthene	206-44-0	0.068	3.4	
		Fluorene	86-73-7	0.059	3.4	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		Hexachloroethane	67-72-1	0.055	30	
		Hexachloropropylene	1888-71-7	0.035	30	
		Indeno (1,2,3-c,d) pyrene	193-39-5	0.0055	3.4	
		Iodomethane	74-88-4	0.19	65	
		Isobutyl alcohol	78-83-1	5.6	170	
		Isodrin	465-73-6	0.021	0.066	
		Isosafrole	120-58-1	0.081	2.6	
		Kepone	143-50-8	0.0011	0.13	
		Methacrylonitrile	126-98-7	0.24	84	
		Methanol	67-56-1	5.6	NA	
		Methapyrilene	91-80-5	0.081	1.5	
		Methoxychlor	72-43-5	0.25	0.18	
		3-Methylcholanthrene	56-49-5	0.0055	15	
		4,4-Methylene bis(2-chloroaniline)	101-14-4	0.50	30	
		Methylene chloride	75-09-2	0.089	30	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Methyl methacrylate	80-62-6	0.14	160	
		Methyl methansulfonate	66-27-3	0.018	NA	
		Methyl parathion	298-00-0	0.014	4.6	
		Naphthalene	91-20-3	0.059	5.6	
		2-Naphthylamine	91-59-8	0.52	NA	
		p-Nitroaniline	100-01-6	0.028	28	
		Nitrobenzene	98-95-3	0.068	14	
		5-Nitro-o-toluidine	99-55-8	0.32	28	
		p-Nitrophenol	100-02-7	0.12	29	
		N-Nitrosodiethylamine	55-18-5	0.40	28	
		N-Nitrosodimethylamine	62-75-9	0.40	NA	
		N-Nitroso-di-n-butylamine	924-16-3	0.40	17	
		N-Nitrosomethylethylamine	10595-95-6	0.40	2.3	
		N-Nitrosomorpholine	59-89-2	0.40	2.3	
		N-Nitrosopiperidine	100-75-4	0.013	35	
		N-Nitrosopyrrolidine	930-55-2	0.013	35	
		Parathion	56-38-2	0.014	4.6	
		Total PCBs
(sum of all PCB isomers, or all Aroclors)	1336-36-3	0.10	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		Pentachloronitrobenzene	82-68-8	0.055	4.8	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenacetin	62-44-2	0.081	16	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Phorate	298-02-2	0.021	4.6	
		Phthalic anhydride	85-44-9	0.055	NA	
		Pronamide	23950-58-5	0.093	1.5	
		Pyrene	129-00-0	0.067	8.2	
		Pyridine	110-86-1	0.014	16	
		Safrole	94-59-7	0.081	22	
		Silvex (2,4,5-TP)	93-72-1	0.72	7.9	
		2,4,5-T	93-76-5	0.72	7.9	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Toluene	108-88-3	0.080	10	
		Toxaphene	8001-35-2	0.0095	2.6	
		Bromoform (Tribromomethane)	75-25-2	0.63	15	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Trichloromonofluoromethane	75-69-4	0.020	30	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		1,2,3-Trichloropropane	96-18-4	0.85	30	
		1,1,2-Trichloro-1,2,2-trifluoroethane	76-13-1	0.057	30	
		tris(2,3-Dibromopropyl) phosphate	126-72-7	0.11	NA	
		Vinyl chloride	75-01-4	0.27	6.0	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Antimony	7440-36-0	1.9	2.1 mg/l TCLP	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Barium	7440-39-3	1.2	7.6 mg/l TCLP	
		Beryllium	7440-41-7	0.82	NA	
		Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	NA	
		Fluoride	16964-48-8	35	NA	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Mercury	7439-97-6	0.15	0.025 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
		Sulfide	8496-25-8	14	NA	
		Thallium	7440-28-0	1.4	NA	
		Vanadium	7440-62-2	4.3	NA	
K001	Bottom sediment sludge from the treatment of wastewaters from wood preserving processes that use creosote and/or pentachlorophenol.	Naphthalene	91-20-3	0.059	5.6	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenanthrene	85-01-8	0.059	5.6	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K002	Wastewater treatment sludge from the production of chrome yellow and orange pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K003	Wastewater treatment sludge from the production of molybdate orange pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K004	Wastewater treatment sludge from the production of zinc yellow pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K005	Wastewater treatment sludge from the production of chrome green pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
K006	Wastewater treatment sludge from the production of chrome oxide green pigments (anhydrous).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
	Wastewater treatment sludge from the production of chrome oxide green pigments (hydrated).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
K007	Wastewater treatment sludge from the production of iron blue pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
K008	Oven residue from the production of chrome oxide green pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K009	Distillation bottoms from the production of acetaldehyde from ethylene.	Chloroform	67-66-3	0.046	6.0	
K010	Distillation side cuts from the production of acetaldehyde from ethylene.	Chloroform	67-66-3	0.046	6.0	
K011	Bottom stream from the wastewater stripper in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	1.8	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K013	Bottom stream from the acetonitrile column in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	1.8	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K014	Bottoms from the acetonitrile purification column in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	1.8	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K015	Still bottoms from the distillation of benzyl chloride.	Anthracene	120-12-7	0.059	3.4	
		Benzal chloride	98-87-3	0.055	6.0	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Phenanthrene	85-01-8	0.059	5.6	
		Toluene	108-88-3	0.080	10	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K016	Heavy ends or distillation residues from the production of carbon tetrachloride.	Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		Hexachloroethane	67-72-1	0.055	30	
		Tetrachloroethylene	127-18-4	0.056	6.0	
K017	Heavy ends (still bottoms) from the purification column in the production of epichlorohydrin.	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		1,2-Dichloropropane	78-87-5	0.85	18	
		1,2,3-Trichloropropane	96-18-4	0.85	30	
K018	Heavy ends from the fractionation column in ethyl chloride production.	Chloroethane	75-00-3	0.27	6.0	
		Chloromethane	74-87-3	0.19	NA	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	NA	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K019	Heavy ends from the distillation of ethylene dichloride in ethylene dichloride production.	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		Chlorobenzene	108-90-7	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		p-Dichlorobenzene	106-46-7	0.090	NA	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		Fluorene	86-73-7	0.059	NA	
		Hexachloroethane	67-72-1	0.055	30	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	NA	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K020	Heavy ends from the distillation of vinyl chloride in vinyl chloride monomer production.	1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
K021	Aqueous spent antimony catalyst waste from fluoromethanes production.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Antimony	7440-36-0	1.9	2.1 mg/l TCLP	
K022	Distillation bottom tars from the production of phenol/acetone from cumene.	Toluene	108-88-3	0.080	10	
		Acetophenone	96-86-2	0.010	9.7	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine)	122-39-4	0.92	13	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine)	86-30-6	0.92	13	
		Phenol	108-95-2	0.039	6.2	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K023	Distillation light ends from the production of phthalic anhydride from naphthalene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	85-44-9	0.055	28	
K024	Distillation bottoms from the production of phthalic anhydride from naphthalene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	85-44-9	0.055	28	
K025	Distillation bottoms from the production of nitrobenzene by the nitration of benzene.	NA	NA	LLEXT fb SSTRP fb CARBN; or INCIN	INCIN	
K026	Stripping still tails from the production of methyl ethyl pyridines.	NA	NA	INCIN	INCIN	
K027	Centrifuge and distillation residues from toluene diisocyanate production.	NA	NA	CARBN; or INCIN	CMBST	
K028	Spent catalyst from the hydrochlorinator reactor in the production of 1,1,1-trichloroethane.	1,1-Dichloroethane	75-34-3	0.059	6.0	
		trans-1,2-Dichloroethylene	156-60-5	0.054	30	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	NA	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Cadmium	7440-43-9	0.69	NA	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K029	Waste from the product steam stripper in the production of 1,1,1-trichloroethane.	Chloroform	67-66-3	0.046	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
K030	Column bodies or heavy ends from the combined production of trichloroethylene and perchloroethylene.	o-Dichlorobenzene	95-50-1	0.088	NA	
		p-Dichlorobenzene	106-46-7	0.090	NA	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Hexachloropropylene	1888-71-7	NA	30	
		Pentachlorobenzene	608-93-5	NA	10	
		Pentachloroethane	76-01-7	NA	6.0	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K031	By-product salts generated in the production of MSMA and cacodylic acid.	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
K032	Wastewater treatment sludge from the production of chlordane.	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
K033	Wastewater and scrub water from the chlorination of cyclopentadiene in the production of chlordane.	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
K034	Filter solids from the filtration of hexachlorocyclopentadiene in the production of chlordane.	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
K035	Wastewater treatment sludges generated in the production of creosote.	Acenaphthene	83-32-9	NA	3.4	
		Anthracene	120-12-7	NA	3.4	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Chrysene	218-01-9	0.059	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Dibenz(a,h)anthracene	53-70-3	NA	8.2	
		Fluoranthene	206-44-0	0.068	3.4	
		Fluorene	86-73-7	NA	3.4	
		Indeno(1,2,3-cd)pyrene	193-39-5	NA	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
K036	Still bottoms from toluene reclamation distillation in the production of disulfoton.	Disulfoton	298-04-4	0.017	6.2	
K037	Wastewater treatment sludges from the production of disulfoton.	Disulfoton	298-04-4	0.017	6.2	
		Toluene	108-88-3	0.080	10	
K038	Wastewater from the washing and stripping of phorate production.	Phorate	298-02-2	0.021	4.6	
K039	Filter cake from the filtration of diethylphosphorodithioc acid in the production of phorate.	NA	NA	CARBN; or INCIN	CMBST	
K040	Wastewater treatment sludge from the production of phorate.	Phorate	298-02-2	0.021	4.6	
K041	Wastewater treatment sludge from the production of toxaphene.	Toxaphene	8001-35-2	0.0095	2.6	
K042	Heavy ends or distillation residues from the distillation of tetrachlorobenzene in the production of 2,4,5-T.	o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K043	2,6-Dichlorophenol waste from the production of 2,4-D.	2,4-Dichlorophenol	120-83-2	0.044	14	
		2,6-Dichlorophenol	187-65-0	0.044	14	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
K044	Wastewater treatment sludges from the manufacturing and processing of explosives.	NA	NA	DEACT	DEACT	
K045	Spent carbon from the treatment of wastewater containing explosives.	NA	NA	DEACT	DEACT	
K046	Wastewater treatment sludges from the manufacturing, formulation and loading of lead-based initiating compounds.	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K047	Pink/red water from TNT operations.	NA	NA	DEACT	DEACT	
K048	Dissolved air flotation (DAF) float from the petroleum refining industry.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-33	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K049	Slop oil emulsion solids from the petroleum refining industry.	Anthracene	120-12-7	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Carbon disulfide	75-15-0	3.8	NA	
		Chrysene	2218-01-9	0.059	3.4	
		2,4-Dimethylphenol	105-67-9	0.036	NA	
		Ethylbenzene	100-41-4	0.057	10	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-. and p-xylene concentrations)	1330-20-7	0.32	30	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K050	Heat exchanger bundle cleaning sludge from the petroleum refining industry.	Benzo(a)pyrene	50-32-8	0.061	3.4	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K051	API separator sludge from the petroleum refining industry.	Acenaphthene	83-32-9	0.059	NA	
		Anthracene	120-12-7	0.059	3.4	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	2218-01-9	0.059	3.4	
		Di-n-butyl phthalate	105-67-9	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.08	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K052	Tank bottoms (leaded) from the petroleum refining industry.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		2,4-Dimethylphenol	105-67-9	0.036	NA	
		Ethylbenzene	100-41-4	0.057	10	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Toluene	108-88-3	0.08	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K060	Ammonia still lime sludge from coking operations.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
K061	Emission control dust/sludge from the primary production of steel in electric furnaces.	Antimony	7440-36-0	NA	2.1 mg/l TCLP	
		Arsenic	7440-38-2	NA	5.0 mg/l TCLP	
		Barium	7440-39-3	NA	7.6 mg/l TCLP	
		Beryllium	7440-41-7	NA	0.014 mg/l TCLP	
		Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Mercury	7439-97-6	NA	0.025 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Selenium	7782-49-2	NA	0.16 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
		Thallium	NA	NA	0.078 mg/l TCLP	
		Zinc	7440-66-6	NA	5.3 mg/l TCLP	
K062	Spent pickle liquor generated by steel finishing operations of facilities within the iron and steel industry (SIC Codes 331 and 332).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	NA	
K069	Emission control dust/sludge from secondary lead smelting. - Calcium Sulfate (Low Lead) Subcategory	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
	Emission control dust/sludge from secondary lead smelting. - Non-Calcium Sulfate (High Lead) Subcategory	NA	NA	NA	RLEAD	
K071	K071 (Brine purification muds from the mercury cell process in chlorine production, where separately prepurified brine is not used) nonwastewaters that are residues from RMERC.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	K071 (Brine purification muds from the mercury cell process in chlorine production, where separately prepurified brine is not used) nonwastewaters that are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All K071 wastewaters.	Mercury	7439-97-6	0.15	NA	
K073	Chlorinated hydrocarbon waste from the purification step of the diaphragm cell process using graphite anodes in chlorine production.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachloroethane	67-72-1	0.055	30	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K083	Distillation bottoms from aniline production.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		Cyclohexanone	108-94-1	0.36	NA	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine)	122-39-4	0.92	13	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine)	86-30-6	0.92	13	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K084	Wastewater treatment sludges generated during the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
K085	Distillation or fractionation column bottoms from the production of chlorobenzenes.	Benzene	71-43-2	0.14	10	
		Chlorobenzene	108-90-7	0.057	6.0	
		m-Dichlorobenzene	541-73-1	0.036	6.0	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Total PCBs
(sum of all PCB isomers, or all Aroclors)	1336-36-3	0.10	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K086	Solvent wastes and sludges, caustic washes and sludges, or water washes and sludges from cleaning tubs and equipment used in the formulation of ink from pigments, driers, soaps, and stabilizers containing chromium and lead.	Acetone	67-64-1	0.28	160	
		Acetophenone	96-86-2	0.010	9.7	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Butylbenzyl phthalate	85-68-7	0.017	28	
		Cyclohexanone	108-94-1	0.36	NA	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		Diethyl phthalate	84-66-2	0.20	28	
		Dimethyl phthalate	131-11-3	0.047	28	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Di-n-octyl phthalate	117-84-0	0.017	28	
		Ethyl acetate	141-78-6	0.34	33	
		Ethylbenzene	100-41-4	0.057	10	
		Methanol	67-56-1	5.6	NA	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Methylene chloride	75-09-2	0.089	30	
		Naphthalene	91-20-3	0.059	5.6	
		Nitrobenzene	98-95-3	0.068	14	
		Toluene	108-88-3	0.080	10	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K087	Decanter tank tar sludge from coking operations.	Acenaphthylene	208-96-8	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Chrysene	218-01-9	0.059	3.4	
		Fluoranthene	206-44-0	0.068	3.4	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K093	Distillation light ends from the production of phthalic anhydride from ortho-xylene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	85-44-9	0.055	28	
K094	Distillation bottoms from the production of phthalic anhydride from ortho-xylene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	85-44-9	0.055	28	
K095	Distillation bottoms from the production of 1,1,1-trichloroethane.	Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	0.055	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
K096	Heavy ends from the heavy ends column from the production of 1,1,1-trichloroethane.	m-Dichlorobenzene	541-73-1	0.036	6.0	
		Pentachloroethane	76-01-7	0.055	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
K097	Vacuum stripper discharge from the chlordane chlorinator in the production of chlordane.	Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
K098	Untreated process wastewater from the production of toxaphene.	Toxaphene	8001-35-2	0.0095	2.6	
K099	Untreated wastewater from the production of 2,4-D.	2,4-Dichlorophenoxyacetic acid	94-75-7	0.72	10	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
K100	Waste leaching solution from acid leaching of emission control dust/sludge from secondary lead smelting.	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K101	Distillation tar residues from the distillation of aniline-based compounds in the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	o-Nitroaniline	88-74-4	0.27	14	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Cadmium	7440-43-9	0.69	NA	
		Lead	7439-92-1	0.69	NA	
		Mercury	7439-97-6	0.15	NA	
K102	Residue from the use of activated carbon for decolorization in the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	o-Nitrophenol	88-75-5	0.028	13	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Cadmium	7440-43-9	0.69	NA	
		Lead	7439-92-1	0.69	NA	
		Mercury	7439-97-6	0.15	NA	
K103	Process residues from aniline extraction from the production of aniline.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
K104	Combined wastewater streams generated from nitrobenzene/aniline production.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
K105	Separated aqueous stream from the reactor product washing step in the production of chlorobenzenes.	Benzene	71-43-2	0.14	10	
		Chlorobenzene	108-90-7	0.057	6.0	
		2-Chlorophenol	95-57-8	0.044	5.7	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Phenol	108-95-2	0.039	6.2	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
K106	K106 (wastewater treatment sludge from the mercury cell process in chlorine production) nonwastewaters that contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	K106 (wastewater treatment sludge from the mercury cell process in chlorine production) nonwastewaters that contain less than 260 mg/kg total mercury that are residues from RMERC.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	Other K106 nonwastewaters that contain less than 260 mg/kg total mercury and are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All K106 wastewaters.	Mercury	7439-97-6	0.15	NA	
K107	Column bottoms from product separation from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K108	Condensed column overheads from product separation and condensed reactor vent gases from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K109	Spent filter cartridges from product purification from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K110	Condensed column overheads from intermediate separation from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K111	Product washwaters from the production of dinitrotoluene via nitration of toluene	2,4-Dinitrotoluene	121-1-1	0.32	140	
		2,6-Dinitrotoluene	606-20-2	0.55	28	
K112	Reaction by-product water from the drying column in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K113	Condensed liquid light ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	CARBN; or INCIN	CMBST	
K114	Vicinals from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	CARBN; or INCIN	CMBST	
K115	Heavy ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		NA	NA	CARBN; or INCIN	CMBST	
K116	Organic condensate from the solvent recovery column in the production of toluene diisocyanate via phosgenation of toluenediamine.	NA	NA	CARBN; or INCIN	CMBST	
K117	Wastewater from the reactor vent gas scrubber in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K118	Spent absorbent solids from purification of ethylene dibromide in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K123	Process wastewater (including supernates, filtrates, and washwaters) from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K124	Reactor vent scrubber water from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K125	Filtration, evaporation, and centrifugation solids from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K126	Baghouse dust and floor sweepings in milling and packaging operations from the production or formulation of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K131	Wastewater from the reactor and spent sulfuric acid from the acid dryer from the production of methyl bromide.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
K132	Spent absorbent and wastewater separator solids from the production of methyl bromide.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
K136	Still bottoms from the purification of ethylene dibromide in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K141	Process residues from the recovery of coal tar, including, but not limited to, collecting sump residues from the production of coke or the recovery of coke by-products produced from coal.  This listing does not include K087 (decanter tank tar sludge from coking operations).	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-2-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K142	Tar storage tank residues from the production of coke from coal or from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Ideno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K143	Process residues from the recovery of light oil, including, but not limited to, those generated in stills, decanters, and wash oil recovery units from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
K144	Wastewater sump residues from light oil refining, including, but not limited to, intercepting or contamination sump sludges from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
K145	Residues from naphthalene collection and recovery operations from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Naphthalene	91-20-3	0.059	5.6	
K147	Tar storage tank residues from coal tar refining.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K148	Residues from coal tar distillation, including, but not limited to, still bottoms.	Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K149	Distillation bottoms from the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.  (This waste does not include still bottoms from the distillations of benzyl chloride.)	Chlorobenzene	108-90-7	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Chloromethane	74-87-3	0.19	30	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Toluene	108-88-3	0.080	10	
K150	Organic residuals, excluding spent carbon adsorbent, from the spent chlorine gas and hydrochloric acid recovery processes associated with the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Chloromethane	74-87-3	0.19	30	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,1,2,2- Tetrachloroethane	79-34-5	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K151	Wastewater treatment sludges, excluding neutralization and biological sludges, generated during the treatment of wastewaters from the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.	Benzene	71-43-2	0.14	10	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		Toluene	108-88-3	0.080	10	
P001	Warfarin, & salts, when present at concentrations greater than 0.3%	Warfarin	81-81-2	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P002	1-Acetyl-2-thiourea	1-Acetyl-2-thiourea	591-08-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P003	Acrolein	Acrolein	107-02-8	0.29	CMBST	
P004	Aldrin	Aldrin	309-00-2	0.021	0.066	
P005	Allyl alcohol	Allyl alcohol	107-18-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P006	Aluminum phosphide	Aluminum phosphide	20859-73-8	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
P007	5-Aminomethyl 3-isoxazolol	5-Aminomethyl 3-isoxazolol	2763-96-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P008	4-Aminopyridine	4-Aminopyridine	504-24-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P009	Ammonium picrate	Ammonium picrate	131-74-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
P010	Arsenic acid	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P011	Arsenic pentoxide	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P012	Arsenic trioxide	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P013	Barium cyanide	Barium	7440-39-3	NA	7.6 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P014	Thiophenol (Benzene thiol)	Thiophenol (Benzene thiol)	108-98-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P015	Beryllium dust	Beryllium	7440-41-7	RMETL;or RTHRM	RMETL; or RTHRM	
P016	Dichloromethyl ether (Bis(chloromethyl)ether)	Dichloromethyl ether	542-88-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P017	Bromoacetone	Bromoacetone	598-31-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P018	Brucine	Brucine	357-57-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P020	2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	88-85-7	0.066	2.5	
P021	Calcium cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P022	Carbon disulfide	Carbon disulfide	75-15-0	3.8	INCIN	
		Carbon disulfide; alternate6 standard for nonwastewaters only	75-15-0	NA	4.8 mg/l TCLP	
P023	Chloroacetaldehyde	Chloroacetaldehyde	107-20-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P024	p-Chloroaniline	p-Chloroaniline	106-47-8	0.46	16	
P026	1-(o-Chlorophenyl)thiourea	1-(o-Chlorophenyl)thiourea	5344-82-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P027	3-Chloropropionitrile	3-Chloropropionitrile	542-76-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P028	Benzyl chloride	Benzyl chloride	100-44-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P029	Copper cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P030	Cyanides (soluble salts and complexes)	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P031	Cyanogen	Cyanogen	460-19-5	CHOXD; WETOX; or INCIN	CHOXD; WETOX; or INCIN	
P033	Cyanogen chloride	Cyanogen chloride	506-77-4	CHOXD; WETOX; or INCIN	CHOXD; WETOX; or INCIN	
P034	2-Cyclohexyl-4,6-dinitrophenol	2-Cyclohexyl-4,6-dinitrophenol	131-89-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P036	Dichlorophenylarsine	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P037	Dieldrin	Dieldrin	60-57-1	0.017	0.13	
P038	Diethylarsine	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P039	Disulfoton	Disulfoton	298-04-4	0.017	6.2	
P040	O,O-Diethyl O-pyrazinyl phosphorothioate	O,O-Diethyl O-pyrazinyl phosphorothioate	297-97-2	CARBN; or INCIN	CMBST	
P041	Diethyl-p-nitrophenyl phosphate	Diethyl-p-nitrophenyl phosphate	311-45-5	CARBN; or INCIN	CMBST	
P042	Epinephrine	Epinephrine	51-43-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P043	Diisopropylfluorophosphate (DFP)	Diisopropylfluorophosphate (DFP)	55-91-4	CARBN; or INCIN	CMBST	
P044	Dimethoate	Dimethoate	60-51-5	CARBN; or INCIN	CMBST	
P045	Thiofanox	Thiofanox	39196-18-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P046	alpha, alpha-Dimethylphenethylamine	alpha, alpha-Dimethylphenethylamine	122-09-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P047	4,6-Dinitro-o-cresol	4,6-Dinitro-o-cresol	543-52-1	0.28	160	
	4,6-Dinitro-o-cresol salts	NA	NA	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P048	2,4-Dinitrophenol	2,4-Dinitrophenol	51-28-5	0.12	160	
P049	Dithiobiuret	Dithiobiuret	541-53-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P050	Endosulfan	Endosulfan I	939-98-8	0.023	0.066	
		Endosulfan II	33213-6-5	0.029	0.13	
		Endosulfan sulfate	1031-07-8	0.029	0.13	
P051	Endrin	Endrin	72-20-8	0.0028	0.13	
		Endrin aldehyde	7421-93-4	0.025	0.13	
P054	Aziridine	Aziridine	151-56-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P056	Fluorine	Fluoride (measured in wastewaters only)	16964-48-8	35	ADGAS fb NEUTR	
P057	Fluoroacetamide	Fluoroacetamide	640-19-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P058	Fluoroacetic acid, sodium salt	Fluoroacetic acid, sodium salt	62-74-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P059	Heptachlor	Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
P060	Isodrin	Isodrin	465-73-6	0.021	0.066	
P062	Hexaethyl tetraphosphate	Hexaethyl tetraphosphate	757-58-4	CARBN; or INCIN	CMBST	
P063	Hydrogen cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P064	Isocyanic acid, ethyl ester	Isocyanic acid, ethyl ester	624-83-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P065	P065 (mercury fulminate) nonwastewaters, regardless of their total mercury content, that are not incinerator residues or are not residues from RMERC.	Mercury	7439-97-6	NA	IMERC	
	P065 (mercury fulminate) nonwastewaters that are either incinerator residues or are residues from RMERC; and contain greater than or equal to 260 mg/kg total mercury.	Mercury	7339-97-6	NA	RMERC	
	P065 (mercury fulminate) nonwastewaters that are residues from RMERC and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	P065 (mercury fulminate) nonwastewaters that are incinerator residues and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All P065 (mercury fulminate) wastewaters.	Mercury	7439-97-6	0.15	NA	
P066	Methomyl	Methomyl	16752-77-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P067	2-Methyl-aziridine	2-Methyl-aziridine	75-55-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P068	Methyl hydrazine	Methyl hydrazine	60-34-4	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED, or CMBST	
P069	2-Methyllactonitrile	2-Methyllactonitrile	75-86-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P070	Aldicarb	Aldicarb	116-06-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P071	Methyl parathion	Methyl parathion	298-00-0	0.014	4.6	
P072	1-Naphthyl-2-thiourea	1-Naphthyl-2-thiourea	86-88-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P073	Nickel carbonyl	Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
P074	Nickel cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
P075	Nicotine and salts	Nicotine and salts	54-11-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P076	Nitric oxide	Nitric oxide	10102-43-9	ADGAS	ADGAS	
P077	p-Nitroaniline	p-Nitroaniline	100-01-6	0.028	28	
P078	Nitrogen dioxide	Nitrogen dioxide	10102-44-0	ADGAS	ADGAS	
P081	Nitroglycerin	Nitroglycerin	55-63-0	CHOXD; CHRED; CARBN; BIODG or INCIN	CHOXD; CHRED; or CMBST	
P082	N-Nitrosodimethylamine	N-Nitrosodimethylamine	62-75-9	0.40	2.3	
P084	N-Nitrosomethylvinylamine	N-Nitrosomethylvinylamine	4549-40-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P085	Octamethylpyrophosphoramide	Octamethylpyrophosphoramide	152-16-9	CARBN; or INCIN	CMBST	
P087	Osmium tetroxide	Osmium tetroxide	20816-12-0	RMETL; or RTHRM	RMETL; or RTHRM	
P088	Endothall	Endothall	145-73-3	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P089	Parathion	Parathion	56-38-2	0.014	4.6	
P092	P092 (phenyl mercuric acetate) nonwastewaters, regardless of their total mercury content, that are not incinerator residues or are not residues from RMERC.	Mercury	7439-97-6	NA	IMERC; or RMERC	
	P092 (phenyl mercuric acetate) nonwastewaters that are either incinerator residues or are residues from RMERC; and still contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	P092 (phenyl mercuric acetate) nonwastewaters that are residues from RMERC and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	P092 (phenyl mercuric acetate) nonwastewaters that are incinerator residues and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All P092 (phenyl mercuric acetate) wastewaters.	Mercury	7439-97-6	0.15	NA	
P093	Phenylthiouea	Phenylthiouea	103-85-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P094	Phorate	Phorate	298-02-2	0.021	4.6	
P095	Phosgene	Phosgene	75-44-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P096	Phosphine	Phosphine	7803-51-2	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
P097	Famphur	Famphur	52-85-7	0.017	15	
P098	Potassium cyanide.	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P099	Potassium silver cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
P101	Ethyl cyanide (Propanenitrile)	Ethyl cyanide (Propanenitrile)	107-12-0	0.24	360	
P102	Propargyl alcohol	Propargyl alcohol	107-19-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P103	Selenourea	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
P104	Silver cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
P105	Sodium azide	Sodium azide	26628-22-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
P106	Sodium cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P108	Strychnine and salts	Strychnine and salts	57-24-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P109	Tetraethyldithiopyrophosphate	Tetraethyldithiopyrophosphate	3689-24-5	CARBN; or INCIN	CMBST	
P110	Tetraethyl lead	lead	7439-92-1	0.69	0.37 mg/l TCLP	
P111	Tetraethylpyrophosphate	Tetraethylpyrophosphate	107-49-3	CARBN; or INCIN	CMBST	
P112	Tetranitromethane	Tetranitromethane	509-14-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
P113	Thallic oxide	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
P114	Thallium selenite	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
P115	Thallium (I) sulfate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
P116	Thiosemicarbazide	Thiosemicarbazide	79-19-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P118	Trichloromethanethiol	Trichloromethanethiol	75-70-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P119	Ammonium vanadate	Vanadium (measured in wastewaters only)	7440-62-2	4.3	STABL	
P120	Vanadium pentoxide	Vanadium (measured in wastewaters only)	7440-62-2	4.3	STABL	
P121	Zinc cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P122	Zinc phosphide Zn3P2, when present at concentrations greater than 10%	Zinc Phosphide	1314-84-7	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
P123	Toxaphene	Toxaphene	8001-35-2	0.0095	2.6	
U001	Acetaldehyde	Acetaldehyde	75-07-0	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U002	Acetone	Acetone	67-64-1	0.28	160	
U003	Acetonitrile	Acetonitrile	75-05-8	5.6	INCIN	
		Acetonitrile; alternate6 standard for nonwastewaters only	75-05-8	NA	1.8	
U004	Acetophenone	Acetophenone	98-86-2	0.010	9.7	
U005	2-Acetylaminofluorene	2-Acetylaminofluorene	53-96-3	0.059	140	
U006	Acetyl chloride	Acetyl Chloride	75-36-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U007	Acrylamide	Acrylamide	79-06-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U008	Acrylic acid	Acrylic acid	79-10-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U009	Acrylonitrile	Acrylonitrile	107-13-1	0.24	84	
U010	Mitomycin C	Mitomycin C	50-07-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U011	Amitrole	Amitrole	61-82-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U012	Aniline	Aniline	62-53-3	0.81	14	
U014	Auramine	Auramine	492-80-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U015	Azaserine	Azaserine	115-02-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U016	Benz(c)acridine	Benz(c)acridine	225-51-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U017	Benzal chloride	Benzal chloride	98-87-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U018	Benz(a)anthracene	Benz(a)anthracene	56-55-3	0.059	3.4	
U019	Benzene	Benzene	71-43-2	0.14	10	
U020	Benzenesulfonyl chloride	Benzenesulfonyl chloride	98-09-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U021	Benzidine	Benzidine	92-87-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U022	Benzo(a)pyrene	Benzo(a)pyrene	50-32-8	0.061	3.4	
U023	Benzotrichloride	Benzotrichloride	98-07-7	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U024	bis(2-Chloroethoxy)methane	bis(2-Chloroethoxy)methane	111-91-1	0.036	7.2	
U025	bis(2-Chloroethyl)ether	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
U026	Chlornaphazine	Chlornaphazine	494-03-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U027	bis(2-Chloroisopropyl)ether	bis(2-Chloroisopropyl)ether	39638-32-9	(WETOX or CHOXD) fb CARBN; or INCIN	7.2	
U028	bis(2-Ethylhexyl)phthalate	bis(2-Ethylhexyl)phthalate	117-81-7	0.28	28	
U029	Methyl bromide (Bromomethane)	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
U030	4-Bromophenyl phenyl ether	4-Bromophenyl phenyl ether	101-55-3	0.055	15	
U031	n-Butyl alcohol	n-Butyl alcohol	71-36-3	5.6	2.6	
U032	Calcium chromate	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
U033	Carbon oxyfluoride	Carbon oxyfluoride	353-50-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U034	Trichloroacetaldehyde (Chloral)	Trichloroacetaldehyde (Chloral)	75-87-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U035	Chlorambucil	Chlorambucil	305-03-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U036	Chlordane	Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
U037	Chlorobenzene	Chlorobenzene	108-90-7	0.057	6.0	
U038	Chlorobenzilate	Chlorobenzilate	510-15-6	0.10	INCIN	
U039	p-Chloro-m-cresol	p-Chloro-m-cresol	59-50-7	0.018	14	
U041	Epichlorohydrin (1-Chloro-2,3-epoxypropane)	Epichlorohydrin (1-Chloro-2,3-epoxypropane)	106-89-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U042	2-Chloroethyl vinyl ether	2-Chloroethyl vinyl ether	110-75-8	0.062	INCIN	
U043	Vinyl chloride	Vinyl chloride	75-01-4	0.27	6.0	
U044	Chloroform	Chloroform	67-66-3	0.046	6.0	
U045	Chloromethane (Methyl chloride)	Chloromethane (Methyl chloride)	74-87-3	0.19	30	
U046	Chloromethyl methyl ether	Chloromethyl methyl ether	107-30-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U047	2-Chloronaphthalene	2-Chloronaphthalene	91-58-7	0.055	5.6	
U048	2-Chlorophenol	2-Chlorophenol	95-57-8	0.044	5.7	
U049	4-Chloro-o-toluidine hydrochloride	4-Chloro-o-toluidine hydrochloride	3165-93-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U050	Chrysene	Chrysene	218-01-9	0.059	3.4	
U051	Creosote	Naphthalene	91-20-3	0.059	5.6	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenanthrene	85-01-8	0.059	5.6	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U052	Cresols (Cresylic acid)	o-Cresol	95-48-7	0.11	5.6	
		m-Cresol (difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol (difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations)	1319-77-3	0.88	11.2	
U053	Crotonaldehyde	Crotonaldehyde	4170-30-3	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U055	Cumene	Cumene	98-82-8	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U056	Cyclohexane	Cyclohexane	110-82-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U057	Cyclohexanone	Cyclohexanone	108-94-1	0.36	CMBST	
		Cyclohexanone; alternate6 standard for nonwastewaters only	108-94-1	NA	0.75 mg/l TCLP	
U058	Cyclophosphamide	Cyclophosphamide	50-18-0	CARBN; or INCIN	CMBST	
U059	Daunomycin	Daunomycin	20830-81-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U060	DDD	o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
U061	DDT	o,p'-DDT	789-02-6	0.0039	0.087	
		p,p'-DDT	50-29-3	0.0039	0.087	
		o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
		o,p'-DDE	3424-82-6	0.031	0.087	
		p,p'-DDE	72-55-9	0.031	0.087	
U062	Diallate	Diallate	2303-16-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U063	Dibenz(a,h)anthracene	Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
U064	Dibenz(a,i)pyrene	Dibenz(a,i)pyrene	189-55-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U066	1,2-Dibromo-3-chloropropane	1,2-Dibromo-3-chloropropane	96-12-8	0.11	15	
U067	Ethylene dibromide (1,2-Dibromoethane)	Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
U068	Dibromomethane	Dibromomethane	74-95-3	0.11	15	
U069	Di-n-butyl phthalate	Di-n-butyl phthalate	84-74-2	0.057	28	
U070	o-Dichlorobenzene	o-Dichlorobenzene	95-50-1	0.088	6.0	
U071	m-Dichlorobenzene	m-Dichlorobenzene	541-73-1	0.036	6.0	
U072	p-Dichlorobenzene	p-Dichlorobenzene	106-46-7	0.090	6.0	
U073	3,3'-Dichlorobenzidine	3,3'-Dichlorobenzidine	91-94-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U074	1,4-Dichloro-2-butene	cis-1,4-Dichloro-2-butene	1476-11-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
		trans-1,4-Dichloro-2-butene	764-41-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U075	Dichlorodifluoromethane	Dichlorodifluoromethane	75-71-8	0.23	7.2	
U076	1,1-Dichloroethane	1,1-Dichloroethane	75-34-3	0.059	6.0	
U077	1,2-Dichloroethane	1,2-Dichloroethane	107-06-2	0.21	6.0	
U078	1,1-Dichloroethylene	1,1-Dichloroethylene	75-35-4	0.025	6.0	
U079	1,2-Dichloroethylene	trans-1,2-Dichloroethylene	156-60-5	0.054	30	
U080	Methylene chloride	Methylene chloride	75-09-2	0.089	30	
U081	2,4-Dichlorophenol	2,4-Dichlorophenol	120-83-2	0.044	14	
U082	2,6-Dichlorophenol	2,6-Dichlorophenol	87-65-0	0.044	14	
U083	1,2-Dichloropropane	1,2-Dichloropropane	78-87-5	0.85	18	
U084	1,3-Dichloropropylene	cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
U085	1,2:3,4-Diepoxybutane	1,2:3,4-Diepoxybutane	1464-53-5	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U086	N,N'-Diethylhydrazine	N,N'-Diethylhydrazine	1615-80-1	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U087	O,O-Diethyl S-methyldithiophosphate	O,O-Diethyl S-methyldithiophosphate	3288-58-2	CARBN; or INCIN	CMBST	
U088	Diethyl phthalate	Diethyl phthalate	84-66-2	0.20	28	
U089	Diethyl stilbestrol	Diethyl stilbestrol	56-53-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U090	Dihydrosafrole	Dihydrosafrole	94-58-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U091	3,3'-Dimethoxybenzidine	3,3'-Dimethoxybenzidine	119-90-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U092	Dimethylamine	Dimethylamine	124-40-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U093	p-Dimethylaminoazobenzene	p-Dimethylaminoazobenzene	60-11-7	0.13	INCIN	
U094	7,12-Dimethylbenz(a)anthracene	7,12-Dimethylbenz(a)anthracene	57-97-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U095	3,3'-Dimethylbenzidine	3,3'-Dimethylbenzidine	119-93-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U096	alpha, alpha-Dimethyl benzyl hydroperoxide	alpha, alpha-Dimethyl benzyl hydroperoxide	80-15-9	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U097	Dimethylcarbamoyl chloride	Dimethylcarbamoyl chloride	79-44-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U098	1,1-Dimethylhydrazine	1,1-Dimethylhydrazine	57-14-7	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U099	1,2-Dimethylhydrazine	1,2-Dimethylhydrazine	540-73-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U101	2,4-Dimethylphenol	2,4-Dimethylphenol	105-67-9	0.036	14	
U102	Dimethyl phthalate	Dimethyl phthalate	131-11-3	0.047	28	
U103	Dimethyl sulfate	Dimethyl sulfate	77-78-1	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U105	2,4-Dinitrotoluene	2,4-Dinitrotoluene	121-14-2	0.32	140	
U106	2,6-Dinitrotoluene	2,6-Dinitrotoluene	606-20-2	0.55	28	
U107	Di-n-octyl phthalate	Di-n-octyl phthalate	117-84-0	0.017	28	
U108	1,4-Dioxane	1,4-Dioxane	123-91-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
		1,4-Dioxane; alternate6 standard for nonwastewaters only	123-91-1	NA	170	
U109	1,2-Diphenylhydrazine	1,2-Diphenylhydrazine	122-66-7	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
		1,2-Diphenylhydrazine; alternate6 standard for wastewaters only	122-66-7	0.087	NA	
U110	Dipropylamine	Dipropylamine	142-84-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U111	Di-n-propylnitrosamine	Di-n-propylnitrosamine	621-64-7	0.40	14	
U112	Ethyl acetate	Ethyl acetate	141-78-6	0.34	33	
U113	Ethyl acrylate	Ethyl acrylate	140-88-5	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U114	Ethylenebisdithiocarbamic acid salts and esters	Ethylenebisdithiocarbamic acid	111-54-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U115	Ethylene oxide	Ethylene oxide 	75-21-8	(WETOX or CHOXD) fb CARBN; or INCIN	CHOXD; or INCIN	
		Ethylene oxide; alternate 6 standard for wastewaters only	75-21-8	0.12	NA	
U116	Ethylene thiourea	Ethylene thiourea	96-45-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U117	Ethyl ether	Ethyl ether	60-29-7	0.12	160	
U118	Ethyl methacrylate	Ethyl methacrylate	97-63-2	0.14	160	
U119	Ethyl methane sulfonate	Ethyl methane sulfonate	62-50-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U120	Fluoranthene	Fluoranthene	206-44-0	0.068	3.4	
U121	Trichloromonofluoromethane	Trichloromonofluoromethane	75-69-4	0.020	30	
U122	Formaldehyde	Formaldehyde	50-00-0	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U123	Formic acid	Formic acid	64-18-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U124	Furan	Furan	110-00-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U125	Furfural	Furfural	98-01-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U126	Glycidylaldehyde	Glycidylaldehyde	765-34-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U127	Hexachlorobenzene	Hexachlorobenzene	118-74-1	0.055	10	
U128	Hexachlorobutadiene	Hexachlorobutadiene	87-68-3	0.055	5.6	
U129	Lindane	alpha-BHC	319-84-6	0.00014	0.066	
		beta-BHC	319-85-7	0.00014	0.066	
		delta-BHC	319-86-8	0.023	0.066	
		gamma-BHC (Lindane)	58-89-9	0.0017	0.066	
U130	Hexachlorocyclopentadiene	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
U131	Hexachloroethane	Hexachloroethane	67-72-1	0.055	30	
U132	Hexachlorophene	Hexachlorophene	70-30-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U133	Hydrazine	Hydrazine	302-01-2	CHOXD; CHRED; CARBN; DIODG; or INCIN	CHOXD; CHRED; or CMBST	
U134	Hydrogen fluoride	Fluoride (measured in wastewaters only)	16964-48-8	35	ADGAS fb NEUTR; or NEUTR	
U135	Hydrogen Sulfide	Hydrogen Sulfide	7783-06-4	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
U136	Cacodylic acid	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
U137	Indeno(1,2,3-cd)pyrene	Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
U138	Iodomethane	Iodomethane	74-88-4	0.19	65	
U140	Isobutyl alcohol	Isobutyl alcohol	78-83-1	5.6	170	
U141	Isosafrole	Isosafrole	120-58-1	0.081	2.6	
U142	Kepone	Kepone	143-50-8	0.0011	0.13	
U143	Lasiocarpine	Lasiocarpine	303-34-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U144	Lead acetate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U145	Lead phosphate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U146	Lead subacetate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U147	Maleic anhydride	Maleic anhydride	108-31-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U148	Maleic hydrazide	Maleic hydrazide	123-33-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U149	Malononitrile	Malononitrile	109-77-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U150	Melphalan	Melphalan	148-82-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U151	U151 (mercury) nonwastewaters that contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	U151 (mercury) nonwastewaters that contain less than 260 mg/kg total mercury and that are residues from RMERC only.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	U151 (mercury) nonwastewaters that contain less than 260 mg/kg total mercury and that are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All U151 (mercury) wastewaters.	Mercury	7439-97-6	0.15	NA	
	Elemental Mercury Contaminated with Radioactive Materials	Mercury	7439-97-6	NA	AMLGM	
U152	Methacrylonitrile	Methacrylonitrile	126-98-7	0.24	84	
U153	Methanethiol	Methanethiol	74-93-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U154	Methanol	Methanol	67-56-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
		Methanol; alternate6 set of standards for both wastewaters and nonwastewaters	67-56-1	5.6	0.75 mg/l TCLP	
U155	Methapyrilene	Methapyrilene	91-80-5	0.081	1.5	
U156	Methyl chlorocarbonate	Methyl chlorocarbonate	79-22-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U157	3-Methylcholanthrene	3-Methylcholanthrene	56-49-5	0.0055	15	
U158	4,4'-Methylene bis(2-chloroaniline)	4,4'-Methylene bis(2-chloroaniline)	101-14-4	0.50	30	
U159	Methyl ethyl ketone	Methyl ethyl ketone	78-93-3	0.28	36	
U160	Methyl ethyl ketone peroxide	Methyl ethyl ketone peroxide	1338-23-4	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U161	Methyl isobutyl ketone	Methyl isobutyl ketone	108-10-1	0.14	33	
U162	Methyl methacrylate	Methyl methacrylate	80-62-6	0.14	160	
U163	N-Methyl N'-nitro N-nitrosoguanidine	N-Methyl N'-nitro N-nitrosoguanidine	70-25-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U164	Methylthiouracil	Methylthiouracil	56-04-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U165	Naphthalene	Naphthalene	91-20-3	0.059	5.6	
U166	1,4-Naphthoquinone	1,4-Naphthoquinone	130-15-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U167	1-Naphthlyamine	1-Naphthlyamine	134-32-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U168	2-Naphthlyamine	2-Naphthlyamine	91-59-8	0.52	INCIN	
U169	Nitrobenzene	Nitrobenzene	98-95-3	0.068	14	
U170	p-Nitrophenol	p-Nitrophenol	100-02-7	0.12	29	
U171	2-Nitropropane	2-Nitropropane	79-46-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U172	N-Nitrosodi-n-butylamine	N-Nitrosodi-n-butylamine	924-16-3	0.40	17	
U173	N-Nitrosodiethanolamine	N-Nitrosodiethanolamine	1116-54-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U174	N-Nitrosodiethylamine	N-Nitrosodiethylamine	55-18-5	0.40	28	
U176	N-Nitroso-N-ethylurea	N-Nitroso-N-ethylurea	759-73-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U177	N-Nitroso-N-methylurea	N-Nitroso-N-methylurea	684-93-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U178	N-Nitroso-N-methylurethane	N-Nitroso-N-methylurethane	615-53-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U179	N-Nitrosopiperidine	N-Nitrosopiperidine	100-75-4	0.013	35	
U180	N-Nitrosopyrrolidine	N-Nitrosopyrrolidine	930-55-2	0.013	35	
U181	5-Nitro-o-toluidine	5-Nitro-o-toluidine	99-55-8	0.32	28	
U182	Paraldehyde	Paraldehyde	123-63-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U183	Pentachlorobenzene	Pentachlorobenzene	608-93-5	0.055	10	
U184	Pentachloroethane	Pentachloroethane	76-01-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
		Pentachloroethane; alternate6 standards for both wastewaters and nonwastewaters	76-01-7	0.055	6.0	
U185	Pentachloronitrobenzene	Pentachloronitrobenzene	82-68-8	0.055	4.8	
U186	1,3-Pentadiene	1,3-Pentadiene	504-60-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U187	Phenacetin	Phenacetin	62-44-2	0.081	16	
U188	Phenol	Phenol	108-95-2	0.039	6.2	
U189	Phosphorus sulfide	Phosphorus sulfide	1314-80-3	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
U190	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride	85-44-9	0.055	28	
U191	2-Picoline	2-Picoline	109-06-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U192	Pronamide	Pronamide	23950-58-5	0.093	1.5	
U193	1,3-Propane sultone	1,3-Propane sultone	1120-71-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U194	n-Propylamine	n-Propylamine	107-10-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U196	Pyridine	Pyridine	110-86-1	0.014	16	
U197	p-Benzoquinone	p-Benzoquinone	106-51-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U200	Reserpine	Reserpine	50-55-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U201	Resorcinol	Resorcinol	108-46-3	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U202	Saccharin and salts	Saccharin	81-07-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U203	Safrole	Safrole	94-59-7	0.081	22	
U204	Selenium dioxide	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
U205	Selenium sulfide	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
U206	Streptozotocin	Streptozotocin	18883-66-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U207	1,2,4,5-Tetrachlorobenzene	1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
U208	1,1,1,2-Tetrachloroethane	1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
U209	1,1,2,2-Tetrachloroethane	1,1,2,2-Tetrachloroethane	79-34-5	0.057	6.0	
U210	Tetrachloroethylene	Tetrachloroethylene	127-18-4	0.056	6.0	
U211	Carbon tetrachloride	Carbon tetrachloride	56-23-5	0.057	6.0	
U213	Tetrahydrofuran	Tetrahydrofuran	109-99-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U214	Thallium (I) acetate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U215	Thallium (I) carbonate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U216	Thallium (I) chloride	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U217	Thallium (I) nitrate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U218	Thioacetamide	Thioacetamide	62-55-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U219	Thiourea	Thiourea	62-56-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U220	Toluene	Toluene	108-88-3	0.080	10	
U221	Toluenediamine	Toluenediamine	25376-45-8	CARBN; or INCIN	CMBST	
U222	o-Toluidine hydrochloride	o-Toluidine hydrochloride	636-21-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U223	Toluene diisocyanate	Toluene diisocyanate	26471-62-5	CARBN; or INCIN	CMBST	
U225	Bromoform (Tribromomethane)	Bromoform (Tribromomethane)	75-25-2	0.63	15	
U226	1,1,1-Trichloroethane	1,1,1-Trichloroethane	71-55-6	0.054	6.0	
U227	1,1,2-Trichloroethane	1,1,2-Trichloroethane	79-00-5	0.054	6.0	
U228	Trichloroethylene	Trichloroethylene	79-01-6	0.054	6.0	
U234	1,3,5-Trinitrobenzene	1,3,5-Trinitrobenzene	99-35-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U235	tris-(2,3-Dibromopropyl)-phosphate	tris-(2,3-Dibromopropyl)-phosphate	126-72-7	0.11	0.10	
U236	Trypan Blue	Trypan Blue	72-57-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U237	Uracil mustard	Uracil mustard	66-75-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U238	Urethane (Ethyl carbamate)	Urethane (Ethyl carbamate)	51-79-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U239	Xylenes	Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
U240	2,4-D (2,4-Dichlorophenoxyacetic acid)	2,4-D (2,4-Dichlorophenoxyacetic acid)	94-75-7	0.72	10	
	2,4-D (2,4-Dichlorophenoxyacetic acid) salts and esters		NA	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U243	Hexachloropropylene	Hexachloropropylene	1888-71-7	0.035	30	
U244	Thiram	Thiram	137-26-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U246	Cyanogen bromide	Cyanogen bromide	506-68-3	CHOXD; WETOX; or INCIN	CHOXD; WETOX; or INCIN	
U247	Methoxychlor	Methoxychlor	72-43-5	0.25	0.18	
U248	Warfarin, & salts, when present at concentrations of 0.3% or less	Warfarin	81-81-2	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U249	Zinc phosphide, Zn3P2, when present at concentrations of 10% or less	Zinc Phosphide	1314-84-7	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
U328	o-Toluidine	o-Toluidine	95-53-4	INCIN; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN	INCIN; or Thermal Destruction	
U353	p-Toluidine	p-Toluidine	106-49-0	INCIN; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN	INCIN; or Thermal Destruction	
U359	2-Ethoxyethanol	2-Ethoxyethanol	110-80-5	INCIN; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN	CMBST	

1	The waste descriptions provided in this table do not replace waste descriptions in 40 CFR part 261.  Descriptions of Treatment/Regulatory Subcategories are provided, as needed, to distinguish between applicability of different standards.
2	CAS means Chemical Abstract Services.  When the waste code and/or regulated constituents are described as a combination of a chemical with its salts and/or esters, the CAS number is given for the parent compound only.
3	Concentration standards for wastewaters are expressed in mg/l are based on analysis of composite samples.
4	All treatment standards expressed as a Technology Code or combination of Technology Codes are explained in detail in 40 CFR 268.42, Table 1 - Technology Codes and Descriptions of Technology-Based Standards.
5	Except for Metals (EP or TCLP) and Cyanides (Total and Amenable) the nonwastewater treatment standards expressed as a concentration were established, in part, based upon incineration in units operated in accordance with the technical requirements of 40 CFR part 264, subpart O or part 265, subpart O, or based upon combustion in fuel substitution units operating in accordance with applicable technical requirements.  A facility may comply with these treatment standards according to provisions in 40 CFR 268.40(d).  All concentration standards for nonwastewaters are based on analysis of grab samples.
6	Where an alternate treatment standard or set of alternate standards has been indicated, a facility may comply with this alternate standard, but only for the Treatment/Regulatory Subcategory or physical form (i.e., wastewater and/or nonwastewater) specified for that alternate standard.
7	Both Cyanides (Total) and Cyanides (Amenable) for nonwastewaters are to be analyzed using Method 9010 or 9012, found in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods", EPA Publication SW-846, as incorporated by reference in 40 CFR 260.11, with a sample size of 10 grams and a distillation time of one hour and 15 minutes.

NOTE:  NA means not applicable.

*	*	*	*	*

	6. Section 268.42 is amended by revising the entry, "CMBST" in Table 1 to read as follows:

§ 268.42   Treatment standards expressed as specified technologies.

*	*	*	*	* 

Table 1. -- Technology Codes and Description of Technology-Based Standards

Technology 
code	Description of technology-based 
standards	
*          *          *          *          *          *          *          *          *		
CMBST	Combusion in incinerators, boilers, or industrial furnaces operated in accordance with the applicable requirements of 40 CFR part 264, subpart O; 40 CFR part 265, subpart O; or 40 CFR part 266, subpart H.	
*          *          *          *          *          *          *          *          *		

*	*	*	*	*

	7. Section 268.48 is amended by adding footnote 5 to the entry for Vanadium and revising the footnote to read as follows:

§ 268.48   Universal Treatment Standards.

*	*	*	*	*

	  § 268.48 Table UTS_Universal Treatment Standards 

*	*	*	*	*

	5 Vanadium and zinc are not "underlying hazardous constituents" in characteristic wastes, according to the definition at 268.2(i).

	8. Appendix X to part 268 is amended by revising Certification Statement B to read as follows:

Appendix X to Part 268_Recordkeeping, Notification, and/or Certification Requirements.

*	*	*	*	* 

Certification Statements

*	*	*	*	*

	B. I certify under penalty of law that I personally have examined and am familiar with the waste and that the lab pack does not contain any wastes identified at Appendix IV to part 268. I am aware that there are significant penalties for submitting a false certification including possibility of fine or imprisonment.

*	*	*	*	* 

[FR Doc. 94_32118 Filed 12_30_94; 8:45 am]
BILLING CODE 6560_50_P