Doc Init;
-
Vol. 59 No. 180 Monday, September 19, 1994  p 47982 (Rule)

40 CFR Parts 148, 260, 261, 264, 265, 266, 268 and 271

[FRL-5028-9]; RIN 2050-AD89

Land Disposal Restrictions Phase II-Universal Treatment Standards, and Treatment Standards for Organic Toxicity Characteristic Wastes and Newly Listed Wastes

AGENCY: Environmental Protection Agency (EPA).

ACTION: Final rule.

SUMMARY: As part of the Agency's Land Disposal Restrictions (LDR) program, EPA is today promulgating treatment standards for the newly identified organic toxicity characteristic (TC) wastes (except those managed in Clean Water Act (CWA) systems, CWA- equivalent systems, or Class I Safe Drinking Water Act (SDWA) injection wells), and for all newly listed coke by-product and chlorotoluene production wastes. The required treatment standards for these wastes must be met before they are land disposed. EPA is also requiring ignitable characteristic wastes with a high total organic carbon (TOC) content and toxic characteristic pesticide wastes, that are being disposed in Class I nonhazardous waste injection wells, to either be injected into a well that is subject to a no-migration determination, or be treated by the designated LDR treatment method. Promulgation of these treatment standards for the newly identified and listed wastes and promulgation of the dilution prohibitions for high TOC ignitables and pesticides fulfills requirements of a proposed consent decree between EPA and the Environmental Defense Fund, and a settlement agreement between EPA, the Hazardous Waste Treatment Council, and a number of environmental groups including the Natural Resources Defense Council.

	EPA is also making a major improvement in the Land Disposal Restrictions program in order to simplify and provide consistency in the requirements. EPA is establishing a single set of requirements, referred to as universal treatment standards, that apply to most hazardous wastes. EPA is also simplifying the Land Disposal Restrictions program by reducing paperwork for the regulated community, and improving guidance to make compliance easier. EPA is also publishing clarifying guidance regarding treatability variances, which largely restates previous Agency statements. Finally, EPA is modifying the hazardous waste recycling regulations which will allow streamlined regulatory decisions to be made regarding the regulation of certain types of recycling activities.

DATES:   Effective date: The final rule is effective on December 19, 1994. Section 266.100 and Appendix VIII are effective September 19, 1994.

	Applicability dates: For high TOC D001 (40 CFR 148.17) and halogenated pesticides wastes (40 CFR 148.17) disposed in Class I nonhazardous injection deep wells, the compliance date is September 19, 1995. For radioactive waste mixed with the newly listed or identified wastes, or soil and debris contaminated with such mixed wastes (40 CFR 268.38), the compliance date is September 19, 1996. Although the effective date of today's rule is December 19, 1994, facilities will be in compliance if they meet the universal treatment standards (UTS) before the 90-day period ends.

ADDRESSES: The official record for this rulemaking is identified as Docket Number F-94-CS2F-FFFFF, and is located in the EPA RCRA Docket, U.S. Environmental Protection Agency, Room 2616, 401 M Street, SW., Washington, DC 20460. The RCRA Docket is open from 9 am to 4 pm Monday through Friday, except for Federal holidays. The public must make an appointment to review docket materials by calling (202) 260-9327. The public may copy a maximum of 100 pages from any regulatory document at no cost. Additional copies cost $.15 per page. The mailing address is EPA RCRA Docket (5305), U.S. Environmental Protection Agency, 401 M Street, SW., Washington, DC 20460.

FOR FURTHER INFORMATION CONTACT: For general information, contact the RCRA Hotline at (800) 424-9346 (toll-free) or (703) 412-9810 locally. For technical information about mercury and radioactive mixed waste, contact Shaun McGarvey on (703) 308-8603; for technical information about lab packs and metal Universal Treatment Standards, contact Anita Cummings on (703) 308-8303; for technical information about organic Universal Treatment Standards, contact Lisa Jones on (703) 308-8451; for technical information about Toxicity Characteristic wastes, contact Mary Cunningham on (703) 308-8453; for technical information about petroleum refining wastes, contact Jose Labiosa on (703) 308-8464; for other information, contact Richard Kinch on (703) 308-8414; of the Waste Treatment Branch, Office of Solid Waste (5302W), U.S. Environmental Protection Agency, 401 M Street, SW., Washington, DC 20460, phone (703) 308-8434. For technical information on capacity analyses, contact Bengie Carroll of the Capacity Programs Branch, Office of Solid Waste (5302W), phone (703) 308-8440. For technical information on Hazardous Waste Recycling, contact Mitch Kidwell of the Regulation Development Branch, Office of Solid Waste (5304), phone (202) 260-8551.

>>>> Preamble has not been included in this file. <<<<

	For the reasons set out in the preamble, title 40, chapter I of the Code of Federal Regulations is amended as follows:

>>>> Part 148 has not been included because it is not required as part of a State's Hazardous Waste
Program. <<<<

PART 260-HAZARDOUS WASTE MANAGEMENT SYSTEM: GENERAL

	3. The authority citation for part 260 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921-6927, 6930, 6934, 6935, 6937, 6938, 6939, and 6974.

	4. In § 260.30, the introductory text and paragraph (b) are revised to read as follows:

§ 260.30   Variances from classification as a solid waste.

	In accordance with the standards and criteria in § 260.31 and the procedures in § 260.33, the Administrator may determine on a case-by-case basis that the following recycled materials are not solid wastes:

*	*	*	*	*

	(b) Materials that are reclaimed and then reused within the original production process in which they were generated; and

*	*	*	*	*

	5. In § 260.31, the introductory text of both paragraph (a) and (b), is revised to read as follows:

§ 260.31   Standards and criteria for variances from classification as a solid waste.

	(a) The Administrator may grant requests for a variance from classifying as a solid waste those materials that are accumulated speculatively without sufficient amounts being recycled if the applicant demonstrates that sufficient amounts of the material will be recycled or transferred for recycling in the following year. If a variance is granted, it is valid only for the following year, but can be renewed, on an annual basis, by filing a new application. The Administrator's decision will be based on the following criteria:

*	*	*	*	*

	(b) The Administrator may grant requests for a variance from classifying as a solid waste those materials that are reclaimed and then reused as feedstock within the original production process in which the materials were generated if the reclamation operation is an essential part of the production process. This determination will be based on the following criteria:

*	*	*	*	*
	6. In § 260.32, the introductory text is revised to read as follows:

§ 260.32   Variance to be classified as a boiler.

	In accordance with the standards and criteria in § 260.10 (definition of ``boiler''), and the procedures in § 260.33, the Administrator may determine on a case-by-case basis that certain enclosed devices using controlled flame combustion are boilers, even though they do not otherwise meet the definition of boiler contained in § 260.10, after considering the following criteria:

*	*	*	*	*

	7. § 260.33 is revised to read as follows:

§ 260.33   Procedures for variances from classification as a solid waste or to be classified as a boiler.

	The Administrator will use the following procedures in evaluating applications for variances from classification as a solid waste or applications to classify particular enclosed controlled flame combustion devices as boilers:

	(a) The applicant must apply to the Administrator for the variance. The application must address the relevant criteria contained in § 260.31 or § 260.32.

	(b) The Administrator will evaluate the application and issue a draft notice tentatively granting or denying the application. Notification of this tentative decision will be provided by newspaper advertisement or radio broadcast in the locality where the recycler is located. The Administrator will accept comment on the tentative decision for 30 days, and may also hold a public hearing upon request or at his discretion. The Administrator will issue a final decision after receipt of comments and after the hearing (if any).

PART 261-IDENTIFICATION AND LISTING OF HAZARDOUS WASTE

	8. The authority citation for Part 261 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921, 6922, and 6938.

	9. Section 261.2 is amended by revising paragraph (e)(1)(iii) to read as follows:

§ 261.2   Definition of solid waste.

*	*	*	*	*

	(e) * * *

	(1) * * *

	(iii) Returned to the original process from which they are generated, without first being reclaimed or land disposed. The material must be returned as a substitute for feedstock materials. In cases where the original process to which the material is returned is a secondary process, the materials must be managed such that there is no placement on the land.

*	*	*	*	*

PART 264-STANDARDS FOR OWNERS AND OPERATORS OF HAZARDOUS WASTE TREATMENT, STORAGE, AND DISPOSAL FACILITIES

	10. The authority citation for Part 264 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6924, and 6925.

	11. In § 264.1, paragraph (g)(6) is revised to read as follows:

§ 264.1   Purpose, scope and applicability.

*	*	*	*	*

	(g) * * *

	(6) The owner or operator of an elementary neutralization unit or a wastewater treatment unit as defined in § 260.10 of this chapter, provided that if the owner or operator is diluting hazardous ignitable (D001) wastes (other than the D001 High TOC Subcategory defined in § 268.40 of this chapter, Table Treatment Standards for Hazardous Wastes), or reactive (D003) waste, to remove the characteristic before land disposal, the owner/operator must comply with the requirements set out in § 264.17(b).

*	*	*	*	*

PART 265-INTERIM STATUS STANDARDS FOR OWNERS AND OPERATORS OF HAZARDOUS WASTE TREATMENT, STORAGE, AND DISPOSAL FACILITIES

	12. The authority citation for part 265 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6924, 6925, 6935, and 6936.

	13. In § 265.1, paragraph (c)(10) is revised to read as follows:

§ 265.1   Purpose, scope, and applicability.

*	*	*	*	*

	(c) * * *

	(10) The owner or operator of an elementary neutralization unit or a wastewater treatment unit as defined in § 260.10 of this chapter, provided that if the owner or operator is diluting hazardous ignitable (D001) wastes (other than the D001 High TOC Subcategory defined in § 268.40 of this chapter, Table Treatment Standards for Hazardous Wastes), or reactive (D003) waste, to remove the characteristic before land disposal, the owner/operator must comply with the requirements set out in § 265.17(b).

*	*	*	*	*

PART 266-STANDARDS FOR THE MANAGEMENT OF SPECIFIC HAZARDOUS WASTES AND SPECIFIC TYPES OF HAZARDOUS WASTE MANAGEMENT FACILITIES

	14. The authority citation for part 266 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6924, and 6934.

Subpart C-Recyclable Materials Used in a Manner Constituting Disposal

	15. In § 266.23, paragraph (a) is revised to read as follows:

§ 266.23   Standards applicable to users of materials that are used in a manner that constitutes disposal.

	(a) Owners or operators of facilities that use recyclable materials in a manner that constitutes disposal are regulated under all applicable provisions of subparts A through N of parts 124, 264, 265, 268, and 270 of this chapter and the notification requirement under section 3010 of RCRA. (These requirements do not apply to products which contain these recyclable materials under the provisions of § 266.20(b) of this chapter.)

*	*	*	*	*

Subpart H-Hazardous Waste Burned in Boilers and Industrial Furnaces

	16. In § 266.100, the introductory text in paragraphs (c)(1), (c)(3), (c)(3)(i), and (c)(3)(ii); and paragraph (c)(3)(i)(A) are revised to read as follows:

§ 266.100   Applicability

*	*	*	*	*
	(c) * * *

	(1) To be exempt from §§ 266.102 through 266.111, an owner or operator of a metal recovery furnace or mercury recovery furnace, must comply with the following requirements, except that an owner or operator of a lead or a nickel-chromium recovery furnace, or a metal recovery furnace that burns baghouse bags used to capture metallic dusts emitted by steel manufacturing, must comply with the requirements of paragraph (c)(3) of this section:

*	*	*	*	*

	(3) To be exempt from §§ 266.102 through 266.111, an owner or operator of a lead or nickel-chromium or mercury recovery furnace, or a metal recovery furnace that burns baghouse bags used to capture metallic dusts emitted by steel manufacturing, must provide a one-time written notice to the Director identifying each hazardous waste burned and specifying whether the owner or operator claims an exemption for each waste under this paragraph or paragraph (c)(1) of this section. The owner or operator must comply with the requirements of paragraph (c)(1) of this section for those wastes claimed to be exempt under that paragraph and must comply with the requirements below for those wastes claimed to be exempt under this paragraph (c)(3).

	(i) The hazardous wastes listed in appendices XI, XII, and XIII, part 266, and baghouse bags used to capture metallic dusts emitted by steel manufacturing are exempt from the requirements of paragraph (c)(1) of this section, provided that:

	(A) A waste listed in appendix IX of this part must contain recoverable levels of lead, a waste listed in appendix XII of this part must contain recoverable levels of nickel or chromium, a waste listed in appendix XIII of this part must contain recoverable levels of mercury and contain less than 500 ppm of 40 CFR part 261, appendix VIII organic constituents, and baghouse bags used to capture metallic dusts emitted by steel manufacturing must contain recoverable levels of metal; and

*	*	*	*	*

	(ii) The Director may decide on a case-by-case basis that the toxic organic constituents in a material listed in appendix XI, XII, or XIII of this part that contains a total concentration of more than 500 ppm toxic organic compounds listed in appendix VIII, part 261 of this chapter, may pose a hazard to human health and the environment when burned in a metal recovery furnace exempt from the requirements of this subpart. In that situation, after adequate notice and opportunity for comment, the metal recovery furnace will become subject to the requirements of this subpart when burning that material. In making the hazard determination, the Director will consider the following factors:

*	*	*	*	*

Appendix XIII to Part 266 [Added]

	17. Appendix XIII is added to read as follows:

Appendix XIII to Part 266-Mercury Bearing Wastes That May Be Processed in Exempt Mercury Recovery Units

	These are exempt mercury-bearing materials with less than 500 ppm of 40 CFR Part 261, appendix VIII organic constituents when generated by manufacturers or users of mercury or mercury products.

1. Activated carbon
2. Decomposer graphite
3. Wood
4. Paper
5. Protective clothing
6. Sweepings
7. Respiratory cartridge filters
8. Cleanup articles
9. Plastic bags and other contaminated containers
10. Laboratory and process control samples
11. K106 and other wastewater treatment plant sludge and filter cake
12. Mercury cell sump and tank sludge
13. Mercury cell process solids
14. Recoverable levels or mercury contained in soil

PART 268-LAND DISPOSAL RESTRICTIONS

	18. The authority citation for Part 268 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921, and 6924.

Subpart A-General

	19. In § 268.1, paragraphs (c)(3)(ii), (e)(4), and (e)(5) are revised, and paragraph (c)(3)(iii) is added, to read as follows:

§ 268.1  Purpose, scope and applicability.

*	*	*	*	*

	(c) * * *

	(3) * * *

	(ii) Do not exhibit any prohibited characteristic of hazardous waste at the point of injection; and

	(iii) If at the point of generation the injected wastes include D001 High TOC subcategory wastes or D012-D017 pesticide wastes that are prohibited under § 148.17(c) of this chapter, those wastes have been treated to meet the treatment standards of § 268.40 before injection.

*	*	*	*	*

	(e) * * *

	(4) De minimis losses to wastewater treatment systems of commercial chemical product or chemical intermediates that are ignitable (D001), corrosive (D002), or are organic constituents that exhibit the characteristic of toxicity (D012-D043), and that contain underlying hazardous constituents as defined in § 268.2(i), are not considered to be prohibited wastes. De minimis is defined as losses from normal material handling operations (e.g. spills from the unloading or transfer of materials from bins or other containers, leaks from pipes, valves or other devices used to transfer materials); minor leaks of process equipment, storage tanks or containers; leaks from well-maintained pump packings and seals; sample purgings; and relief device discharges; discharges from safety showers and rinsing and cleaning of personal safety equipment; and rinsate from empty containers or from containers that are rendered empty by that rinsing; or

	(5) Land disposal prohibitions for hazardous characteristic wastes do not apply to laboratory wastes displaying the characteristic of ignitability (D001), corrosivity (D002), or organic toxicity (D012-D043), that are mixed with other plant wastewaters at facilities whose ultimate discharge is subject to regulation under the CWA (including wastewaters at facilities which have eliminated the discharge of wastewater), provided that the annualized flow of laboratory wastewater into the facility's headworks does not exceed one per cent, or provided that the laboratory wastes' combined annualized average concentration does not exceed one part per million in the facility's headworks.

	20. In § 268.2, paragraphs (g) and (i) are revised to read as follows:

§ 268.2  Definitions applicable in this part.

*	*	*	*	*

	(g) "Debris" means solid material exceeding a 60 mm particle size that is intended for disposal and that is: A manufactured object; or plant or animal matter; or natural geologic material. However, the following materials are not debris: Any material for which a specific treatment standard is provided in Subpart D, Part 268, namely lead acid batteries, cadmium batteries, and radioactive lead solids; Process residuals such as smelter slag and residues from the treatment of waste, wastewater, sludges, or air emission residues; and Intact containers of hazardous waste that are not ruptured and that retain at least 75% of their original volume. A mixture of debris that has not been treated to the standards provided by § 268.45 and other material is subject to regulation as debris if the mixture is comprised primarily of debris, by volume, based on visual inspection.

*	*	*	*	*

	(i) "Underlying hazardous constituent" means any constituent listed in § 268.48, Table UTS-Universal Treatment Standards, except zinc, which can reasonably be expected to be present at the point of generation of the hazardous waste, at a concentration above the constituent-specific UTS treatment standard.

	21. Section 268.7 is amended by revising paragraphs (a) and (b)(4)(ii), and by adding paragraph (b)(5)(iv) to read as follows:

§ 268.7   Waste analysis and recordkeeping.

	(a) Except as specified in § 268.32, if a generator's waste is listed in 40 CFR part 261, subpart D, the generator must test his waste, or test an extract using test method 1311 (the Toxicity Characteristic Leaching Procedure, described in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods," EPA Publication SW-846 as incorporated by reference in § 260.11 of this chapter), or use knowledge of the waste, to determine if the waste is restricted from land disposal under this part. Except as specified in § 268.32, if a generator's waste exhibits one or more of the characteristics set out at 40 CFR part 261, subpart C, the generator must test an extract using test method 1311 (the Toxicity Characteristic Leaching Procedure, described in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods" (SW-846)), or use knowledge of the waste, to determine if the waste is restricted from land disposal under this Part. If the generator determines that his waste exhibits the characteristic of ignitability (D001) (and is not in the High TOC Ignitable Liquids Subcategory or is not treated by CMBST or RORGS of § 268.42, Table 1), or the characteristic of corrosivity (D002), and is prohibited under § 268.37; and/or the characteristic of organic toxicity (D012-D043), and is prohibited under § 268.38, the generator must determine the underlying hazardous constituents (as defined in § 268.2, in the D001, D002, or D012-D043 wastes.

	(1) If a generator determines that he is managing a restricted waste under this part and the waste does not meet the applicable treatment standards set forth in Subpart D of this part or exceeds the applicable prohibition levels set forth in § 268.32 or RCRA section 3004(d), with each shipment of waste the generator must notify the treatment or storage facility in writing of the appropriate treatment standards set forth in Subpart D of this part and any applicable prohibition levels set forth in § 268.32 or RCRA section 3004(d). The notice must include the following information:

	(i) EPA Hazardous Waste Number;

	(ii) The waste constituents that the treater will monitor, if monitoring will not include all regulated constituents, for wastes F001-F005, F039, D001, D002, and D012-D043. Generators must also include whether the waste is a nonwastewater or wastewater (as defined in § 268.2(d) and (f), and indicate the subcategory of the waste (such as "D003 reactive cyanide"), if applicable;

	(iii) The manifest number associated with the shipment of waste;

	(iv) For hazardous debris when using the alternative treatment technologies provided by § 268.45:

	(A) The contaminants subject to treatment, as described in § 268.45(b); and

	(B) An indication that these contaminants are being treated to comply with § 268.45.

	(v) For hazardous debris when using the treatment standards for the contaminating waste(s) in § 268.40: the requirements described in paragraphs (a)(1) (i), (ii), (iii), and (vi) of this section.

	(2) If a generator determines that he is managing a restricted waste under this Part, and determines that the waste can be land disposed without further treatment, with each shipment of waste he must submit, to the treatment, storage, or land disposal facility, a notice and a certification stating that the waste meets the applicable treatment standards set forth in subpart D of this part and the applicable prohibition levels set forth in § 268.32 or RCRA section 3004(d). Generators of hazardous debris that is excluded from the definition of hazardous waste under § 261.3(e)(2) of this chapter (i.e., debris that the Director has determined does not contain hazardous waste), however, are not subject to these notification and certification requirements.

	(i) The notice must include the following information:

	(A) EPA Hazardous Waste Number;

	(B) The waste constituents that the treater will monitor, if monitoring will not include all regulated constituents, for wastes F001-F005, F039, D001, D002, and D012-D043. Generators must also include whether the waste is a nonwastewater or wastewater (as defined in § 268.2 (d) and (f)), and indicate the subcategory of the waste (such as "D003 reactive cyanide"), if applicable;

	(C) The manifest number associated with the shipment of waste;

	(D) Waste analysis data, where available.

	(ii) The certification must be signed by an authorized representative and must state the following:

	I certify under penalty of law that I personally have examined and am familiar with the waste through analysis and testing or through knowledge of the waste to support this certification that the waste complies with the treatment standards specified in 40 CFR Part 268 Subpart D and all applicable prohibitions set forth in 40 CFR 268.32 or RCRA section 3004(d). I believe that the information I submitted is true, accurate and complete. I am aware that there are significant penalties for submitting a false certification, including the possibility of a fine and imprisonment.

	(3) If a generator's waste is subject to an exemption from a prohibition on the type of land disposal method utilized for the waste (such as, but not limited to, a case-by-case extension under § 268.5, an exemption under § 268.6, or a nationwide capacity variance under subpart C of this part), with each shipment of waste he must submit a notice to the facility receiving his waste stating that the waste is not prohibited from land disposal. The notice must include the following information:

	(i) EPA Hazardous Waste Number;

	(ii) The waste constituents that the treater will monitor, if monitoring will not include all regulated constituents, for wastes F001-F005, F039, D001, D002, and D012-D043. Generators must also include whether the waste is a nonwastewater or wastewater (as defined in § 268.2 (d) and (f)), and indicate the subcategory of the waste (such as "D003 reactive cyanide"), if applicable;

	(iii) The manifest number associated with the shipment of waste;

	(iv) Waste analysis data, where available;

	(v) For hazardous debris when using the alternative treatment technologies provided by § 268.45:

	(A) The contaminants subject to treatment, as described in § 268.45(b); and

	(B) An indication that these contaminants are being treated to comply with § 268.45.
	(vi) For hazardous debris when using the treatment standards for the contaminating waste(s) in § 268.40: the requirements described in paragraphs (a)(1) (i), (ii), (iii), and (vi) of this section.

	(4) If a generator is managing prohibited waste in tanks, containers, or containment buildings regulated under 40 CFR 262.34, and is treating such waste in such tanks, containers, or containment buildings to meet applicable treatment standards under subpart D of this part, the generator must develop and follow a written waste analysis plan which describes the procedures the generator will carry out to comply with the treatment standards. (Generators treating hazardous debris under the alternative treatment standards of Table 1, § 268.45, however, are not subject to these waste analysis requirements.) The plan must be kept on site in the generator's records, and the following requirements must be met:

	(i) The waste analysis plan must be based on a detailed chemical and physical analysis of a representative sample of the prohibited waste(s) being treated, and contain all information necessary to treat the waste(s) in accordance with the requirements of this Part, including the selected testing frequency.

	(ii) Such plan must be filed with the EPA Regional Administrator (or his designated representative) or State authorized to implement Part 268 requirements a minimum of 30 days prior to the treatment activity, with delivery verified.

	(iii) Wastes shipped off-site pursuant to this paragraph must comply with the notification requirements of § 268.7(a)(2).

	(5) If a generator determines whether the waste is restricted based solely on his knowledge of the waste, all supporting data used to make this determination must be retained on-site in the generator's files. If a generator determines whether the waste is restricted based on testing this waste or an extract developed using the test method described in Appendix I of this part, all waste analysis data must be retained on-site in the generator's files.

	(6) If a generator determines that he is managing a restricted waste that is excluded from the definition of hazardous or solid waste or exempt from Subtitle C regulation, under 40 CFR 261.2 through 261.6 subsequent to the point of generation, he must place a one-time notice stating such generation, subsequent exclusion from the definition of hazardous or solid waste or exemption from RCRA Subtitle C regulation, and the disposition of the waste, in the facility's file.

	(7) Generators must retain on-site a copy of all notices, certifications, demonstrations, waste analysis data, and other documentation produced pursuant to this section for at least five years from the date that the waste that is the subject of such documentation was last sent to on-site or off-site treatment, storage, or disposal. The five year record retention period is automatically extended during the course of any unresolved enforcement action regarding the regulated activity or as requested by the Administrator. The requirements of this paragraph apply to solid wastes even when the hazardous characteristic is removed prior to disposal, or when the waste is excluded from the definition of hazardous or solid waste under 40 CFR 261.2 through 261.6, or exempted from RCRA Subtitle C regulation, subsequent to the point of generation.

	(8) If a generator is managing a lab pack waste and wishes to use the alternative treatment standard under § 268.42(c), with each shipment of waste the generator must submit a notice to the treatment facility in accordance with paragraph (a)(1) of this section, except that underlying hazardous constituents need not be determined. The generator must also comply with the requirements in paragraphs (a)(5) and (a)(6) of this section and must submit the following certification, which must be signed by an authorized representative:

	I certify under penalty of law that I personally have examined and am familiar with the waste and that the lab pack contains only wastes which have not been excluded under appendix IV to 40 CFR part 268 or solid wastes not subject to regulation under 40 CFR part 261. I am aware that there are significant penalties for submitting a false certification, including the possibility of fine or imprisonment.

	(9) [Reserved]

	(10) Small quantity generators with tolling agreements pursuant to 40 CFR 262.20(e) must comply with the applicable notification and certification requirements of paragraph (a) of this section for the initial shipment of the waste subject to the agreement. Such generators must retain on-site a copy of the notification and certification, together with the tolling agreement, for at least three years after termination or expiration of the agreement. The three-year record retention period is automatically extended during the course of any unresolved enforcement action regarding the regulated activity or as requested by the Administrator.

	(b) * * *

	(4) * * *

	(ii) The waste constituents to be monitored, if monitoring will not include all regulated constituents, for wastes F001-F005, F039, D001, D002, and D012-D043. Generators must also include whether the waste is a nonwastewater or wastewater (as defined in § 268.2 (d) and (f), and indicate the subcategory of the waste (such as D003 reactive cyanide), if applicable.

*	*	*	*	*

	(5) * * *

	(iv) For characteristic wastes D001, D002, and D012-D043 that are: subject to the treatment standards in § 268.40 (other than those expressed as a required method of treatment); that are reasonably expected to contain underlying hazardous constituents as defined in § 268.2(i); are treated on-site to remove the hazardous characteristic; and are then sent off-site for treatment of underlying hazardous constituents, the certification must state the following:

	I certify under penalty of law that the waste has been treated in accordance with the requirements of 40 CFR 268.40 to remove the hazardous characteristic. This decharacterized waste contains underlying hazardous constituents that require further treatment to meet universal treatment standards. I am aware that there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment.

*	*	*	*	*

	22. In § 268.9, paragraph (a), (d)(1)(i), and (d)(1)(ii) are revised, (d)(1)(iii) is removed and (d)(2) (i) and (ii) are added to read as follows:

§ 268.9   Special rules regarding wastes that exhibit a characteristic.

	(a) The initial generator of a solid waste must determine each EPA Hazardous Waste Number (waste code) applicable to the waste in order to determine the applicable treatment standards under subpart D of this part. For purposes of part 268, the waste will carry the waste code for any applicable listing under 40 CFR part 261, subpart D. In addition, the waste will carry one or more of the waste codes under 40 CFR part 261, subpart C, where the waste exhibits a characteristic, except in the case when the treatment standard for the waste code listed in 40 CFR part 261, subpart D operates in lieu of the treatment standard for the waste code under 40 CFR part 261, subpart C, as specified in paragraph (b) of this section. If the generator determines that his waste displays the characteristic of ignitability (D001) (and is not in the High TOC Ignitable Liquids Subcategory or is not treated by CMBST, or RORGS), or the waste code listed in 40 CFR part 261, subpart D operates in lieu of the treatment standard for the waste code under 40 CFR part 261, subpart C, as specified in paragraph (b) of this section. If the generator determines that his waste displays the characteristic of ignitability (D001) (and is not in the High TOC Ignitable Liquids Subcategory or is not treated by CMBST, or RORGS), or the characteristic of corrosivity (D002), and is prohibited under § 268.37; or that his waste displays the characteristic of toxicity (D012-D043), and is prohibited under § 268.38, the generator must determine the underlying hazardous constituents (as defined in § 268.2), in the D001, D002, or D012-D043 wastes.

*	*	*	*	*

	(d) * * *

	(1) * * *

	(i) Name and address of the RCRA Subtitle D facility receiving the waste shipment; and

	(ii) A description of the waste as initially generated, including the applicable EPA Hazardous Waste Number(s), treatability group(s), and underlying hazardous constituents (as defined in § 268.2(i) in D001 and D002 wastes prohibited under § 268.37, or D012-D043 wastes under § 268.38.

	(2) * * *

	(i) If treatment removes the characteristic but does not treat underlying hazardous constituents, then the certification found in § 268.7 (b)(5)(v) apply.

	(ii) [Reserved]

Subpart C-Prohibitions on Land Disposal

	23. In subpart C, § 268.38 is added to read as follows:

§ 268.38   Waste specific prohibitions-newly identified organic toxicity characteristic wastes and newly listed coke by-product and chlorotoluene production wastes.

	(a) Effective December 19, 1994, the wastes specified in 40 CFR 261.32 as EPA Hazardous Waste numbers K141, K142, K143, K144, K145, K147, K148, K149, K150, and K151 are prohibited from land disposal. In addition, debris contaminated with EPA Hazardous Waste numbers F037, F038, K107-K112, K117, K118, K123-K126, K131, K132, K136, U328, U353, U359, and soil and debris contaminated with D012-D043, K141-K145, and K147-K151 are prohibited from land disposal. The following wastes that are specified in 40 CFR 261.24, Table 1 as EPA Hazardous Waste numbers: D012, D013, D014, D015, D016, D017, D018, D019, D020, D021, D022, D023, D024, D025, D026, D027, D028, D029, D030, D031, D032, D033, D034, D035, D036, D037, D038, D039, D040, D041, D042, D043 that are not radioactive, or that are managed in systems other than those whose discharge is regulated under the Clean Water Act (CWA), or that are zero dischargers that do not engage in CWA-equivalent treatment before ultimate land disposal, or that are injected in Class I deep wells regulated under the Safe Drinking Water Act (SDWA), are prohibited from land disposal. CWA-equivalent treatment means biological treatment for organics, alkaline chlorination or ferrous sulfate precipitation for cyanide, precipitation/ sedimentation for metals, reduction of hexavalent chromium, or other treatment technology that can be demonstrated to perform equally or better than these technologies.

	(b) On September 19, 1996, radioactive wastes that are mixed with D018-D043 that are managed in systems other than those whose discharge is regulated under the Clean Water Act (CWA), or that inject in Class I deep wells regulated under the Safe Drinking Water Act (SDWA), or that are zero dischargers that engage in CWA-equivalent treatment before ultimate land disposal, are prohibited from land disposal. CWA-equivalent treatment means biological treatment for organics, alkaline chlorination or ferrous sulfate precipitation for cyanide, precipitation/ sedimentation for metals, reduction of hexavalent chromium, or other treatment technology that can be demonstrated to perform equally or greater than these technologies. Radioactive wastes mixed with K141-K145, and K147-K151 are also prohibited from land disposal. In addition, soil and debris contaminated with these radioactive mixed wastes are prohibited from land disposal.

	(c) Between December 19, 1994 and September 19, 1996, the wastes included in paragraphs (b) of this section may be disposed in a landfill or surface impoundment, only if such unit is in compliance with the requirements specified in § 268.5(h)(2) of this Part.

	(d) The requirements of paragraphs (a), (b), and (c) of this section do not apply if:

	(1) The wastes meet the applicable treatment standards specified in Subpart D of this part;

	(2) Persons have been granted an exemption from a prohibition pursuant to a petition under § 268.6, with respect to those wastes and units covered by the petition;

	(3) The wastes meet the applicable alternate treatment standards established pursuant to a petition granted under § 268.44;

	(4) Persons have been granted an extension to the effective date of a prohibition pursuant to § 268.5, with respect to these wastes covered by the extension.

	(e) To determine whether a hazardous waste identified in this section exceeds the applicable treatment standards specified in § 268.40, the initial generator must test a sample of the waste extract or the entire waste, depending on whether the treatment standards are expressed as concentrations in the waste extract or the waste, or the generator may use knowledge of the waste. If the waste contains constituents in excess of the applicable Subpart D levels, the waste is prohibited from land disposal, and all requirements of part 268 are applicable, except as otherwise specified.

Subpart D-Treatment Standards

	24. Section 268.40 is revised to read as follows:

§ 268.40   Applicability of Treatment Standards.

	(a) A waste identified in the table "Treatment Standards for Hazardous Wastes" may be land disposed only if it meets the requirements found in the table. For each waste, the table identifies one of three types of treatment standard requirements:

	(1) All hazardous constituents in the waste or in the treatment residue must be at or below the values found in the table for that waste ("total waste standards"); or

	(2) The hazardous constituents in the extract of the waste or in the extract of the treatment residue must be at or below the values found in the table ("waste extract standards"); or

	(3) The waste must be treated using the technology specified in the table ("technology standard"), which are described in detail in § 268.42, Table 1-Technology Codes and Description of Technology-Based Standards.

	(b) For wastewaters, compliance with concentration level standards is based on maximums for any one day, except for D004 through D011 wastes for which the previously promulgated treatment standards based on grab samples remain in effect. For all nonwastewaters, compliance with concentration level standards is based on grab sampling. For wastes covered by the waste extract standards, the test Method 1311, the Toxicity Characteristic Leaching Procedure found in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods", EPA Publication SW-846, as incorporated by reference in § 260.11, must be used to measure compliance. An exception is made for D004 and D008, for which either of two test methods may be used: Method 1311, or Method 1310, the Extraction Procedure Toxicity Test. For wastes covered by a technology standard, the wastes may be land disposed after being treated using that specified technology or an equivalent treatment technology approved by the Administrator under the procedures set forth in § 268.42(b).

	(c) When wastes with differing treatment standards for a constituent of concern are combined for purposes of treatment, the treatment residue must meet the lowest treatment standard for the constituent of concern.

	(d) Notwithstanding the prohibitions specified in paragraph (a) of this section, treatment and disposal facilities may demonstrate (and certify pursuant to 40 CFR 268.7(b)(5)) compliance with the treatment standards for organic constituents specified by a footnote in the table "Treatment Standards for Hazardous Wastes" in this section, provided the following conditions are satisfied:

	(1) The treatment standards for the organic constituents were established based on incineration in units operated in accordance with the technical requirements of 40 CFR part 264, subpart O, or based on combustion in fuel substitution units operating in accordance with applicable technical requirements;

	(2) The treatment or disposal facility has used the methods referenced in paragraph (d)(1) of this section to treat the organic constituents; and

	(3) The treatment or disposal facility may demonstrate compliance with organic constituents if good-faith analytical efforts achieve detection limits for the regulated organic constituents that do not exceed the treatment standards specified in this section by an order of magnitude.

	(e) For characteristic wastes (D001, D002, and D012-D043 that are subject to treatment standards in the following table "Treatment Standards for Hazardous Wastes," all underlying hazardous constituents (as defined in § 268.2(i)) must meet Universal Treatment Standards, found in § 268.48, Table UTS, prior to land disposal.

	(f) The treatment standards for F001-F005 nonwastewater constituents carbon disulfide, cyclohexanone, and/or methanol apply to wastes which contain only one, two, or three of these constituents. Compliance is measured for these constituents in the waste extract from test Method 1311, the Toxicity Characteristic Leaching Procedure found in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods", EPA Publication SW-846, as incorporated by reference in § 260.11. If the waste contains any of these three constituents along with any of the other 25 constituents found in F001-F005, then compliance with treatment standards for carbon disulfide, cyclohexanone, and/or methanol are not required.

Treatment Standards for Hazardous Wastes

	Note: The treatment standards that heretofore appeared in tables in §§ 268.41, 268.42, and 268.43 of this part have been consolidated into the table "Treatment Standards for Hazardous Wastes" in this section.

TREATMENT STANDARDS FOR HAZARDOUS WASTES						
Waste Code	Waste Description and Treatment/Regulatory Subcategory1	REGULATED HAZARDOUS CONSTITUENT		WASTEWATERS	NONWASTEWATERS	
		Common Name	CAS2 Number	Concentration mg/l3; or Technology Code4	Concentration in mg/kg3 unless noted as "mg/l TCLP"; or Technology Code	
D001	Ignitable Characteristic Wastes, except for the § 261.21(a)(1) High TOC Subcategory, that are managed in non-CWA/non-CWA-equivalent/non-Class I SDWA systems.	NA	NA	DEACT and meet § 268.48 standards; or RORGS; or CMBST	DEACT and meet § 268.48 standards; or RORGS; or CMBST	
	Ignitable Characteristic Wastes, except for the § 261.21(a)(1) High TOC Subcategory, that are managed in CWA/CWA-equivalent/Class I SDWA systems	NA	NA	DEACT	DEACT	
	High TOC Ignitable Characteristic Liquids Subcategory based on 40 CFR 261.21(a)(1) - Greater than or equal to 10% total organic carbon.
(Note:  This subcategory consists of nonwastewaters only.)	NA	NA	NA	RORGS; or CMBST	
D002	Corrosive Characteristic Wastes that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems.	NA	NA	DEACT
and meet § 268.48 standards	DEACT
and meet § 268.48 standards	
D002, D004, D005, D006, D007, D008, D009, D010, D011	Radioactive high level wastes generated during the reprocessing of fuel rods.
(Note:  This subcategory consists of nonwastewaters only.)	Corrosivity (pH)	NA	NA	HLVIT	
		Arsenic	7440-38-2	NA	HLVIT	
		Barium	7440-39-3	NA	HLVIT	
		Cadmium	7440-43-9	NA	HLVIT	
		Chromium (Total)	7440-47-3	NA	HLVIT	
		Lead	7439-92-1	NA	HLVIT	
		Mercury	7439-87-6	NA	HLVIT	
		Selenium	7782-49-2	NA	HLVIT	
		Silver	7440-22-4	NA	HLVIT	
D003	Reactive Sulfides Subcategory based on 261.23(a)(5).	NA	NA	DEACT	DEACT	
	Explosive subcategory based on 261.23(a)(6), (7), and (8).	NA	NA	DEACT	DEACT	
	Other Reactives Subcategory based on 261.23(a)(1).	NA	NA	DEACT	DEACT	
	Water Reactive Subcategory based on 261.23(a)(2), (3), and (4).
(Note:  This subcategory consists of nonwastewaters only.)	NA	NA	NA	DEACT	
	Reactive Cyanides Subcategory based on 261.23(a)(5).	Cyanides (Total)7	57-12-5	Reserved	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
D004	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for arsenic based on the extraction procedure (EP) in SW846 Method 1310.	Arsenic	7440-38-2	5.0	5.0 mg/l EP	
		Arsenic; alternate6 standard for nonwastewaters only.	7440-38-2	NA	5.0 mg/l TCLP	
D005	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for barium based on the extraction procedure (EP) in SW846 Method 1310.	Barium	7440-39-3	100	100 mg/l TCLP	
D006	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for cadmium based on the extraction procedure (EP) in SW846 Method 1310.	Cadmium	7440-43-9	1.0	1.0 mg/l TCLP	
	Cadmium Containing Batteries Subcategory
(Note:  This subcategory consists of nonwastewaters only.)	Cadmium	7440-43-9	NA	RTHRM	
D007	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for chromium based on the extraction procedure (EP) in SW846 Metod 1310.	Chromium (Total)	7440-47-3	5.0	5.0 mg/l TCLP	
D008	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for lead based on the extraction procedure (EP) in SW846 Method 1310.	Lead	7439-92-1	5.0	5.0 mg/l EP	
		Lead; alternate6 standard for nonwastewaters only	7439-92-1	NA	5.0 mg/l TCLP	
	Lead Acid Batteries Subcategory (Note:  This standard only applies to lead acid batteries that are identified as RCRA hazardous wastes and that are not excluded elsewhere from regulation under the land disposal restrictions of 40 CFR 268 or exempted under other EPA regulations (see 40 CFR 266.80).).
(Note:  This subcategory consists of nonwastewaters only.)	Lead	7439-92-1	NA	RLEAD	
	Radioactive Lead Solids Subcategory (Note:  These lead solids include, but are not limited to, all forms of lead shielding and other elemental forms of lead.  These lead solids do not include treatment residuals such as hydroxide sludges, other wastewater treatment residuals, or incinerator ashes that can undergo conventional pozzolanic stabilization, nor do they include organo-lead materials that can be incinerated and stabilized as ash.).
(Note:  This subcategory consists of nonwastewaters only.)	Lead	7439-92-1	NA	MACRO	
D009	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain greater than or equal to 260 mg/kg total mercury that also contain organics and are not incinerator residues.
(High Mercury-Organic Subcategory)	Mercury	7439-97-6	NA	IMERC; OR RMERC	
	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain greater than or equal to 260 mg/kg total mercury that are inorganic, including incinerator residues and residues from RMERC.
(High Mercury-Inorganic Subcategory)	Mercury	7439-97-6	NA	RMERC	
	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain less than 260 mg/kg total mercury.
(Low Mercury Subcategory)	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	All D009 wastewaters.	Mercury	7439-97-6	0.20	NA	
	Elemental mercury contaminated with radioactive materials.
(Note:  This subcategory consists of nonwastewaters only.)	Mercury	7439-97-6	NA	AMLGM	
	Hydraulic oil contaminated with Mercury Radioactive Materials Subcategory.
(Note:  This subcategory consists of nonwastewaters only.)	Mercury	7439-97-6	NA	IMERC	
D010	Wastes that exhibit, or are expected to exhibit, the characteristic or toxicity for selenium based on the extraction procedure (EP) in SW846 Method 1310.	Selenium	7782-49-2	1.0	5.7 mg/l TCLP	
D011	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for silver based on the extraction procedure (EP) in SW846 Method 1310.	Silver	7440-22-4	5.0	5.0 mg/l TCLP	
D012	Wastes that are TC for Endrin based on the TCLP in SW846 Method 1311.	Endrin	72-20-8	BIODG; or INCIN	0.13
and meet § 268.48 standards	
		Endrin aldehyde	7421-93-4	BIODG; or INCIN	0.13
and meet § 268.48 standards	
D013	Wastes that are TC for Lindane based on the TCLP in SW846 Method 1311.	alpha-BHC	319-84-6	CARBN; or INCIN	0.066
and meet § 268.48 standards	
		beta-BHC	319-85-7	CARBN; or INCIN	0.066
and meet § 268.48 standards	
		delta-BHC	319-86-8	CARBN; or INCIN	0.066
and meet § 268.48 standards	
		gamma-BHC (Lindane)	58-89-9	CARBN; or INCIN	0.066
and meet § 268.48 standards	
D014	Wastes that are TC for Methoxychlor based on the TCLP in SW846 Method 1311.	Methoxychlor	72-43-5	WETOX or INCIN	0.18
and meet § 268.48 standards	
D015	Wastes that are TC for Toxaphene based on the TCLP in SW846 Method 1311.	Toxaphene	8001-35-2	BIODG or INCIN	2.6
and meet § 268.48 standards	
D016	Wastes that are TC for 2,4-D (2,4-Dichlorophenoxyacetic acid) based on the TCLP in SW846 Method 1311.	2,4-D (2,4-Dichlorophenoxyacetic acid)	94-75-7	CHOXD, BIODG, or INCIN	10
and meet § 268.48 standards	
D017	Wastes that are TC for 2,4,5-TP (Silvex) based on the TCLP in SW846 Method 1311.	2,4,5-TP (Silvex)	93-72-1	CHOXD or INCIN	7.9
and meet § 268.48 standards	
D018	Wastes that are TC for Benzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Benzene	71-43-2	0.14	10
and meet § 268.48 standards	
D019	Wastes that are TC for Carbon tetrachloride based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Carbon tetrachloride	56-23-5	0.057	6.0
and meet § 268.48 standards	
D020	Wastes that are TC for Chlordane based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26
and meet § 268.48 standards	
D021	Wastes that are TC for Chlorobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Chlorobenzene	108-90-7	0.057	6.0
and meet § 268.48 standards	
D022	Wastes that are TC for Chloroform based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Chloroform	67-66-3	0.046	6.0
and meet § 268.48 standards	
D023	Wastes that are TC for o-Cresol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	o-Cresol	95-48-7	0.11	5.6
and meet § 268.48 standards	
D024	Wastes that are TC for m-Cresol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6
and meet § 268.48 standards	
D025	Wastes that are TC for p-Cresol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6
and meet § 268.48 standards	
D026	Wastes that are TC for Cresols (Total) based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations)	1319-77-3	0.88	11.2
and meet § 268.48 standards	
D027	Wastes that are TC for p-Dichlorobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	p-Dichlorobenzene (1,4-Dichlorobenzene)	106-46-7	0.090	6.0
and meet § 268.48 standards	
D028	Wastes that are TC for 1,2-Dichloroethane based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	1,2-Dichloroethane	107-06-2	0.21	6.0
and meet § 268.48 standards	
D029	Wastes that are TC for 1,1-Dichloroethylene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	1,1-Dichloroethylene	75-35-4	0.025	6.0
and meet § 268.48 standards	
D030	Wastes that are TC for 2,4-Dinitrotoluene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	2,4-Dinitrotoluene	121-14-2	0.32	140
and meet § 268.48 standards	
D031	Wastes that are TC for Heptachlor based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Heptachlor	76-44-8	0.0012	0.066
and meet § 268.48 standards	
		Heptachlor epoxide	1024-57-3	0.016	0.066
and meet § 268.48 standards	
D032	Wastes that are TC for Hexachlorobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Hexachlorobenzene	118-74-1	0.055	10
and meet § 268.48 standards	
D033	Wastes that are TC for Hexachlorobutadiene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Hexachlorobutadiene	67-68-3	0.055	5.6
and meet § 268.48 standards	
D034	Wastes that are TC for Hexachloroethane based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Hexachloroethane	67-72-1	0.055	30
and meet § 268.48 standards	
D035	Wastes that are TC for Methyl ethyl ketone based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Methyl ethyl ketone	78-93-3	0.28	36
and meet § 268.48 standards	
D036	Wastes that are TC for Nitrobenzene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Nitrobenzene	98-95-3	0.068	14
and meet § 268.48 standards	
D037	Wastes that are TC for Pentachlorophenol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Pentachlorophenol	87-86-5	0.089	7.4
and meet § 268.48 standards	
D038	Wastes that are TC for Pyridine based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Pyridine	110-86-1	0.014	16
and meet § 268.48 standards	
D039	Wastes that are TC for Tetrachloroethylene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Tetrachloroethylene	127-18-4	0.056	6.0
and meet § 268.48 standards	
D040	Wastes that are TC for Trichloroethylene based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Trichloroethylene	79-01-6	0.054	6.0
and meet § 268.48 standards	
D041	Wastes that are TC for 2,4,5-Trichlorophenol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	2,4,5-Trichlorophenol	95-95-4	0.18	7.4
and meet § 268.48 standards	
D042	Wastes that are TC for 2,4,6-Trichlorophenol based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	2,4,6-Trichlorophenol	88-06-2	0.035	7.4
and meet § 268.48 standards	
D043	Wastes that are TC for Vinyl chloride based on the TCLP in SW846 Method 1311 and that are managed in non-CWA/non-CWA equivalent/non-Class I SDWA systems only.	Vinyl chloride	75-01-4	0.27	6.0
and meet § 268.48 standards	
F001, F002, F003, F004, & F005	F001, F002, F003, F004 and/or F005 solvent wastes that contain any combination of one or more of the following spent solvents:  acetone, benzene, n-butyl alcohol, carbon disulfide, carbon tetrachloride, chlorinated fluorocarbons, chlorobenzene, o-cresol, m-cresol, p-cresol, cyclohexanone, o-dichlorobenzene, 2-ethoxyethanol, ethyl acetate, ethyl benzene, ethyl ether, isobutyl alcohol, methanol, methylene chloride, methyl ethyl ketone, methyl isobutyl ketone, nitrobenzene, 2-nitropropane, pyridine, tetrachloroethylene, toluene, 1,1,1-trichloroethane, 1,1,2-trichloroethane, 1,1,2-trichloro- 1,2,2-trifluoroethane, trichloroethylene, trichloromonofluoromethane, and/or xylenes (except as specifically noted in other subcategories).  See further details of these listings in § 261.31	Acetone	67-64-1	0.28	160	
		Benzene	71-43-2	?0.14	10	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Carbon disulfide	75-15-0	3.8	NA	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chlorobenzene	108-90-7	0.057	6.0	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations)	1319-77-3	0.88	11.2	
		Cyclohexanone	108-94-1	0.36	NA	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		Ethyl acetate	141-7-6	0.34	33	
		Ethyl benzene	100-41-4	0.057	10	
		Ethyl ether	60-29-7	0.12	160	
		Isobutyl alcohol	78-83-1	5.6	170	
		Methanol	67-56-1	5.6	NA	
		Methylene chloride	75-9-2	0.089	30	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Nitrobenzene	98-95-3	0.068	14	
		Pyridine	110-86-1	0.014	16	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		Toluene	108-88-3	0.080	10	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		1,1,2-Trichloro-1,2,2-trifluoroethane	76-13-1	0.057	30	
		Trichloroethylene	79-01-6	0.054	6.0	
		Trichloromonofluoromethane	75-69-4	0.020	30	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
	F003 and/or F005 solvent wastes that contain any combination of one or more of the following three solvents as the only listed F001-5 solvents:  carbon disulfide, cyclohexanone, and/or methanol.  (formerly 268.41(c))	Carbon disulfide	75-15-0	3.8	4.8 mg/l TCLP	
		Cyclohexanone	108-94-1	0.36	0.75 mg/l TCLP	
		Methanol	67-56-1	5.6	0.75 mg/l TCLP	
	F005 solvent waste containing 2-Nitropropane as the only listed F001-5 solvent.	2-Nitropropane	79-46-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
	F005 solvent waste containing 2-Ethoxyethanol as the only listed F001-5 solvent.	2-Ethoxyethanol	110-80-5	BIODG; or INCIN	INCIN	
F006	Wastewater treatment sludges from electroplating operations except from the following processes:  (1) Sulfuric acid anodizing of aluminum; (2) tin plating on carbon steel; (3) zinc plating (segregated basis) on carbon steel; (4) aluminum or zinc-aluminum plating on carbon steel; (5) cleaning/stripping associated with tin, zinc and aluminum plating on carbon steel; and (6) chemical etching and milling of aluminum.	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F007	Spent cyanide plating bath solutions from electroplating operations.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F008	Plating bath residues from the bottom of plating baths from electroplating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F009	Spent stripping and cleaning bath solutions from electroplating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F010	Quenching bath residues from oil baths from metal heat treating operations where cyanides are used in the process.	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.88	NA	
F011	Spent cyanide solutions from salt bath pot cleaning from metal heat treating operations.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F012	Quenching wastewater treatment sludges from metal heat treating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F019	Wastewater treatment sludges from the chemical conversion coating of aluminum except from zirconium phosphating in aluminum can washing when such phosphating is an exclusive conversion coating process.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
F020, F021, F022, F023, F026	Wastes (except wastewater and spent carbon from hydrogen chloride purification) from the production or manufacturing use (as a reactant, chemical intermediate, or component in a formulating process) of:  (1) tri- or tetrachlorophenol, or of intermediates used to produce their pesticide derivatives, excluding wastes from the production of Hexachlorophene from highly purified 2,4,5-trichlorophenol (F020); (2) pentachlorophenol, or of intermediates used to produce its derivatives (i.e., F021); (3) tetra-, penta-, or hexachlorobenzenes under alkaline conditions (i.e., F022).
Wastes (except wastewater and spent carbon from hydrogen chloride purification) from the production of materials on equipment previously used for the production or manufacturing use (as a reactant, chemical intermediate, or component in a formulating process) of:  (1) tri- or tetrachlorophenols, excluding wastes from equipment used only for the production of Hexachlorophene from highly purified 2,4,5-trichlorophenol (F023); (2) tetra-, penta-, or hexachlorobenzenes under alkaline conditions (i.e., F026).	HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
F027	Discarded unused formulations contianing tri-, tetra-, or pentachlorophenol or discarded unused formulations containing compounds derived from these chlorophenols.  (This listing does not include formulations containing hexachlorophene synthesized from prepurified 2,4,5-trichlorophenol as the sole component.).	HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
F028	Residues resulting from the incineration or thermal treatment of soil contaminated with EPA Hazardous Wastes Nos. F020, F021, F023, F026, and F027.	HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
F024	Process wastes, including but not limited to, distillation residues, heavy ends, tars, and reactor clean-out wastes, from the production of certain chlorinated aliphatic hydrocarbons by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.  (This listing does not include wastewaters, wastewater treatment sludges, spent catalysts, and wastes listed in § 261.31 or § 261.32.).	All F024 wastes	NA	INCIN	INCIN	
		2-Chloro-1,3-butadiene	126-99-8	0.057	0.28	
		3-Chloropropylene	107-05-1	0.036	30	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,2-Dichloropropane	78-87-5	0.85	18	
		cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Hexachloroethane	67-72-1	0.055	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
F026	Condensed light ends from the production of certain chlorinated aliphatic hydrocarbons, by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.
F025 - Light Ends Subcategory	Carbon tetrachloride	56-23-6	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		Methylene chloride	75-9-2	0.089	30	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
	Spent filters and filter aids, and spent desiccant wastes from the production of certain chlorinated aliphatic hydrocarbons, by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.
F026 - Spent Filters/Aids and Desiccants Subcategory	Carbon tetrachloride	56-23-5	0.067	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Methylene chloride	75-9-2	0.089	30	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
F037	Petroleum refinery primary oil/water/solids separation sludge-Any sludge generated from the gravitational separation of oil/water/solids during the storage or treatment of process wastewaters and oily cooling wastewaters from petroleum refineries.  Such sludges include, but are not limited to, those generated in:  oil/water/solids separators; tanks and impoundments; ditches and other conveyances; sumps; and stormwater units receiving dry weather flow.  Sludge generated in stormwater units that do not receive dry weather flow, sludges generated from non-contact once-through cooling waters segregated for treatment from other process or oily cooling waters, sludges generated in agressive biological treatment units as defined in § 261.31(b)(2) (including sludges generated in one or more additional units after wastewaters have been treated in agressive biological treatment units) and K051 wastes are not included in this listing.	Acenaphthene	83-32-9	0.059	NA	
		Anthracene	120-12-7	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	.032	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
F038	Petroleum refinery secondary (emulsified) oil/water/solids separation sludge and/or float generated from the physical and/or chemical separation of oil/water/solids in process wastewaters and oily cooling wastewaters from petroleum refineries.  Such wastes include, but are not limited to, all sludges and floats generated in:  induced air floatation (IAF) units, tanks and impoundments, and all sludges generated in DAF units.  Sludges generated in stormwater units that do not receive dry weather flow, sludges generated from non-contact once-through cooling waters segregated for treatment from other process or oily cooling waters, sludges and floats generated in agressive biological treatment units as defined in § 261.31(b)(2) (including sludges and floats generated in one or more additional units after wastewaters have been treated in agressive biological units) and F037, K048, and K051 are not included in this listing.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
F039	Leachate (liquids that have percolated through land disposed wastes) resulting from the disposal of more than one restricted waste classified as hazardous under subpart D of this part.  (Leachate resulting from the disposal of one or more of the following EPA Hazardous Wastes and no other Hazardous Wastes retains its EPA Hazardous Waste Number(s):  F020, F021, F022, F026, F027, and/or F028.).	Acenaphthylene	208-96-8	0.059	3.4	
		Acenaphthene	83-32-9	0.059	3.4	
		Acetone	67-64-1	0.28	160	
		Acetonitrile	75-05-8	5.6	NA	
		Acetophenone	96-86-2	0.010	9.7	
		2-Acetylaminofluorene	53-96-3	0.059	140	
		Acrolein	107-02-8	0.29	NA	
		Acrylonitrile	107-13-1	0.24	84	
		Aldrin	309-00-2	0.021	0.066	
		4-Aminobiphenyl	92-67-1	0.13	NA	
		Aniline	62-53-3	0.81	14	
		Anthracene	120-12-7	0.059	3.4	
		Aramite	140-57-8	0.36	NA	
		alpha-BHC	319-84-6	0.00014	0.066	
		beta-BHC	319-85-7	0.00014	0.066	
		delta-BHC	319-86-8	0.023	0.066	
		gamma-BHC	58-89-9	0.0017	0.066	
		Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Benzo(g,h,i)perylene	191-24-2	0.0055	1.8	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Bromodichloromethane	75-27-4	0.35	15	
		Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		4-Bromophenyl phenyl ether	101-55-3	0.055	15	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Butyl benzyl phthalate	85-68-7	0.017	28	
		2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	88-85-7	0.066	2.5	
		Carbon disulfide	75-15-0	3.8	NA	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		p-Chloroaniline	106-47-8	0.46	16	
		Chlorobenzene	108-90-7	0.057	6.0	
		Chlorobenzilate	510-15-6	0.10	NA	
		2-Chloro-1,3-butadiene	126-99-8	0.057	NA	
		Chlorodibromomethane	124-48-1	0.057	15	
		Chloroethane	75-00-3	0.27	6.0	
		bis(2-Chloroethoxy)methane	111-91-1	0.036	7.2	
		bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		Chloroform	67-66-3	0.046	6.0	
		bis(2-Chloroisopropyl)ehter	108-60-1	0.055	7.2	
		p-Chloro-m-cresol	59-50-7	0.018	14	
		Chloromethane (Methyl chloride)	74-87-3	0.19	30	
		2-Chloronaphthalene	91-58-7	0.055	5.6	
		2-Chlorophenol	95-57-8	0.044	5.7	
		3-Chloropropylene	107-05-1	0.036	30	
		Chrysene	218-01-9	0.059	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Cyclohexanone	108-94-1	0.36	NA	
		1,2-Dibromo-3-chloropropane	96-12-8	0.11	15	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
		Dibromomethane	74-95-3	0.11	15	
		2,4-D (2,4-Dichlorophenoxyacetic acid)	94-75-7	0.72	10	
		o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
		o,p'-DDE	3424-82-6	0.031	0.087	
		p,p'-DDE	72-55-9	0.031	0.087	
		o,p'-DDT	789-02-6	0.0039	0.087	
		p,p'-DDT	50-29-3	0.0039	0.087	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Dibenz(a,e)pyrene	192-65-4	0.061	NA	
		m-Dichlorobenzene	541-73-1	0.036	6.0	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Dichlorodifluoromethane	75-71-8	0.23	7.2	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		trans-1,2-Dichloroethylene	156-60-5	0.054	30	
		2,4-Dichlorophenol	120-83-2	0.044	14	
		2,6-Dichlorophenol	87-65-0	0.044	14	
		1,2-Dichloropropane	78-87-5	0.85	18	
		cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
		Dieldrin	60-57-1	0.017	0.13	
		Diethyl phthalate	84-66-2	0.20	28	
		2-4-Dimethyl phenol	105-67-9	0.036	14	
		Dimethyl phthalate	131-11-3	0.047	28	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		1,4-Dinitrobenzene	100-25-4	0.32	2.3	
		4,6-Dinitro-o-cresol	534-52-1	0.28	160	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		2,4-Dinitrotoluene	121-14-2	0.32	140	
		2,6-Dinitrotoluene	606-20-2	0.55	28	
		Di-n-octyl phthalate	117-84-0	0.017	28	
		Di-n-propylnitrosamine	621-64-7	0.40	14	
		1,4-Dioxane	123-91-1	NA	170	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine)	122-39-4	0.92	NA	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine)	86-30-6	0.92	NA	
		1,2-Diphenylhydrazine	122-66-7	0.087	NA	
		Disulfoton	298-04-4	0.017	6.2	
		Endosulfan I	939-98-8	0.023	0.066	
		Endosulfan II	33213-6-5	0.029	0.13	
		Endosulfan sulfate	1-31-07-8	0.029	0.13	
		Endrin	72-20-8	0.0028	0.13	
		Endrin aldehyde	7421-93-4	0.025	0.13	
		Ethyl acetate	141-78-6	0.34	33	
		Ethyl cyanide (Propanenitrile)	107-12-0	0.24	360	
		Ethyl benzene	100-41-4	0.057	10	
		Ethyl ether	60-29-7	0.12	160	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Ethyl methacrylate	97-63-2	0.14	160	
		Ethylene oxide	75-21-8	0.12	NA	
		Famphur	52-85-7	0.017	15	
		Fluoranthene	206-44-0	0.068	3.4	
		Fluorene	86-73-7	0.059	3.4	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		Hexachloroethane	67-72-1	0.055	30	
		Hexachloropropylene	1888-71-7	0.035	30	
		Indeno (1,2,3-c,d) pyrene	193-39-5	0.0055	3.4	
		Iodomethane	74-88-4	0.19	65	
		Isobutyl alcohol	78-83-1	5.6	170	
		Isodrin	465-73-6	0.021	0.066	
		Isosafrole	120-58-1	0.081	2.6	
		Kepone	143-50-8	0.0011	0.13	
		Methacrylonitrile	126-98-7	0.24	84	
		Methanol	67-56-1	5.6	NA	
		Methapyrilene	91-80-5	0.081	1.5	
		Methoxychlor	72-43-5	0.25	0.18	
		3-Methylcholanthrene	56-49-5	0.0055	15	
		4,4-Methylene bis(2-chloroaniline)	101-14-4	0.50	30	
		Methylene chloride	75-09-2	0.089	30	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Methyl methacrylate	80-62-6	0.14	160	
		Methyl methansulfonate	66-27-3	0.018	NA	
		Methyl parathion	298-00-0	0.014	4.6	
		Naphthalene	91-20-3	0.059	5.6	
		2-Naphthylamine	91-59-8	0.52	NA	
		p-Nitroaniline	100-01-6	0.028	28	
		Nitrobenzene	98-95-3	0.068	14	
		5-Nitro-o-toluidine	99-55-8	0.32	28	
		p-Nitrophenol	100-02-7	0.12	29	
		N-Nitrosodiethylamine	55-18-5	0.40	28	
		N-Nitrosodimethylamine	62-75-9	0.40	NA	
		N-Nitroso-di-n-butylamine	924-16-3	0.40	17	
		N-Nitrosomethylethylamine	10595-95-6	0.40	2.3	
		N-Nitrosomorpholine	59-89-2	0.40	2.3	
		N-Nitrosopiperidine	100-75-4	0.013	35	
		N-Nitrosopyrrolidine	930-55-2	0.013	35	
		Parathion	56-38-2	0.014	4.6	
		Total PCBs
(sum of all PCB isomers, or all Aroclors)	1336-36-3	0.10	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PcCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		Pentachloronitrobenzene	82-68-8	0.055	4.8	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenacetin	62-44-2	0.081	16	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Phorate	298-02-2	0.021	4.6	
		Phthalic anhydride	85-44-9	0.055	NA	
		Pronamide	23950-58-5	0.093	1.5	
		Pyrene	129-00-0	0.067	8.2	
		Pyridine	110-86-1	0.014	16	
		Safrole	94-59-7	0.081	22	
		Silvex (2,4,5-TP)	93-72-1	0.72	7.9	
		2,4,5-T	93-76-5	0.72	7.9	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Toluene	108-88-3	0.080	10	
		Toxaphene	8001-35-2	0.0095	2.6	
		Bromoform (Tribromomethane)	75-25-2	0.63	15	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Trichloromonofluoromethane	75-69-4	0.020	30	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		1,2,3-Trichloropropane	96-18-4	0.85	30	
		1,1,2-Trichloro-1,2,2-trifluoroethane	76-13-1	0.057	30	
		tris(2,3-Dibromopropyl) phosphate	126-72-7	0.11	NA	
		Vinyl chloride	75-01-4	0.27	6.0	
		Xylenes-mixed isomers
(sum or o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Antimony	7440-36-0	1.9	2.1 mg/l TCLP	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Barium	7440-39-3	1.2	7.6 mg/l TCLP	
		Beryllium	7440-41-7	0.82	NA	
		Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	NA	
		Fluoride	16964-48-8	35	NA	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Mercury	7439-97-6	0.15	0.025 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
		Sulfide	8496-25-8	14	NA	
		Thallium	7440-28-0	1.4	NA	
		Vanadium	7440-62-2	4.3	NA	
K001	Bottom sediment sludge from the treatment of wastewaters from wood preserving processes that use creosote and/or pentachlorophenol.	Naphthalene	91-20-3	0.059	5.6	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenanthrene	85-01-8	0.059	5.6	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K002	Wastewater treatment sludge from the production of chrome yellow and orange pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K003	Wastewater treatment sludge from the production of molybdate orange pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K004	Wastewater treatment sludge from the production of zinc yellow pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K005	Wastewater treatment sludge from the production of chrome green pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
K006	Wastewater treatment sludge from the production of chrome oxide green pigments (anhydrous).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
	Wastewater treatment sludge from the production of chrome oxide green pigments (hydrated).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
K007	Wastewater treatment sludge from the production of iron blue pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
K008	Oven residue from the production of chrome oxide green pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K009	Distillation bottoms from the production of acetaldehyde from ethylene.	Chloroform	67-66-3	0.046	6.0	
K010	Distillation side cuts from the production of acetaldehyde from ethylene.	Chloroform	67-66-3	0.046	6.0	
K011	Bottom stream from the wastewater stripper in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	18	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K013	Bottom stream from the acetonitrile column in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	1.8	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K014	Bottoms from the acetonitrile purification column in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	1.8	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K015	Still bottoms from the distillation of benzyl chloride.	Anthracene	120-12-7	0.059	3.4	
		Benzal chloride	98-87-3	0.055	6.0	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Phenanthrene	85-01-8	0.059	5.6	
		Toluene	108-88-3	0.080	10	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K016	Heavy ends or distillation residues from the production of carbon tetrachloride.	Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		Hexachloroethane	67-72-1	0.055	30	
		Tetrachloroethylene	127-18-4	0.056	6.0	
K017	Heavy ends (still bottoms) from the purification column in the production of epichlorohydrin.	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		1,2-Dichloropropane	78-87-5	0.85	18	
		1,2,3-Trichloropropane	96-18-4	0.85	30	
K018	Heavy ends from the fractionation column in ethyl chloride production.	Chloroethane	75-00-3	0.27	6.0	
		Chloromethane	74-87-3	0.19	NA	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	NA	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K019	Heavy ends from the distillation of ethylene dichloride in ethylene dichloride production.	bis(2-Chloroethyl)ether	111-44-1	0.033	6.0	
		Chlorobenzene	108-90-7	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		p-Dichlorobenzene	106-46-7	0.090	NA	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		Fluorene	86-73-7	0.059	NA	
		Hexachloroethane	67-72-1	0.055	30	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	NA	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K020	Heavy ends from the distillation of vinyl chloride in vinyl chloride monomer production.	1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
K021	Aqueous spent antimony catalyst waste from fluoromethanes production.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Antimony	7440-36-0	1.9	2.1 mg/l TCLP	
K022	Distillation bottom tars from the production of phenol/acetone from cumene.	Toluene	108-88-3	0.080	10	
		Acetophenone	96-86-2	0.010	9.7	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine)	22-39-4	0.92	13	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine)	86-30-6	0.92	13	
		Phenol	108-95-2	0.039	6.2	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	0.98	5.0 mg/l TCLP	
K023	Distillation light ends from the production of phthalic anhydride from naphthalene.	Phthalic anhydride (measured as Phthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride	85-44-9	0.055	28	
K024	Distillation bottoms from the production of phthalic anhydride from naphthalene.	Phthalic anhydride (measured as Phthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride	85-44-9	0.055	28	
K025	Distillation bottoms from the production of nitrobenzene by the nitration of benzene.	NA	NA	LLEXT fb SSTRP fb CARBN; or INCIN	INCIN	
K026	Stripping still tails from the production of methyl ethyl pyridines.	NA	NA	INCIN	INCIN	
K027	Centrifuge and distillation residues from the toluene diisocyanate production.	NA	NA	CARBN; or INCIN	CMBST	
K028	Spent catalyst from the hydrochlorinator reactor in the production of 1,1,1-trichloroethane.	1,1-Dichloroethane	76-34-3	0.059	6.0	
		trans-1,2-Dichloroethylene	156-60-5	0.054	30	
		Hexachlorobutadiene	87-88-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	NA	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Cadmium	7440-43-9	0.69	NA	
		Chromium(Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K029	Waste from the product steam stripper in the production of 1,1,1-trichloroethane.	Chloroform	67-66-3	0.046	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
K030	Column bodies or heavy ends from the combined production of trichloroethylene and perchloroethylene.	o-Dichlorobenzene	95-50-1	0.088	NA	
		p-Dichlorobenzene	106-46-7	0.090	NA	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Hexachloropropylene	1888-71-7	NA	30	
		Pentachlorobenzene	608-93-5	NA	10	
		Pentachloroethane	76-01-7	NA	6.0	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K031	By-product salts generated in the production of MSMA and cacodylic acid.	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
K032	Wastewater treatment sludge from the production of chlordane.	Hexachlorocyclopentadiene	77-48-4	0.057	2.4	
		Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
K033	Wastewater and scrub water from the chlorination of cyclopentadiene in the production of chlordane.	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
K034	Filter solids from the filtration of hexachlorocyclopentadiene in the production of chlordane.	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
K035	Wastewater treatment sludges generated in the production of creosote.	Acenaphthene	83-32-9	NA	3.4	
		Anthracene	120-12-7	NA	3.4	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Chrysene	218-01-9	0.059	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Dibenz(a,h)anthracene	53-70-3	NA	8.2	
		Fluoranthene	206-44-0	0.068	3.4	
		Fluorene	86-73-7	NA	3.4	
		Indeno(1,2,3-cd)pyrene	193-39-5	NA	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
K036	Still bottoms from toluene reclamation distillaiton in the production of disulfoton.	Disulfoton	298-04-4	0.017	6.2	
K037	Wastewater treatment sludges from the production of disulfoton.	Disulfoton	298-04-4	0.017	6.2	
		Toluene	108-88-3	0.080	10	
K038	Wastewater from the washing and stripping of phorate production.	Phorate	298-02-2	0.021	4.6	
K039	Filter cake from the filtration of diethylphosphorodithioc acid in the production of phorate.	NA	NA	CARBN; or INCIN	CMBST	
K040	Wastewater treatment sludge from the production of phorate.	Phorate	298-02-2	0.021	4.6	
K041	Wastewater treatment sludge from the production of toxaphene.	Toxaphene	8001-35-2	0.0095	2.6	
K042	Heavy ends or distillation residues from the distillation of tetrachlorobenzene in the production of 2,4,5-T.	o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K043	2,6-Dichlorophenol waste from the production of 2,4-D.	2,4-Dichlorophenol	120-83-2	0.044	14	
		2,6-Dichlorophenol	187-65-0	0.044	14	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Tetrachloroethylene	79-01-6	0.056	6.0	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
K044	Wastewater treatment sludges from the manufacturing and processing of explosives.	NA	NA	DEACT	DEACT	
K045	Spent carbon from the treatment of wastewater containing explosives.	NA	NA	DEACT	DEACT	
K046	Wastewater treatment sludges from the manufacturing, formulation and loading of lead-based initiating compounds.	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K047	Pink/red water from TNT operations.	NA	NA	DEACT	DEACT	
K048	Dissolved air flotation (DAF) float from the petroleum refining industry.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-33	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K049	Slop oil emulsion solids from the petroleum refining industry.	Anthracene	120-12-7	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Carbon disulfide	75-15-0	3.8	NA	
		Chrysene	2218-01-9	0.059	3.4	
		2,4-Dimethylphenol	105-67-9	0.036	NA	
		Ethylbenzene	100-41-4	0.057	10	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-. and p-xylene concentrations)	1330-20-7	0.32	30	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K050	Heat exchanger bundle cleaning sludge from the petroleum refining industry.	Benzo(a)pyrene	50-32-8	0.061	3.4	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K051	API separator sludge from the petroleum refining industry.	Acenaphthene	83-32-9	0.059	NA	
		Anthracene	120-12-7	0.059	3.4	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	2218-01-9	0.059	3.4	
		Di-n-butyl phthalate	105-67-9	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	106-88-3	0.08	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K052	Tank bottoms (leaded) from the petroleum refining industry.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		2,4-Dimethylphenol	105-67-9	0.036	NA	
		Ethylbenzene	100-41-4	0.057	10	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Toluene	108-88-3	0.08	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K060	Ammonia still lime sludge from coking operations.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
K061	Emission control dust/sludge from the primary production of steel in electric furnaces.	Antimony	7440-36-0	NA	2.1 mg/l TCLP	
		Arsenic	7440-38-2	NA	5.0 mg/l TCLP	
		Barium	7440-39-3	NA	7.6 mg/l TCLP	
		Beryllium	7440-41-7	NA	0.014 mg/l TCLP	
		Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Mercury	7439-97-6	NA	0.025 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Selenium	7782-49-2	NA	0.16 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
		Thallium	NA	NA	0.078 mg/l TCLP	
		Zinc	7440-66-6	NA	5.3 mg/l TCLP	
K062	Spent pickle liquor generated by steel finishing operations of facilities within the iron and steel industry (SIC Codes 331 and 332).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	NA	
K069	Emission control dust/sludge from secondary lead smelting. - Calcium sulfate (Low Lead) Subcategory	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
	Emission control dust/sludge from secondary lead smelting. - Non-Calcium sulfate (High Lead) Subcategory	NA	NA	NA	RLEAD	
K071	K071 (Brine purification muds from the mercury cell process in chlorine production, where separately prepurified brine is not used) nonwastewaters that are residues from RMERC.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	K071 (Brine purification muds from the mercury cell process in chlorine production, where separately prepurified brine is not used) nonwastewaters that are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All K071 wastewaters.	Mercury	7439-97-6	0.15	NA	
K073	Chlorinated hydrocarbon waste from the purification step of the diaphragm cell process using graphite anodes in chlorine production.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachloroethane	67-72-1	0.055	30	
		Tetrachloroethylene	127-18-4	0.058	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K083	Distillation bottoms from aniline production.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		Cyclohexanone	108-94-1	0.36	NA	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine)	22-39-4	0.92	13	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine)	86-30-6	0.92	13	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K084	Wastewater treatment sludges generated during the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
K085	Distillation or fractionation column bottoms from the production of chlorobenzenes.	Benzene	71-43-2	0.14	10	
		Chlorobenzene	108-90-7	0.057	6.0	
		m-Dichlorobenzene	541-73-1	0.036	6.0	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Total PCBs
(sum of all PCB isomers, or all Aroclors)	1336-36-3	0.10	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K086	Solvent wastes and sludges, caustic washes and sludges, or water washes and sludges from cleaning tubs and equipment used in the formulation of ink from pigments, driers, soaps, and stabilizers containing chromium and lead.	Acetone	67-64-1	0.28	160	
		Acetophenone	96-86-2	0.010	9.7	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Butylbenzyl phthalate	85-68-7	0.017	28	
		Cyclohexanone	108-94-1	0.36	NA	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		Diethyl phthalate	84-66-2	0.20	28	
		Dimethyl phthalate	131-11-3	0.047	28	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Di-n-octyl phthalate	117-84-0	0.017	28	
		Ethyl acetate	141-78-6	0.34	33	
		Ethylbenzene	100-41-4	0.057	10	
		Methanol	67-56-1	5.6	NA	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Methylene chloride	75-09-2	0.089	30	
		Naphthalene	91-20-3	0.059	5.6	
		Nitrobenzene	98-95-3	0.068	14	
		Toluene	108-88-3	0.080	10	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K087	Decanter tank tar sludge from coking operations.	Acenaphthylene	208-96-8	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Chrysene	218-01-9	0.059	3.4	
		Fluoranthene	206-44-0	0.068	3.4	
		Indenol(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K093	Distillation light ends from the production of phthalic anhydride from ortho-xylene.	Phthalic anhydride (measured as Phthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride	85-44-9	0.055	28	
K094	Distillation bottoms from the production of phthalic anhydride from ortho-xylene.	Phthalic anhydride (measured as Phthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride	85-44-9	0.055	28	
K095	Distillation bottoms from the production of 1,1,1-trichloroethane.	Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	0.055	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
K096	Heavy ends from the heavy ends column from the production of 1,1,1-trichloroethane.	m-Dichlorobenzene	541-73-1	0.036	6.0	
		Pentachloroethane	76-01-7	0.055	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
K097	Vacuum stripper discharge from the chlordane chlorinator in the production of chlordane.	Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.068	
		Hexachlorcyclopentadiene	77-47-4	0.057	2.4	
K098	Untreated process wastewater from the production of toxaphene.	Toxaphene	8001-35-2	0.0095	2.6	
K099	Untreated wastewater from the production of 2,4-D.	2,4-Dichlorophenoxyacetic acid	94-75-7	0.72	10	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
K100	Waste leaching solution from acid leaching of emission control dust/sludge from secondary lead smelting.	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K101	Distillation tar residues from the distillation of aniline-based compounds in the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	o-Nitroaniline	88-74-4	0.27	14	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Cadmium	7440-43-9	0.69	NA	
		Lead	7439-92-1	0.69	NA	
		Mercury	7439-97-6	0.15	NA	
K102	Residue from the use of activated carbon f--decolorization in the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	o-Nitrophenol	88-75-5	0.028	13	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Cadmium	7440-43-9	0.69	NA	
		Lead	7439-92-1	0.69	NA	
		Mercury	7439-97-6	0.15	NA	
K103	Process residues from aniline extraction from the production of aniline.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
K104	Combined wastewater streams generated from nitrobenzene/aniline production.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
K105	Separated aqueous stream from the reactor product washing step in the production of chlorobenzenes.	Benzene	71-43-2	0.14	10	
		Chlorobenzene	108-90-7	0.057	6.0	
		2-Chlorophenol	95-57-8	0.044	5.7	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Phenol	108-95-2	0.039	6.2	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
K106	K106 (wastewater treatment sludge from the mercury cell process in chlorine production) nonwastewaters that contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	K106 (wastewater treatment sludge from the mercury cell process in chlorine production) nonwastewaters that contain less than 260 mg/kg total mercury that are residues from RMERC.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	Other K106 nonwastewaters that contain less than 260 mg/kg total mercury and are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All K106 wastewaters.	Mercury	7439-97-6	0.15	NA	
K107	Column bottoms from product separation from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K108	Condensed column overheads from product separation and condensed reactor vent gases from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K109	Spent filter cartridges from product purification from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K110	Condensed column overheads from intermediate separation from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K111	Product washwaters from the production of dinitrotoluene via nitration of toluene	2,4-Dinitrotoluene	121-1-1	0.32	140	
		2,6-Dinitrotoluene	606-20-2	0.55	28	
K112	Reaction by-product water from the drying column in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	INCIN; or CHOXD fb CARBN; or BIODG fb CARBN	INCIN	
K113	Condensed liquid light ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	CARBN; or INCIN	CMBST	
K114	Vicinals from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	CARBN; or INCIN	CMBST	
K115	Heavy ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		NA	NA	CARBN; or INCIN	CMBST	
K116	Organic condensate from the solvent recovery column in the production of toluene diisocyanate via phosgenation of toluenediamine.	NA	NA	CARBN; or INCIN	CMBST	
K117	Wastewater from the reactor vent gas scrubber in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K118	Spent absorbent solids from purification of ethylene dibromide in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K123	Process wastewater (including supernates, filtrates, and washwaters) from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K124	Reactor vent scrubber water from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K125	Filtration, evaporation, and centrifugation solids from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K126	Baghouse dust and floor sweepings in milling and pachaging operations from the production or formulation of ethylenebisdithiocarbamic acid and its salts.	NA	NA	INCIN; or CHOXD fb (BIODG or CARBN)	INCIN	
K131	Wastewater from the reactor and spent sulfuric acid from the acid dryer from the production of methyl bromide.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
K132	Spent absorbent and wastewater separator solids from the production of methyl bromide.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
K136	Still bottoms from the purification of ethylene dibromide in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K141	Process residues from the recovery of coal tar, including, but not limited to, collecting sump residues from the production of coke or the recovery of coke by-products produced from coal.  This listing does not include K087 (decanter tank tar sludge from coking operations).	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-2-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K142	Tar storage tank residues from the production of coke from coal or from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Ideno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K143	Process residues from the recovery of light oil, including, but not limited to, those generated in stills, decanters, and wash oil recovery units from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
K144	Wastewater sump residues from light oil refining, including, but not limited to, intercepting or contamination sump sludges from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
K145	Residues from naphthalene collection and recovery operations from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	6.2	
		Naphthalene	91-20-3	0.059	5.6	
K147	Tar storage tank residues from coal tar refining.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K148	Residues from coal tar distillation, including, but not limited to, still bottoms.	Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K149	Distillation bottoms from the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.  (This waste does not include still bottoms from the distillations of benzyl chloride.)	Chlorobenzene	108-90-7	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Chloromethane	74-87-3	0.19	30	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Toluene	108-88-3	0.080	10	
K150	Organic residuals, excluding spent carbon adsorbent, from the spent chlorine gas and hydrochloric acid recovery processes associated with the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Chloromethane	74-87-3	0.19	30	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,1,2,2- Tetrachloroethane	79-34-5	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K151	Wastewater treatment sludges, excluding neutralization and biological sludges, generated during the treatment of wastewaters from the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.	Benzene	71-43-2	0.14	10	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		Toluene	108-88-3	0.080	10	
P001	Warfarin, & salts, when present at concentrations greater than 0.3%	Warfarin	81-81-2	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P002	1-Acetyl-2-thiourea	1-Acetyl-2-thiourea	591-08-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P003	Acrolein	Acrolein	107-02-6	0.29	CMBST	
P004	Aldrin	Aldrin	309-00-2	0.021	0.068	
P005	Allyl alcohol	Allyl alcohol	107-18-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P006	Aluminum phosphide	Aluminum phosphide	20859-73-6	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
P007	5-Aminomethyl 3-isoxazolol	5-Aminomethyl 3-isoxazolol	2763-96-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P008	4-Aminopyridine	4-Aminopyridine	504-24-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P009	Ammonium picrate	Ammonium picrate	131-74-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
P010	Arsenic acid	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P011	Arsenic pentoxide	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P012	Arsenic trioxide	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P013	Barium cyanide	Barium	7440-39-3	NA	7.6 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P014	Thiophenol (Benzene thiol)	Thiophenol (Benzene thiol)	108-98-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P015	Beryllium dust	Beryllium	7440-41-7	RMETL;or RTHRM	RMETL; or RTHRM	
P016	Dichloromethyl ether (Bis(chloromethyl)ether)	Dichloromethyl ether	542-88-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P017	Bromoacetone	Bromoacetone	598-31-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P018	Brucine	Brucine	357-57-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P020	2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	88-85-7	0.066	2.5	
P021	Calcium cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P022	Carbon disulfide	Carbon disulfide	75-15-0	3.8	INCIN	
		Carbon disulfide; alternate6 standard for nonwastewaters only	75-15-0	NA	4.8 mg/l TCLP	
P023	Chloroacetaldehyde	Chloroacetaldehyde	107-20-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P024	p-Chloroaniline	p-Chloroaniline	106-47-8	.046	16	
P026	1-(o-Chlorophenyl)thiourea	1-(o-Chlorophenyl)thiourea	5344-82-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P027	3-Chloropropionitrile	3-Chloropropionitrile	542-76-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P028	Benzyl chloride	Benzyl chloride	100-44-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P029	Copper cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P030	Cyanides (soluble salts and complexes)	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P031	Cyanogen	Cyanogen	460-19-5	CHOXD; WETOX; or INCIN	CHOXD; WETOX; or INCIN	
P033	Cyanogen chloride	Cyanogen chloride	506-77-4	CHOXD; WETOX; or INCIN	CHOXD; WETOX; or INCIN	
P034	2-Cyclohexyl-4,6-dinitrophenol	2-Cyclohexyl-4,6-dinitrophenol	131-89-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P036	Dichlorophenylarsine	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P037	Dieldrin	Dieldrin	60-57-1	0.017	0.13	
P038	Diethylarsine	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P039	Disulfoton	Disulfoton	298-04-4	0.017	6.2	
P040	O,O-Diethyl O-pyrazinyl phosphorothioate	O,O-Diethyl O-pyrazinyl phosphorothioate	297-97-2	CARBN; or INCIN	CMBST	
P041	Diethyl-p-nitrophenyl phosphate	Diethyl-p-nitrophenyl phosphate	311-45-5	CARBN; or INCIN	CMBST	
P042	Epinephrine	Epinephrine	51-43-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P043	Diisopropylfluorophosphate (DFP)	Diisopropylfluorophosphate (DFP)	55-91-4	CARBN; or INCIN	CMBST	
P044	Dimethoate	Dimethoate	60-51-5	CARBN; or INCIN	CMBST	
P045	Thiofanox	Thiofanox	39196-18-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P046	alpha, alpha-Dimethylphenethylamine	alpha, alpha-Dimethylphenethylamine	122-09-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P047	4,6-Dinitro-o-cresol	4,6-Dinitro-o-cresol	543-52-1	0.28	160	
	4,6-Dinitro-o-cresol salts	NA	NA	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P048	2,4-Dinitrophenol	2,4-Dinitrophenol	51-28-5	0.12	160	
P049	Dithiobiuret	Dithiobiuret	541-53-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P050	Endosulfan	Endosulfan I	939-98-8	0.023	0.066	
		Endosulfan II	33213-6-5	0.029	0.13	
		Endosulfan sulfate	1031-07-8	0.029	0.13	
P051	Endrin	Endrin	72-20-8	0.0028	0.13	
		Endrin aldehyde	7421-93-4	0.025	0.13	
P054	Aziridine	Aziridine	151-56-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P056	Fluorine	Fluoride (measured in wastewaters only)	16964-48-8	35	ADGAS fb NEUTR	
P057	Fluoroacetamide	Fluoroacetamide	640-19-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P058	Fluoroacetic acid, sodium salt	Fluoroacetic acid, sodium salt	62-74-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P059	Heptachlor	Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
P060	Isodrin	Isodrin	465-73-6	0.021	0.066	
P062	Hexaethyl tetraphosphate	Hexaethyl tetraphosphate	757-58-4	CARBN; or INCIN	CMBST	
P063	Hydrogen cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P064	Isocyanic acid, ethyl ester	Isocyanic acid, ethyl ester	624-83-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P065	P065 (mercury fulminate) nonwastewaters, regardless of their total mercury contant, that are not incinerator residues or are not residues from RMERC.	Mercury	7439-97-6	NA	IMERC	
	P065 (mercury fulminate) nonwastewaters that are either incinerator residues or are residues from RMERC; and contain greater than or equal to 260 mg/kg total mercury.	Mercury	7339-97-6	NA	RMERC	
	P065 (mercury fulminate) nonwastewaters that are residues from RMERC and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	P065 (mercury fulminate) nonwastewaters that are incinerator residues and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All P065 (mercury fulminate) wastewaters.	Mercury	7439-97-6	0.15	NA	
P066	Methomyl	Methomyl	16752-77-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P067	2-Methyl-aziridine	2-Methyl-aziridine	75-55-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P068	Methyl hydrazine	Methyl hydrazine	60-34-4	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED, or CMBST	
P069	2-Methyllactonitrile	2-Methyllactonitrile	75-86-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P070	Aldicarb	Aldicarb	116-06-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P071	Methyl parathion	Methyl parathion	298-00-0	0.014	4.6	
P072	1-Naphthyl-2-thiourea	1-Naphthyl-2-thiourea	86-88-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P073	Nickel carbonyl	Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
P074	Nickel cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
P075	Nicotine and salts	Nicotine and salts	54-11-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P076	Nitric oxide	Nitric oxide	10102-43-9	ADGAS	ADGAS	
P077	p-Nitroaniline	p-Nitroaniline	100-01-6	0.028	28	
P078	Nitrogen dioxide	Nitrogen dioxide	10102-44-0	ADGAS	ADGAS	
P081	Nitroglycerin	Nitroglycerin	55-63-0	CHOXD; CHRED; CARBN; BIODG or INCIN	CHOXD; CHRED; or CMBST	
P082	N-Nitrosodimethylamine	N-Nitrosodimethylamine	62-75-9	0.40	2.3	
P084	N-Nitrosomethylvinylamine	N-Nitrosomethylvinylamine	4549-40-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P085	Octamethylpyrophosphoramide	Octamethylpyrophosphoramide	152-16-9	CARBN; or INCIN	CMBST	
P087	Osmium tetroxide	Osmium tetroxide	20816-12-0	RMETL; or RTHRM	RMETL; or RTHRM	
P088	Endothall	Endothall	145-73-3	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P089	Parathion	Parathion	56-38-2	0.014	4.6	
P092	P092 (phenyl mercuric acetate) nonwastewaters, regardless of their total mercury content, that are not incinerator residues or are not residues from RMERC.	Mercury	7439-97-6	NA	IMERC; or RMERC	
	P092 (phenyl mercuric acetate) nonwastewaters that are either incinerator residues or are residues from RMERC; and still contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	P092 (phenyl mercuric acetate) nonwastewaters that are residues from RMERC and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	P092 (phenyl mercuric acetate) nonwastewaters that are incinerator residues and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All P092 (phenyl mercuric acetate) wastewaters.	Mercury	7439-97-6	0.15	NA	
P093	Phenylthiouea	Phenylthiouea	103-85-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P094	Phorate	Phorate	298-02-2	0.021	4.6	
P095	Phosgene	Phosgene	75-44-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P096	Phosphine	Phosphine	7803-51-2	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
P097	Famphur	Famphur	52-85-7	0.017	15	
P098	Potassium cyanide.	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P099	Potassium silver cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
P101	Ethyl cyanide (Propanenitrile)	Ethyl cyanide (Propanenitrile)	107-12-0	0.24	360	
P102	Propargyl alcohol	Propargyl alcohol	107-19-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
P103	Selenourea	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
P104	Silver cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
P105	Sodium azide	Sodium azide	26628-22-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
P106	Sodium cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P108	Strychnine and salts	Strychnine and salts	57-24-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P109	Tetraethyldithiopyrophosphate	Tetraethyldithiopyrophosphate	3689-24-5	CARBN; or INCIN	CMBST	
P110	Tetraethyl lead	lead	7439-92-1	0.69	0.37 mg/l TCLP	
P111	Tetraethylpyrophosphate	Tetraethylpyrophosphate	107-49-3	CARBN; or INCIN	CMBST	
P112	Tetranitromethane	Tetranitromethane	509-14-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
P113	Thallic oxide	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
P114	Thallium selenite	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
P115	Thallium (I) sulfate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
P116	Thiosemicarbazide	Thiosemicarbazide	79-19-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P118	Trichloromethanethiol	Trichloromethanethiol	75-70-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
P119	Ammonium vanadate	Vanadium (measured in wastewaters only)	7440-62-2	4.3	STABL	
P120	Vanadium pentoxide	Vanadium (measured in wastewaters only)	7440-62-2	4.3	STABL	
P121	Zinc cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P122	Zinc phosphide Zn3P2, when present at concentrations greater than 10%	Zinc Phosphide	1314-84-7	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
P123	Toxaphene	Toxaphene	8001-35-2	0.0095	2.6	
U001	Acetaldehyde	Acetaldehyde	75-07-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U002	Acetone	Acetone	67-64-1	0.28	160	
U003	Acetonitrile	Acetonitrile	75-05-8	5.6	INCIN	
		Acetonitrile; alternate6 standard for nonwastewaters only	75-05-8	NA	1.8	
U004	Acetophenone	Acetophenone	98-86-2	0.010	9.7	
U005	2-Acetylaminofluorene	2-Acetylaminofluorene	53-96-3	0.059	140	
U006	Acetyl chloride	Acetyl chloride	75-36-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U007	Acrylamide	Acrylamide	79-06-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U008	Acrylic acid	Acrylic acid	79-10-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U009	Acrylonitrile	Acrylonitrile	107-13-1	0.24	84	
U010	Mitomycin C	Mitomycin C	50-07-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U011	Amitrole	Amitrole	61-82-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U012	Aniline	Aniline	62-53-3	0.81	14	
U014	Auramine	Auramine	492-80-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U015	Azaserine	Azaserine	115-02-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U016	Benz(c)acridine	Benz(c)acridine	225-51-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U017	Benzal chloride	Benzal chloride	98-87-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U018	Benz(a)anthracene	Benz(a)anthracene	56-55-3	0.059	3.4	
U019	Benzene	Benzene	71-43-2	0.14	10	
U020	Benzenesulfonyl chloride	Benzenesulfonyl chloride	98-09-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U021	Benzidine	Benzidine	92-87-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U022	Benzo(a)pyrene	Benzo(a)pyrene	50-32-8	0.061	3.4	
U023	Benzotrichloride	Benzotrichloride	98-07-7	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U024	bis(2-Chloroethoxy)methane	bis(2-Chloroethoxy)methane	111-91-1	0.036	7.2	
U025	bis(2-Chloroethyl)ether	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
U026	Chlornaphazine	Chlornaphazine	494-03-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U027	bis(2-Chloroisopropyl)ether	bis(2-Chloroisopropyl)ether	108-60-1	0.055	7.2	
U028	bis(2-Ethylhexyl)phthalate	bis(2-Ethylhexyl)phthalate	117-81-7	0.28	28	
U029	Methyl bromide (Bromomethane)	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
U030	4-Bromophenyl phenyl ether	4-Bromophenyl phenyl ether	101-55-3	0.055	15	
U031	n-Butyl alcohol	n-Butyl alcohol	71-36-3	5.6	2.6	
U032	Calcium chromate	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
U033	Carbon oxyfluoride	Carbon oxyfluoride	353-50-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U034	Trichloroacetaldehyde (Chloral)	Trichloroacetaldehyde (Chloral)	75-87-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U035	Chlorambucil	Chlorambucil	305-03-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U036	Chlordane	Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
U037	Chlorobenzene	Chlorobenzene	108-90-7	0.057	6.0	
U038	Chlorobenzilate	Chlorobenzilate	510-15-6	0.10	INCIN	
U039	p-Chloro-m-cresol	p-Chloro-m-cresol	59-50-7	0.018	14	
U041	Epichlorohydrin (1-Chloro-2,3-epoxypropane)	Epichlorohydrin (1-Chloro-2,3-epoxypropane)	106-89-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U042	2-Chloroethyl vinyl ether	2-Chloroethyl vinyl ether	110-75-8	0.062	INCIN	
U043	Vinyl chloride	Vinyl chloride	75-01-4	0.27	6.0	
U044	Chloroform	Chloroform	67-66-3	0.046	6.0	
U045	Chloromethane (Methyl chloride)	Chloromethane (Methyl chloride)	74-87-3	0.19	30	
U046	Chloromethyl methyl ether	Chloromethyl methyl ether	107-30-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U047	2-Chloronaphthalene	2-Chloronaphthalene	91-58-7	0.055	5.6	
U048	2-Chlorophenol	2-Chlorophenol	95-57-8	0.044	5.7	
U049	4-Chloro-o-toluidine hydrochloride	4-Chloro-o-toluidine hydrochloride	3165-93-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U050	Chrysene	Chrysene	218-01-9	0.059	3.4	
U051	Creosote	Naphthalene	91-20-3	0.059	5.6	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenanthrene	85-01-8	0.059	5.6	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U052	Cresols (Cresylic acid)	o-Cresol	95-48-7	0.11	5.6	
		m-Cresol (difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol (difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations)	1319-77-3	0.88	11.2	
U053	Crotonaldehyde	Crotonaldehyde	4170-30-3	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U055	Cumene	Cumene	98-82-8	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U056	Cyclohexane	Cyclohexane	110-82-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U057	Cyclohexanone	Cyclohexanone	108-94-1	0.36	CMBST	
		Cyclohexanone; alternate6 standard for nonwastewaters only	108-94-1	NA	0.75 mg/l TCLP	
U058	Cyclophosphamide	Cyclophosphamide	50-18-0	CARBN; or INCIN	CMBST	
U059	Daunomycin	Daunomycin	20830-81-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U060	DDD	o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
U061	DDT	o,p'-DDT	789-02-6	0.0039	0.087	
		p,p'-DDT	50-29-3	0.0039	0.087	
		o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
		o,p'-DDE	3424-82-6	0.031	0.087	
		p,p'-DDE	72-55-9	0.031	0.087	
U062	Diallate	Diallate	2303-16-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U063	Dibenz(a,h)anthracene	Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
U064	Dibenz(a,i)pyrene	Dibenz(a,i)pyrene	189-55-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U066	1,2-Dibromo-3-chloropropane	1,2-Dibromo-3-chloropropane	96-12-8	0.11	15	
U067	Ethylene dibromide (1,2-Dibromoethane)	Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
U068	Dibromomethane	Dibromomethane	74-95-3	0.11	15	
U069	Di-n-butyl phthalate	Di-n-butyl phthalate	84-74-2	0.057	28	
U070	o-Dichlorobenzene	o-Dichlorobenzene	95-50-1	0.088	6.0	
U071	m-Dichlorobenzene	m-Dichlorobenzene	541-73-1	0.036	6.0	
U072	p-Dichlorobenzene	p-Dichlorobenzene	106-46-7	0.090	6.0	
U073	3,3'-Dichlorobenzidine	3,3'-Dichlorobenzidine	91-94-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U074	1,4-Dichloro-2-butene	cis-1,4-Dichloro-2-butene	1476-11-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
		trans-1,4-Dichloro-2-butene	764-41-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U075	Dichlorodifluoromethane	Dichlorodifluoromethane	75-71-8	0.23	7.2	
U076	1,1-Dichloroethane	1,1-Dichloroethane	75-34-3	0.059	6.0	
U077	1,2-Dichloroethane	1,2-Dichloroethane	107-06-2	0.21	6.0	
U078	1,1-Dichloroethylene	1,1-Dichloroethylene	75-35-4	0.025	6.0	
U079	1,2-Dichloroethylene	trans-1,2-Dichloroethylene	156-60-5	0.054	30	
U080	Methylene chloride	Methylene chloride	75-09-2	0.089	30	
U081	2,4-Dichlorophenol	2,4-Dichlorophenol	120-83-2	0.044	14	
U082	2,6-Dichlorophenol	2,6-Dichlorophenol	87-65-0	0.044	14	
U083	1,2-Dichloropropane	1,2-Dichloropropane	78-87-5	0.85	18	
U084	1,3-Dichloropropylene	cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
U085	1,2:3,4-Diepoxybutane	1,2:3,4-Diepoxybutane	1464-53-5	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U086	N,N'-Diethylhydrazine	N,N'-Diethylhydrazine	1615-80-1	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U087	O,O-Diethyl S-methyldithiophosphate	O,O-Diethyl S-methyldithiophosphate	3288-58-2	CARBN; or INCIN	CMBST	
U088	Diethyl phthalate	Diethyl phthalate	84-66-2	0.20	28	
U089	Diethyl stilbestrol	Diethyl stilbestrol	56-53-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U090	Dihydrosafrole	Dihydrosafrole	94-58-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U091	3,3'-Dimethoxybenzidine	3,3'-Dimethoxybenzidine	119-90-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U092	Dimethylamine	Dimethylamine	124-40-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U093	p-Dimethylaminoazobenzene	p-Dimethylaminoazobenzene	60-11-7	0.13	INCIN	
U094	7,12-Dimethylbenz(a)anthracene	7,12-Dimethylbenz(a)anthracene	57-97-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U095	3,3'-Dimethylbenzidine	3,3'-Dimethylbenzidine	119-93-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U096	alpha, alpha-Dimethyl benzyl hydroperoxide	alpha, alpha-Dimethyl benzyl hydroperoxide	80-15-9	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U097	Dimethylcarbamoyl chloride	Dimethylcarbamoyl chloride	79-44-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U098	1,1-Dimethylhydrazine	1,1-Dimethylhydrazine	57-14-7	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U099	1,2-Dimethylhydrazine	1,2-Dimethylhydrazine	540-73-8	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U101	2,4-Dimethylphenol	2,4-Dimethylphenol	105-67-9	0.036	14	
U102	Dimethyl phthalate	Dimethyl phthalate	131-11-3	0.047	28	
U103	Dimethyl sulfate	Dimethyl sulfate	77-78-1	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U105	2,4-Dinitrotoluene	2,4-Dinitrotoluene	121-14-2	0.32	140	
U106	2,6-Dinitrotoluene	2,6-Dinitrotoluene	606-20-2	0.55	28	
U107	Di-n-octyl phthalate	Di-n-octyl phthalate	117-84-0	0.017	28	
U108	1,4-Dioxane	1,4-Dioxane	123-91-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
		1,4-Dioxane; alternate 6 standard for nonwastewaters only	123-91-1	NA	170	
U109	1,2-Diphenylhydrazine	1,2-Diphenylhydrazine	122-66-7	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
		1,2-Diphenylhydrazine; alternate 6 standard for wastewaters only	122-66-7	0.087	NA	
U110	Dipropylamine	Dipropylamine	142-84-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U111	Di-n-propylnitrosamine	Di-n-propylnitrosamine	621-64-7	0.40	14	
U112	Ethyl acetate	Ethyl acetate	141-78-8	0.34	33	
U113	Ethyl acrylate	Ethyl acrylate	140-88-5	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U114	Ethylenebisdithiocarbamic acid salts and esters	Ethylenebisdithiocarbamic acid	111-54-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U115	Ethylene oxide	Ethylene oxide 	75-21-8	(WETOX or CHOXD) fb CARBN; or INCIN	CHOXD; or INCIN	
		Ethylene oxide; alternate 6 standard for wastewaters only	75-21-8	0.12	NA	
U116	Ethylene thiourea	Ethylene thiourea	96-45-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U117	Ethyl ether	Ethyl ether	60-29-7	0.12	160	
U118	Ethyl methacrylate	Ethyl methacrylate	97-63-2	0.14	160	
U119	Ethyl methane sulfonate	Ethyl methane sulfonate	62-50-0	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U120	Fluoranthene	Fluoranthene	206-44-0	0.068	3.4	
U121	Trichloromonofluoromethane	Trichloromonofluoromethane	75-69-4	0.020	30	
U122	Formaldehyde	Formaldehyde	50-00-0	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U123	Formic acid	Formic acid	64-18-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U124	Furan	Furan	110-00-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U125	Furfural	Furfural	98-01-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U126	Glycidylaldehyde	Glycidylaldehyde	765-34-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U127	Hexachlorobenzene	Hexachlorobenzene	118-74-1	0.055	10	
U128	Hexachlorobutadiene	Hexachlorobutadiene	87-68-3	0.055	5.6	
U129	Lindane	alpha-BHC	319-84-6	0.00014	0.066	
		beta-BHC	319-85-7	0.00014	0.066	
		delta-BHC	319-86-8	0.023	0.066	
		gamma-BHC (Lindane)	58-89-9	0.0017	0.066	
U130	Hexachlorocyclopentadiene	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
U131	Hexachloroethane	Hexachloroethane	67-72-1	0.055	30	
U132	Hexachlorophene	Hexachlorophene	70-30-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U133	Hydrazine	Hydrazine	302-01-2	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U134	Hydrogen fluoride	Fluoride (measured in wastewaters only)	16964-48-8	35	ADGAS fb NEUTR; or NEUTR	
U135	Hydrogen sulfide	Hydrogen sulfide	7783-06-4	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
U136	Cacodylic acid	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
U137	Indeno(1,2,3-cd)pyrene	Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
U138	Iodomethane	Iodomethane	74-88-4	0.19	65	
U140	Isobutyl alcohol	Isobutyl alcohol	78-83-1	5.6	170	
U141	Isosafrole	Isosafrole	120-58-1	0.081	2.6	
U142	Kepone	Kepone	143-50-8	0.0011	0.13	
U143	Lasiocarpine	Lasiocarpine	303-34-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U144	Lead acetate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U145	Lead phosphate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U146	Lead subacetate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U147	Maleic anhydride	Maleic anhydride	108-31-6	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U148	Maleic hydrazide	Maleic hydrazide	123-33-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U149	Malononitrile	Malononitrile	109-77-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U150	Melphalan	Melphalan	148-82-3	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U151	U151 (mercury) nonwastewaters that contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	U151 (mercury) nonwastewaters that contain less than 260 mg/kg total mercury and that are residues from RMERC only.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	U151 (mercury) nonwastewaters that contain less than 260 mg/kg total mercury and that are not residues from RMERC only.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All U151 (mercury) wastewater.	Mercury	7439-97-6	0.15	NA	
	Element Mercury Contaminated with Radioactive Materials	Mercury	7439-97-6	NA	AMLGM	
U152	Methacrylonitrile	Methacrylonitrile	126-98-7	0.24	84	
U153	Methanethiol	Methanethiol	74-93-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U154	Methanol	Methanol	67-56-1	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
		Methanol; alternate6 set of standards for both wastewaters and nonwastewaters	67-56-1	5.6	0.75 mg/l TCLP	
U155	Methapyrilene	Methapyrilene	91-80-5	0.081	1.5	
U156	Methyl chlorocarbonate	Methyl chlorocarbonate	79-22-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U157	3-Methylcholanthrene	3-Methylcholanthrene	56-49-5	0.0055	15	
U158	4,4'-Methylene bis(2-chloroaniline)	4,4'-Methylene bis(2-chloroaniline)	101-14-4	0.50	30	
U159	Methyl ethyl ketone	Methyl ethyl ketone	78-93-3	0.28	36	
U160	Methyl ethyl ketone peroxide	Methyl ethyl ketone peroxide	1338-23-4	CHOXD; CHRED; CARBN; BIODG; or INCIN	CHOXD; CHRED; or CMBST	
U161	Methyl isobutyl ketone	Methyl isobutyl ketone	108-10-1	0.14	33	
U162	Methyl methacrylate	Methyl methacrylate	80-62-6	0.14	160	
U163	N-Methyl N'-nitro N-nitrosoguanidine	N-Methyl N'-nitro N-nitrosoguanidine	70-25-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U164	Methylthiouracil	Methylthiouracil	56-04-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U165	Naphthalene	Naphthalene	91-20-3	0.059	5.6	
U166	1,4-Naphthoquinone	1,4-Naphthoquinone	130-15-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U167	1-Naphthlyamine	1-Naphthlyamine	134-32-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U168	2-Naphthlyamine	2-Naphthlyamine	91-59-8	0.52	INCIN	
U169	Nitrobenzene	Nitrobenzene	98-95-3	0.068	14	
U170	p-Nitrophenol	p-Nitrophenol	100-02-7	0.12	29	
U171	2-Nitropropane	2-Nitropropane	79-46-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U172	N-Nitrosodi-n-butylamine	N-Nitrosodi-n-butylamine	924-16-3	0.40	17	
U173	N-Nitrosodiethanolamine	N-Nitrosodiethanolamine	1116-54-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U174	N-Nitrosodiethylamine	N-Nitrosodiethylamine	55-18-5	0.40	28	
U176	N-Nitroso-N-ethylurea	N-Nitroso-N-ethylurea	759-73-9	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U177	N-Nitroso-N-methylurea	N-Nitroso-N-methylurea	684-93-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U178	N-Nitroso-N-methylurethane	N-Nitroso-N-methylurethane	615-53-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U179	N-Nitrosopiperidine	N-Nitrosopiperidine	100-75-4	0.013	35	
U180	N-Nitrosopyrrolidine	N-Nitrosopyrrolidine	930-55-2	0.013	35	
U181	5-Nitro-o-toluidine	5-Nitro-o-toluidine	99-55-8	0.32	28	
U182	Paraldehyde	Paraldehyde	123-63-7	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U183	Pentachlorobenzene	Pentachlorobenzene	608-93-5	0.055	10	
U184	Pentachloroethane	Pentachloroethane	76-01-7	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
		Pentachloroethane; alternate6 standards for both wastewaters and nonwastewaters	76-01-7	0.055	6.0	
U185	Pentachloronitrobenzene	Pentachloronitrobenzene	82-68-8	0.055	4.8	
U186	1,3-Pentadiene	1,3-Pentadiene	504-60-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U187	Phenacetin	Phenacetin	62-44-2	0.081	16	
U188	Phenol	Phenol	108-95-2	0.039	6.2	
U189	Phosphorus sulfide	Phosphorus sulfide	1314-80-3	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
U190	Phthalic anhydride	Phthalic anhydride (measured as Phthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride	85-44-9	0.055	28	
U191	2-Picoline	2-Picoline	109-06-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U192	Pronamide	Pronamide	23950-58-5	0.093	1.5	
U193	1,3-Propane sultone	1,3-Propane sultone	1120-71-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U194	n-Propylamine	n-Propylamine	107-10-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U196	Pyridine	Pyridine	110-86-1	0.014	16	
U197	p-Benzoquinone	p-Benzoquinone	106-51-4	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U200	Reserpine	Reserpine	50-55-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U201	Resorcinol	Resorcinol	108-46-3	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U202	Saccharin and salts	Saccharin	81-07-2	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U203	Safrole	Safrole	94-59-7	0.081	22	
U204	Selenium dioxide	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
U205	Selenium sulfide	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
U206	Streptozotocin	Streptozotocin	18883-66-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U207	1,2,4,5-Tetrachlorobenzene	1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
U208	1,1,1,2-Tetrachloroethane	1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
U209	1,1,2,2-Tetrachloroethane	1,1,2,2-Tetrachloroethane	79-34-5	0.057	6.0	
U210	Tetrachloroethylene	Tetrachloroethylene	127-18-4	0.056	6.0	
U211	Carbon tetrachloride	Carbon tetrachloride	56-23-5	0.057	6.0	
U213	Tetrahydrofuran	Tetrahydrofuran	109-99-9	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U214	Thallium (I) acetate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U215	Thallium (I) carbonate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U216	Thallium (I) chloride	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U217	Thallium (I) nitrate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
U218	Thioacetamide	Thioacetamide	62-55-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U219	Thiourea	Thiourea	62-56-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U220	Toluene	Toluene	108-88-3	0.080	10	
U221	Toluenediamine	Toluenediamine	25376-45-8	CARBN; or INCIN	CMBST	
U222	o-Toluidine hydrochloride	o-Toluidine hydrochloride	636-21-5	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U223	Toluene diisocyanate	Toluene diisocyanate	26471-62-5	CARBN; or INCIN	CMBST	
U225	Bromoform (Tribromomethane)	Bromoform (Tribromomethane)	75-25-2	0.63	15	
U226	1,1,1-Trichloroethane	1,1,1-Trichloroethane	71-55-6	0.054	6.0	
U227	1,1,2-Tricloroethane	1,1,2-Tricloroethane	79-00-5	0.054	6.0	
U228	Trichloroethylene	Trichloroethylene	79-01-6	0.054	6.0	
U234	1,3,5-Trinitrobenzene	1,3,5-Trinitrobenzene	99-35-4	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U235	tris-(2,3-Dibromopropyl)-phosphate	tris-(2,3-Dibromopropyl)-phosphate	126-72-7	0.11	0.10	
U236	Trypan Blue	Trypan Blue	72-57-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U237	Uracil mustard	Uracil mustard	66-75-1	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U238	Urethane (Ethyl carbamate)	Urethane (Ethyl carbamate)	51-79-6	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U239	Xylenes	Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
U240	2,4-D (2,4-Dichlorophenoxyacetic acid)	2,4-D (2,4-Dichlorophenoxyacetic acid)	94-75-7	0.72	10	
	2,4-D (2,4-Dichlorophenoxyacetic acid) salts and esters		NA	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U243	Hexachloropropylene	Hexachloropropylene	1888-71-7	0.035	30	
U244	Thiram	Thiram	137-26-8	(WETOX or CHOXD) fb CARBN; or INCIN	INCIN	
U246	Cyanogen bromide	Cyanogen bromide	506-68-3	CHOXD; WETOX; or INCIN	CHOXD; WETOX; or INCIN	
U247	Methoxychlor	Methoxychlor	72-43-5	0.25	0.18	
U248	Warfarin, & salts, when present at concentrations of 0.3% or less	Warfarin	81-81-2	(WETOX or CHOXD) fb CARBN; or INCIN	CMBST	
U249	Zinc phosphide, Zn3P2, when present at concentrations of 10% or less	Zinc Phosphide	1314-84-7	CHOXD; CHRED; or INCIN	CHOXD; CHRED; or INCIN	
U328	o-Toluidine	o-Toluidine	95-53-4	INCIN; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN	INCIN; or Thermal Destruction	
U353	p-Toluidine	p-Toluidine	106-49-0	INCIN; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN	INCIN; or Thermal Destruction	
U359	2-Ethoxyethanol	2-Ethoxyethanol	110-80-5	INCIN; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN	CMBST	

1	The waste descriptions provided in this table do not replace waste descriptions in 40 CFR part 261.  Descriptions of Treatment/Regulatory Subcategories are provided, as needed, to distinguish between applicability of different standards.
2	CAS means Chemical Abstract Services.  When the waste code and/or regulated constituents are described as a combination of a chemical with its salts and/or esters, the CAS number is given for the parent compound only.
3	Concentration standards for wastewaters are expressed in mg/l are based on analysis of composite samples.
4	All treatment standards expressed as a Technology Code or combination of Technology Codes are explained in detail in 40 CFR 268.42, Table 1 - Technology Codes and Descriptions of Technology-Based Standards.
5	Except for Metals (EP or TCLP) and Cyanides (Total and Amenable) the nonwastewater treatment standards expressed as a concentration were established, in part, based upon incineration in units operated in accordance with the technical requirements of 40 CFR part 264, subpart O or 40 CFR part 265, subpart O, or based upon combustion in fuel substitution units operating in accordance with applicable technical requirements.  A facility may comply with these treatment standards according to provisions in 40 CFR 268.40(d).  All concentration standards for nonwastewaters are based on analysis of grab samples.
6	Where an alternate treatment standard or set of alternate standards has been indicated, a facility may comply with this alternate standard, but only for the Treatment/Regulatory Subcategory or physical form (i.e., wastewater and/or nonwastewater) specified for that alternate standard.
7	Both Cyanides (Total) and Cyanides (Amenable) for nonwastewaters are to be analyzed using Method 9010 or 9012, found in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods", EPA Publication SW-846, as incorporated by reference in 40 CFR 260.11, with a sample size of 10 grams and a distillation time of one hour and 15 minutes.

NOTE:  NA means not applicable.

	25. Section 268.41 is revised to read as follows:

§ 268.41   Treatment standards expressed as concentrations in waste extract.

	For the requirements previously found in this section and for treatment standards in Table CCWE-Constituent Concentrations in Waste Extracts, refer to § 268.40.

	26. Section 268.42 is amended by removing Table 2 and Table 3; revising paragraphs (a) introductory text, (c)(2), and (d); adding a note before paragraph (a); and adding the entry "CMBST" into Table 1.-Technology Codes and Description of Technology-Based Standards in alphabetical order, to read as follows:

§ 268.42   Treatment standards expressed as specified technologies.

	Note: For the requirements previously found in this section in Table 2-Technology-Based Standards By RCRA Waste Code, and Table 3-Technology-Based Standards for Specific Radioactive Hazardous Mixed Waste, refer to § 268.40.

	(a) The following wastes in paragraphs (a)(1) and (a)(2) of this section and in the table in § 268.40 "Treatment Standards for Hazardous Wastes," for which standards are expressed as a treatment method rather than a concentration level, must be treated using the technology or technologies specified in paragraphs (a)(1) and (a)(2) and Table 1 of this section.

*	*	*	*	*

	 Table 1.-Technology Codes and Description of Technology-Based Standards 
Technology code				Description of technology_based standards          	
*          *          *          *          *          *          *	
CMBST			Combustion in incinerators, boilers, or industrial furnaces operated in accordance with the applicable requirements of 40 CFR part 264, subpart O, or 40 CFR part 266, subpart H.	
*          *          *          *          *          *          *	

*	*	*	*	*

	(c) * * *

	(2) The lab pack does not contain any of the wastes listed in Appendix IV to part 268.

*	*	*	*	*

	(d) Radioactive hazardous mixed wastes are subject to the treatment standards in § 268.40. Where treatment standards are specified for radioactive mixed wastes in the Table of Treatment Standards, those treatment standards will govern. Where there is no specific treatment standard for radioactive mixed waste, the treatment standard for the hazardous waste (as designated by EPA waste code) applies. Hazardous debris containing radioactive waste is subject to the treatment standards specified in § 268.45.

	28. Section 268.43 is revised to read as follows:

§ 268.43   Treatment standards expressed as waste concentrations.

	For the requirements previously found in this section and for treatment standards in Table CCW-Constituent Concentrations in Wastes, refer to § 268.40.

	29. Section 268.45(b)(2) is revised to read as follows:

§ 268.45   Treatment standards for hazardous debris.

*	*	*	*	*

	(b) * * *

	(2) Debris contaminated with listed waste. The contaminants subject to treatment for debris that is contaminated with a prohibited listed hazardous waste are those constituents or wastes for which treatment standards are established for the waste under § 268.40.

	30. Section 268.46 is revised to read as follows:

§ 268.46   Alternative treatment standards based on HTMR.

	For the treatment standards previously found in this section, refer to § 268.40.

	31. In Subpart D, § 268.48 is added to read as follows:

§ 268.48   Universal Treatment Standards

	(a) Table UTS identifies the hazardous constituents, along with the nonwastewater and wastewater treatment standard levels, that are used to regulate most prohibited hazardous wastes with numerical limits. For determining compliance with treatment standards for underlying hazardous constituents as defined in § 268.2(i), these treatment standards may not be exceeded. Compliance with these treatment standards is measured by an analysis of grab samples, unless otherwise noted in the following Table UTS.

	
§ 268.48 Table UTS-Universal Treatment Standards				
Regulated constituent-common name	CAS1 No.	Wastewater standard.  Concentration in mg/2	Nonwastewater standard.  Concentration in mg/kg3 unless noted as "mg/l TCLP"	
Acenaphthylene						208_96_8	0.059		3.4				
Acenaphthene						83_32_9		0.059		3.4				
Acetone							67_64_1		0.28		160				
Acetonitrile						75_05_8		5.6		1.8				
Acetophenone						96_86_2		0.010		9.7				
2_Acetylaminofluorene					53_96_3		0.059		140				
Acrolein						107_02_8	0.29		NA				
Acrylamide						79_06_1		19		23				
Acrylonitrile						107_13_1	0.24		84				
Aldrin							309_00_2	0.021		0.066				
4_Aminobiphenyl						92_67_1		0.13		NA				
Aniline							62_53_3		0.81		14				
Anthracene						120_12_7	0.059		3.4				
Aramite							140_57_8	0.36		NA				
alpha_BHC						319_84_6	0.00014		0.066				
beta_BHC						319_85_7	0.00014		0.066				
delta_BHC						319_86_8	0.023		0.066				
gamma_BHC						58_89_9		0.0017		0.066				
Benzene							71_43_2		0.14		10				
Benz(a)anthracene					56_55_3		0.059		3.4				
Benzal chloride						98_87_3		0.055		6.0				
Benzo(b)fluoranthene (difficult to distinguish 	205_99_2	0.11		6.8
  from benzo(k)fluoranthene)				
Benzo(k)fluoranthene (difficult to distinguish	207_08_9	0.11		6.8
  from benzo(b)fluoranthene)				
Benzo(g,h,i)perylene					191_24_2	0.0055		1.8				
Benzo(a)pyrene						50_32_8		0.061		3.4				
Bromodichloromethane					75_27_4		0.35		15				
Methyl bromide (Bromomethane)				74_83_9		0.11		15				
4_Bromophenyl phenyl ether				101_55_3	0.055		15				
n_Butyl alcohol						71_36_3		5.6		2.6				
Butyl benzyl phthalate					85_68_7		0.017		28				
2_sec_Butyl_4,6_dinitrophenol (Dinoseb)			88_85_7		0.066		2.5				
Carbon disulfide					75_15_0		3.8		4.8 mg/l TCLP				
Carbon tetrachloride					56_23_5		0.057		6.0				
Chlordane (alpha and gamma isomers)			57_74_9		0.0033		0.26				
p_Chloroaniline						106_47_8	0.46		16				
Chlorobenzene						108_90_7	0.057		6.0				
Chlorobenzilate						510_15_6	0.10		NA				
2_Chloro_1,3_butadiene					126_99_8	0.057		0.28				
Chlorodibromomethane					124_48_1	0.057		15				
Chloroethane						75_00_3		0.27		6.0				
bis(2_Chloroethoxy)methane				111_91_1	0.036		7.2				
bis(2_Chloroethyl)ether					111_44_4	0.033		6.0				
Chloroform						67_66_3		0.046		6.0				
bis(2_Chloroisopropyl)ether				108_60_1	0.055		7.2				
p_Chloro_m_cresol					59_50_7		0.018		14				
2_Chloroethyl vinyl ether				110_75_8	0.062		NA				
Chloromethane (Methyl chloride)				74_87_3		0.19		30				
2_Chloronaphthalene					91_58_7		0.055		5.6				
2_Chlorophenol						95_57_8		0.044		5.7				
3_Chloropropylene					107_05_1	0.036		30				
Chrysene						218_01_9	0.059		3.4				
o_Cresol						95_48_7		0.11		5.6				
m_Cresol (difficult to distinguish			108_39_4	0.77		5.6
  from p-cresol)				
p_Cresol (difficult to distinguish			106_44_5	0.77		5.6
  from m-cresol)				
Cyclohexanone						108_94_1	0.36		0.75 mg/l TCLP				
1,2_Dibromo_3_chloropropane				96_12_8		0.11		15				
Ethylene dibromide (1,2_Dibromoethane)			106_93_4	0.028		15				
Dibromomethane						74_95_3		0.11		15				
2,4_D (2,4_Dichlorophenoxyacetic acid)			94_75_7		0.72		10				
o,p'_DDD						53_19_0		0.023		0.087				
p,p'_DDD						72_54_8		0.023		0.087				
o,p'_DDE						3424_82_6	0.031		0.087				
p,p'_DDE						72_55_9		0.031		0.087				
o,p'_DDT						789_02_6	0.0039		0.087				
p,p'_DDT						50_29_3		0.0039		0.087				
Dibenz(a,h)anthracene					53_70_3		0.055		8.2				
Dibenz(a,e)pyrene					192_65_4	0.061		NA				
m_Dichlorobenzene					541_73_1	0.036		6.0				
o_Dichlorobenzene					95_50_1		0.088		6.0				
p_Dichlorobenzene					106_46_7	0.090		6.0				
Dichlorodifluoromethane					75_71_8		0.23		7.2				
1,1_Dichloroethane					75_34_3		0.059		6.0				
1,2_Dichloroethane					107_06_2	0.21		6.0				
1,1_Dichloroethylene					75_35_4		0.025		6.0				
trans_1,2_Dichloroethylene				156_60_5	0.054		30				
2,4_Dichlorophenol					120_83_2	0.044		14				
2,6_Dichlorophenol					87_65_0		0.044		14				
1,2_Dichloropropane					78_87_5		0.85		18				
cis_1,3_Dichloropropylene				10061_01_5	0.036		18				
trans_1,3_Dichloropropylene				10061_02_6	0.036		18				
Dieldrin						60_57_1		0.017		0.13				
Diethyl phthalate					84_66_2		0.20		28				
2_4_Dimethyl phenol					105_67_9	0.036		14				
Dimethyl phthalate					131_11_3	0.047		28				
Di_n_butyl phthalate					84_74_2		0.057		28				
1,4_Dinitrobenzene					100_25_4	0.32		2.3				
4,6_Dinitro_o_cresol					534_52_1	0.28		160				
2,4_Dinitrophenol					51_28_5		0.12		160				
2,4_Dinitrotoluene					121_14_2	0.32		140				
2,6_Dinitrotoluene					606_20_2	0.55		28				
Di_n_octyl phthalate					117_84_0	0.017		28				
p_Dimethylaminoazobenzene				60_11_7		0.13		NA				
Di_n_propylnitrosamine					621_64_7	0.40		14				
1,4_Dioxane						123_91_1	NA		170				
Diphenylamine (difficult to distinguish			122_39_4	0.92		13
  from diphenylnitrosamine)				
Diphenylnitrosamine (difficult to distinguish	86_30_6		0.92		13
  from diphenylamine)				
1,2_Diphenylhydrazine					122_66_7	0.087		NA				
Disulfoton						298_04_4	0.017		6.2				
Endosulfan I						939_98_8	0.023		0.066				
Endosulfan II						33213_6_5	0.029		0.13				
Endosulfan sulfate					1_31_07_8	0.029		0.13				
Endrin							72_20_8		0.0028		0.13				
Endrin aldehyde						7421_93_4	0.025		0.13				
Ethyl acetate						141_78_6	0.34		33				
Ethyl cyanide (Propanenitrile)				107_12_0	0.24		360				
Ethyl benzene						100_41_4	0.057		10				
Ethyl ether						60_29_7		0.12		160				
bis(2_Ethylhexyl) phthalate				117_81_7	0.28		28				
Ethyl methacrylate					97_63_2		0.14		160				
Ethylene oxide						75_21_8		0.12		NA				
Famphur							52_85_7		0.017		15				
Fluoranthene						206_44_0	0.068		3.4				
Fluorene						86_73_7		0.059		3.4				
Heptachlor						76_44_8		0.0012		0.066				
Heptachlor epoxide					1024_57_3	0.016		0.066				
Hexachlorobenzene					118_74_1	0.055		10				
Hexachlorobutadiene					87_68_3		0.055		5.6				
Hexachlorocyclopentadiene				77_47_4		0.057		2.4				
HxCDDs (All Hexachlorodibenzo_p_dioxins)			NA		0.000063	0.001				
HxCDFs (All Hexachlorodibenzofurans)			NA		0.000063	0.001				
Hexachloroethane					67_72_1		0.055		30				
Hexachloropropylene					1888_71_7	0.035		30				
Indeno (1,2,3_c,d) pyrene				193_39_5	0.0055		3.4				
Iodomethane						74_88_4		0.19		65				
Isobutyl alcohol					78_83_1		5.6		170				
Isodrin							465_73_6	0.021		0.066				
Isosafrole						120_58_1	0.081		2.6				
Kepone							143_50_8	0.0011		0.13				
Methacrylonitrile					126_98_7	0.24		84				
Methanol						67_56_1		5.6		0.75 mg/l TCLP				
Methapyrilene						91_80_5		0.081		1.5				
Methoxychlor						72_43_5		0.25		0.18				
3_Methylcholanthrene					56_49_5		0.0055		15				
4,4_Methylene bis(2_chloroaniline)			101_14_4	0.50		30				
Methylene chloride					75_09_2		0.089		30				
Methyl ethyl ketone					78_93_3		0.28		36				
Methyl isobutyl ketone					108_10_1	0.14		33				
Methyl methacrylate					80_62_6		0.14		160				
Methyl methansulfonate					66_27_3		0.018		NA				
Methyl parathion					298_00_0	0.014		4.6				
Naphthalene						91_20_3		0.059		5.6				
2_Naphthylamine						91_59_8		0.52		NA				
o_Nitroaniline						88_74_4		0.27		14				
p_Nitroaniline						100_01_6	0.028		28				
Nitrobenzene						98_95_3		0.068		14				
5_Nitro_o_toluidine					99_55_8		0.32		28				
o_Nitrophenol						88_75_5		0.028		13				
p_Nitrophenol						100_02_7	0.12		29				
N_Nitrosodiethylamine					55_18_5		0.40		28				
N_Nitrosodimethylamine					62_75_9		0.40		2.3				
N_Nitroso_di_n_butylamine				924_16_3	0.40		17				
N_Nitrosomethylethylamine				10595_95_6	0.40		2.3				
N_Nitrosomorpholine					59_89_2		0.40		2.3				
N_Nitrosopiperidine					100_75_4	0.013		35				
N_Nitrosopyrrolidine					930_55_2	0.013		35				
Parathion						56_38_2		0.014		4.6				
Total PCBs (sum of all PCB isomers,			1336_36_3	0.10		10
  or all Aroclors)				
Pentachlorobenzene					608_93_5	0.055		10				
PeCDDs (All Pentachlorodibenzo_p_dioxins)		NA		0.000063	0.001				
PeCDFs (All Pentachlorodibenzofurans)			NA		0.000035	0.001				
Pentachloroethane					76_01_7		0.055		6.0				
Pentachloronitrobenzene					82_68_8		0.055		4.8				
Pentachlorophenol					87_86_5		0.089		7.4				
Phenacetin						62_44_2		0.081		16				
Phenanthrene						85_01_8		0.059		5.6				
Phenol							108_95_2	0.039		6.2				
Phorate							298_02_2	0.021		4.6				
Phthalic acid						100_21_0	0.055		28				
Phthalic anhydride					85_44_9		0.055		28				
Pronamide						23950_58_5	0.093		1.5				
Pyrene							129_00_0	0.067		8.2				
Pyridine						110_86_1	0.014		16				
Safrole							94_59_7		0.081		22				
Silvex (2,4,5_TP)					93_72_1		0.72		7.9				
2,4,5_T (2,4,5_Trichlorophenoxyacetic acid)		93_76_5		0.72		7.9				
1,2,4,5_Tetrachlorobenzene				95_94_3		0.055		14				
TCDDs (All Tetrachlorodibenzo_p_dioxins)			NA		0.000063	0.001				
TCDFs (All Tetrachlorodibenzofurans)			NA		0.000063	0.001				
1,1,1,2_Tetrachloroethane				630_20_6	0.057		6.0				
1,1,2,2_Tetrachloroethane				79_34_6		0.057		6.0				
Tetrachloroethylene					127_18_4	0.056		6.0				
2,3,4,6_Tetrachlorophenol				58_90_2		0.030		7.4				
Toluene							108_88_3	0.080		10				
Toxaphene						8001_35_2	0.0095		2.6				
Bromoform (Tribromomethane)				75_25_2		0.63		15				
1,2,4_Trichlorobenzene					120_82_1	0.055		19				
1,1,1_Trichloroethane					71_55_6		0.054		6.0				
1,1,2_Trichloroethane					79_00_5		0.054		6.0				
Trichloroethylene					79_01_6		0.054		6.0				
Trichloromonofluoromethane				75_69_4		0.020		30				
2,4,5_Trichlorophenol					95_95_4		0.18		7.4				
2,4,6_Trichlorophenol					88_06_2		0.035		7.4				
1,2,3_Trichloropropane					96_18_4		0.85		30				
1,1,2_Trichloro_1,2,2_trifluoroethane			76_13_1		0.057		30				
tris_(2,3_Dibromopropyl) phosphate			126_72_7	0.11		0.10				
Vinyl chloride						75_01_4		0.27		6.0				
Xylenes_mixed isomers (sum of o_,m-,			1330_20_7	0.32		30
  and p-xylene concentrations)				
Antimony						7440_36_0	1.9		2.1 mg/l TCLP				
Arsenic							7440_38_2	1.4		5.0 mg/l TCLP				
Barium							7440_39_3	1.2		7.6 mg/l TCLP				
Beryllium						7440_41_7	0.82		0.014 mg/l TCLP				
Cadmium							7440_43_9	0.69		0.19 mg/l TCLP				
Chromium (Total)					7440_47_3	2.77		0.86 mg/l TCLP				
Cyanides (Total)4					57_12_5		1.2		590				
Cyanides (Amenable)4					57_12_5		0.86		30				
Fluoride						16964_48_8	35		NA				
Lead							7439_92_1	0.69		0.37 mg/l TCLP				
Mercury_Nonwastewater from Retort			7439_97_6	NA		0.20 mg/l TCLP				
Mercury_All Others					7439_97_6	0.15		0.025 mg/l TCLP				
Nickel							7440_02_0	3.98		5.0 mg/l TCLP				
Selenium						7782_49_2	0.82		0.16 mg/l TCLP				
Silver							7440_22_4	0.43		0.30 mg/l TCLP				
Sulfide							8496_25_8	14		NA				
Thallium						7440_28_0	1.4		0.078 mg/l TCLP				
Vanadium						7440_62_2	4.3		0.23 mg/l TCLP				
Zinc5							7440_66_6	2.61		5.3 mg/l TCLP				

	1 CAS means Chemical Abstract Services. When the waste code and/or regulated constituents are described as a combination of a chemical with its salts and/or esters, the CAS number is given for the parent compound only.
	2 Concentration standards for wastewaters are expressed in mg/l are based on analysis of composite samples.
	3 Except for Metals (EP or TCLP) and Cyanides (Total and Amenable) the nonwastewater treatment standards expressed as a concentration were established, in part, based upon incineration in units operated in accordance with the technical requirements of 40 CFR part 264, subpart O or 40 CFR part 265, subpart O, or based upon combustion in fuel substitution units operating in accordance with applicable technical requirements. A facility may comply with these treatment standards according to provisions in 40 CFR 268.40(d). All concentration standards for nonwastewaters are based on analysis of grab samples.
	4 Both Cyanides (Total) and Cyanides (Amenable) for nonwastewaters are to be analyzed using Method 9010 or 9012, found in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods", EPA Publication SW-846, as incorporated by reference in 40 CFR 260.11, with a sample size of 10 grams and a distillation time of one hour and 15 minutes.
	5 Zinc is not an "underlying hazardous constituent" in characteristic wastes, according to the definition at 268.2(i).
Note: NA means not applicable.

Appendix IV to Part 268 [Revised]

	32. Appendix IV to part 268 is revised to read as follows:

Appendix IV to Part 268-Wastes Excluded From Lab Packs Under the Alternative Treatment Standards of § 268.42(c)

	Hazardous waste with the following EPA Hazardous Waste Codes may not be placed in lab packs under the alternative lab pack treatment standards of § 268.42(c): D009, F019, K003, K004, K005, K006, K062, K071, K100, K106, P010, P011, P012, P076, P078, U134, U151.

Appendix V to Part 268 [Removed]

	33. Appendix V to part 268 is removed and reserved.

Appendix X to Part 268 [Added]

	34. Appendix X to part 268 is added to read as follows:

Appendix X to Part 268-Recordkeeping, Notification, and/or Certification Requirements					
Entity	Scenario	Frequency	Recipient of notification	Recordkeeping, notification, and/or certification requirements	
I. Generator	A.	Waste does not meet applicable treatment standards or exceeds applicable prohibition levels (see § 268.7(a)(1)).	Each shipment	Treatment or storage facility.	Notice must include:
!EPA hazardous waste number.
!Constituents of concern.
!Treatability group.
!Manifest number.
!Waste analysis data (where available).	
	B.	Waste can be disposed of without further treatment (meets applicable treatment standards or does not exceed prohibition levels upon generation) (see § 268.7(a)(2)).	Each shipment	Land disposal facility	Notice and certification statement that waste meets applicable treatment standards or applicable prohibition levels.
Notice must include:
!EPA hazardous waste number.
!Constituents of concern.
!Treatability group.
!Manifest number.
!Waste analysis data (where available).
Certification statement required under § 268. 7(a)(2)(ii) that waste complies with treatment standards and prohibitions.	
	C.	Waste is subject to exemption from a prohibition on the type of land disposal utilized for the waste, such as a case_by_case extension under § 268.5, an exemption under § 268.6, or a nationwide capacity variance (see § 268.7(a)(3)).	Each shipment	Receiving facility	Notice must include:
!Statement that waste is not prohibited from land disposal.
!EPA hazardous waste number.
!Constituents of concern.
!Treatability group.
!Manifest number.
!Waste analysis data (where available).
!Date the waste is subject to the prohibitions.	
	D.	Waste is being accumulated in tanks or containers regulated under 40 CFR 262.34 and is being treated in such tanks or containers to meet applicable treatment standards (see § 268.7 (a)(4)).	Minimum of 30 days prior to treatment activity.	EPA Regional Administrator (or designated representative) or authorized State. Delivery must be verified.	Generator must develop, keep on_site, and follow a written waste analysis plan describing procedures used to comply with the treatment standards.
If waste is shipped off_site, generator also must comply with notification requirement of § 268.7(a)(2).	
	E.	Generator is managing a lab pack containing certain wastes and wishes to use an alternative treatment standard (see § 268.7(a)(8)).	Each shipment	Treatment facility	Notice in accordance with § 268.7(a) (1), (a)(5), and (a)(6), where applicable.
Certification in accordance with § 268.7(a)(8).	
	F.	Small quantity generators with tolling agreements (pursuant to 40 CFR 262.20(e)) (see §268.7(a)(9)).	Initial shipment	Treatment facility	Must comply with applicable notification and certification requirements in § 268.7(a).
Generator also must retain copy of the notification and certification together with tolling agreement on_site for at least 3 years after termination or expiration of agreement.	
	G.	Generator has determined waste is restricted based solely on his knowledge of the waste (see § 268.7(a)(5)).	N/A	Generator's file	All supporting data must be retained on_site in generator's files.	
	H.	Generator has determined waste is restricted based on testing waste or an extract (see § 268.7(a)(5))	N/A	Generator's file	All waste analysis data must be retained on_site in generator's files.	
	I.	Generator has determined that waste is excluded from the definition of hazardous or solid waste or exempt from Subtitle C regulation (see § 268.7(a)(6)).	One_time	Generator's file	Notice of generation and subsequent exclusion from the definition of hazardous or solid waste, or exemption from Subtitle C regulation, and information regarding the disposition of the waste.	
	J.	Generator (or treater) claims that hazardous debris is excluded from the definition of hazardous waste under 40 CFR 261.3(f)(1) (see § 268.7(d)).	One_time	EPA Regional Administrator or authorized State. Notification must be updated as necessary under § 268.7(d)(2).	Notice must include:
!Name and address of Subtitle D facility receiving treated debris.
!EPA hazardous waste number and description of debris as initially generated.
!Technology used to treat the debris (Table 1 of § 268.45).
Certification and recordkeeping in accordance with § 268.7(d)(3).	
	K.	Generator (or treater) claims that characteristic wastes are no longer hazardous (see § 268.9 (d)).	One_time	Generator's (or treater's) files and EPA Regional Administrator or authorized State. Notification must be updated as necessary under § 268.9(d).	Notice must include:
!Name and address of Subtitle D facility receiving the waste.
!EPA hazardous waste number and description of waste as initially generated.
!Treatability group.
!Underlying hazardous constituents.
Certification in accordance with § 268.9(d)(2).	
	L.	Other recordkeeping requirements (see § 268.7(a)(7)).	N/A	Generator's file	Generator must retain a copy of all 	notices, certifications, demonstrations, waste analysis data, and other documentation produced pursuant to § 268.7 on_site for at least 5 years from the date that the waste was last sent to on_site or off_site treatment, storage, or disposal. This period is automatically extended during enforcement actions or as requested by the Administrator.	
II. Treatment Facility	A.	Waste shipped from treatment facility to land disposal facility (see § 268.7(b)(4), (b)(5)).	Each shipment	Land disposal facility	Notice must include:
!EPA hazardous waste number.
!Constituents of concern.
!Treatability group.
!Manifest number.
!Waste analysis data (where available).
Application certification, in accordance with § 268.7(b)(5)(i), (ii) or (iii), stating that the waste or treatment residue has been treated in compliance with applicable treatment standards and prohibitions.	
	B.	Waste treatment residue from a treatment or storage facility will be further managed at a different treatment or storage facility (see § 268.7(b)(6)).	Each shipment	Receiving facility	Treatment, storage, or disposal facility must comply with all notice and certification requirements applicable to generators.	
 	C.	Where wastes are recyclable materials used in a manner constituting disposal subject to § 266.20(b) (see § 268.7(b)(7)).	Each shipment	Regional Administrator (or delegated representative).	No notification to receiving facility required pursuant to § 268.7(b)(4).
Certification as described in § 	268.7(b)(5) and notice with 	information listed in § 268.7(b)(4), except manifest number.
Recycling facility must keep records of the name and location of each entity receiving hazardous waste_derived products.	
III. Land Disposal Facility.	A.	Wastes accepted by land disposal facility (see § 268.7(c)).	N/A	N/A	Maintain copies of notice and certifications specified in § 268.7	(a) and (b).	

Certification Statements

	A. I certify under penalty of law that I personally have examined and am familiar with the waste through analysis and testing or through knowledge of the waste to support this certification that the waste complies with the treatment standards specified in 40 CFR part 268, subpart D and all applicable prohibitions set forth in 40 CFR 268.32 or RCRA section 3004(d). I believe that the information I submitted is true, accurate and complete. I am aware that there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment. (§ 268.7(a)(2)(ii))

	B. I certify under penalty of law that I personally have examined and am familiar with the waste and that the lab pack does not contain any wastes identified at § 268.42(c)(2). I am aware that there are significant penalties for submitting a false certification, including the possibility of fine or imprisonment. (§ 268.7(a)(8))

	C. I certify under penalty of law that I have personally examined and am familiar with the treatment technology and operation of the treatment process used to support this certification and that, based on my inquiry of those individuals immediately responsible for obtaining this information, I believe that the treatment process has been operated and maintained properly so as to comply with the performance levels specified in 40 CFR part 268, subpart D, and all applicable prohibitions set forth in 40 CFR 268.32 or RCRA section 3004(d) without impermissible dilution of the prohibited waste. I am aware that there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment. (§ 268.7(b)(5)(i))

	D. I certify under penalty of law that the waste has been treated in accordance with the requirements of 40 CFR 268.42. I am aware that there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment. (§ 268.7(b)(5)(ii))

	E. I certify under penalty of law that I have personally examined and am familiar with the treatment technology and operation of the treatment process used to support this certification and that, based on my inquiry of those individuals immediately responsible for obtaining this information, I believe that the nonwastewater organic constituents have been treated by incineration in units operated in accordance with 40 CFR part 264, subpart O or 40 CFR part 265, subpart O, or by combustion in fuel substitution units operating in accordance with applicable technical requirements, and I have been unable to detect the nonwastewater organic constituents, despite having used best good faith efforts to analyze for such constituents. I am aware that there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment. (§ 268.7(b)(5)(iii))

	F. I certify under penalty of law that the waste has been treated in accordance with the requirements of 40 CFR 268.40 to remove the hazardous characteristic. This decharacterized waste contains underlying hazardous constituents that require further treatment to meet universal treatment standards. I am aware that there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment. (§ 268.7(b)(5)(iv))

	G. I certify under penalty of law that the debris have been treated in accordance with the requirements of 40 CFR 268.45. am aware that there are significant penalties for making a false certification, including the possibility of fine and imprisonment. (§ 268.7(d)(3)(iii))

>>>> Part 271 has not been included because it is not required as part of a State's Hazardous Waste
Program. <<<<

[FR Doc. 94-22493 Filed 9-16-94; 8:45 am]
BILLING CODE 6560-50-P