Vol. 62 No. 91 Monday, May 12, 1997 p 25998

ENVIRONMENTAL PROTECTION AGENCY

40 CFR Parts 148, 261, 268, and 271

RIN 2050 AE05

[FRL 5816‑5]

Land Disposal Restrictions‑‑Phase IV: Treatment Standards for Wood Preserving Wastes, Paperwork Reduction and Streamlining, Exemptions From RCRA for Certain Processed Materials; and Miscellaneous Hazardous Waste Provisions

AGENCY: Environmental Protection Agency (EPA, the Agency).

ACTION: Final rule.

SUMMARY: The Agency is finalizing treatment standards for hazardous wastes generated from wood preserving operations, and is making a conforming amendment to the standard for wastes from production of chlorinated aliphatics which carry the F024 hazardous waste code.   These treatment standards will minimize threats to human health and the environment posed by these wastes. In addition, this final rule revises the land disposal restrictions (LDR) program to significantly reduce paperwork requirements by 1.6 million hours. This rule also finalizes both the decision to employ polymerization as an alternative method of treatment for certain ignitable wastes as well as the decision not to ban certain wastes from biological treatment because there is no need to classify these wastes as "nonamenable." It also clarifies an exception from LDR requirements for de minimis amounts of characteristic wastewaters. Finally, this rule excludes processed circuit boards and scrap metal from RCRA regulation which is intended to promote the goal of safe recycling.

EFFECTIVE DATE: This final rule is effective on August 11, 1997 except §§ 148.18(b) and 268.30(b), which are effective on May 12, 1999.

ADDRESSES: The public docket for this rulemaking is available for public inspection at EPA's RCRA Docket, located at Crystal Gateway, First Floor, 1235 Jefferson Davis Highway, Arlington, Virginia. The regulatory docket for this final rule contains a number of background materials. To obtain a list of these items, contact the RCRA Docket at 703‑603‑9230 and request the list of references in EPA Docket #F‑97‑PH4F‑FFFFF.

FOR FURTHER INFORMATION CONTACT: The RCRA Hotline between 9:00 a.m.‑6:00 p.m. EST, toll‑free, at 800‑424‑9346; (703) 412‑9810 from Government phones or if in the Washington, DC local calling area; or 800‑553‑7672 for the hearing impaired. For more detailed information on specific aspects of the rulemaking, contact the Waste Treatment Branch (5302W), Office of Solid Waste (OSW), U.S. Environmental Protection Agency, 401 M Street SW., Washington, DC 20460; phone (703) 308‑8434.  For technical information on the treatment standards for wood preserving wastes, ask for Nick Vizzone; for information on paperwork reduction and clean‑up of Part 268, call Rhonda Minnick at (703) 308‑8771 or Nick Vizzone at (703) 308‑8460. Contact Kristina Meson at (703) 308‑8488 for information on the exclusions for scrap metal and shredded circuit boards. Call Pan Lee at (703) 308‑8478 for information on the capacity analyses. For questions on the regulatory impact analyses, contact Paul Borst at (703) 308‑0481. For other questions, call Sue Slotnick at (703) 308‑8434.

>>>> The preamble has not been included in this file. <<<<

	For the reasons set out in the preamble, Title 40, chapter I of the Code of Federal Regulations is amended as follows:

>>>> Part 148 has not been included because it is not required as part of a State's Hazardous Waste Program. <<<<

PART 261‑‑IDENTIFICATION AND LISTING OF HAZARDOUS WASTE

Subpart A‑‑General

	3. The authority citation for part 261 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921, 6922, 6924(y), and 6938.
	4. Section 261.1 is amended by adding paragraphs (c) (9) through (12) to read as follows:

§ 261.1  Purpose and scope.
*   *   *   *   *
	(c) * * *
	(9) "Excluded scrap metal" is processed scrap metal, unprocessed home scrap metal, and unprocessed prompt scrap metal.
	(10) "Processed scrap metal" is scrap metal which has been manually or physically altered to either separate it into distinct materials to enhance economic value or to improve the handling of materials. Processed scrap metal includes, but is not limited to scrap
metal which has been baled, shredded, sheared, chopped, crushed, flattened, cut, melted, or separated by metal type (i.e., sorted), and, fines, drosses and related materials which have been agglomerated.  (Note: shredded circuit boards being sent for recycling are not considered processed scrap metal. They are covered under the exclusion from the definition of solid waste for shredded circuit boards being recycled (§ 261.4(a)(13)).
	(11) "Home scrap metal" is scrap metal as generated by steel mills, foundries, and refineries such as turnings, cuttings, punchings, and borings.
	(12) "Prompt scrap metal" is scrap metal as generated by the metal working/fabrication industries and includes such scrap metal as turnings, cuttings, punchings, and borings. Prompt scrap is also known as industrial or new scrap metal.
	5. Section 261.2(c) is amended by revising table 1 to read as follows:

§ 261.2  Definition of solid waste.
*   *   *   *   *
	(c) * * *
Table 1
	Use constitu-ting disposal (§261.2(c)(1))

(1)	Energy recovery/fuel (§261.2(c)(2))

(2)	
Reclamation (§261.2(c)(3))

(3)	Speculative accumulation (§261.2(c)(4))

(4)	
Spent Materials		(*)	(*)	(*)	(*)	
Sludges (listed in 40 CFR Part 261.31 or 261.32		(*)	(*)	(*)	(*)	
Sludges exhibiting a characteristic of hazardous waste		(*)	(*)	...............	(*)	
By‑products (listed in 40 CFR 261.31 or 261.32)		(*)	(*)	(*)	(*)	
By‑products exhibiting a characteristic of hazardous waste		(*)	(*)	...............	(*)	
Commercial chemical products listed in 40 CFR 261.33		(*)	(*)	...............	...............	
Scrap metal other than excluded scrap metal (see 261.1(c)(9))		(*)	(*)	(*)	(*)	

Note: The terms "spent materials", "sludges", "by‑products", and "scrap metal" and "processed scrap metal" are defined in §261.1.

*   *   *   *   *

	6. Section 261.4(a) is amended by adding paragraphs (a) (13) and (14) to read as follows:

§ 261.4  Exclusions.
	(a) * * *
	(13) Excluded scrap metal (processed scrap metal, unprocessed home scrap metal, and unprocessed prompt scrap metal) being recycled. 
	(14) Shredded circuit boards being recycled provided that they are:
	(i) Stored in containers sufficient to prevent a release to the environment prior to recovery; and
	(ii) Free of mercury switches, mercury relays and nickel‑cadmium batteries and lithium batteries.
*   *   *   *   *

	7. Section 261.6 is amended by revising paragraph (a)(3)(ii) to read as follows:

§ 261.6  Requirements for recyclable materials.
	(a) * * *
	(3) * * *
	(ii) Scrap metal that is not excluded under § 261.4(a)(13);
*   *   *   *   *

PART 268‑‑LAND DISPOSAL RESTRICTIONS

	8. The authority citation for part 268 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921, and 6924.

Subpart A‑‑General

	9. Section 268.1 is amended by revising paragraph (e) to read as follows:

§ 268.1  Purpose, scope and applicability.

*   *   *   *   *
	(e) The following hazardous wastes are not subject to any provision of part 268:
	(1) Waste generated by small quantity generators of less than 100 kilograms of non‑acute hazardous waste or less than 1 kilogram of acute hazardous waste per month, as defined in § 261.5 of this chapter;
	(2) Waste pesticides that a farmer disposes of pursuant to § 262.70;
	(3) Wastes identified or listed as hazardous after November 8, 1984 for which EPA has not promulgated land disposal prohibitions or treatment standards;
	(4) De minimis losses of characteristic wastes to wastewaters are not considered to be prohibited wastes and are defined as losses from normal material handling operations (e.g. spills from the unloading or transfer of materials from bins or other containers, leaks from pipes, valves or other devices used to transfer materials); minor leaks of process equipment, storage tanks or containers; leaks from well‑maintained pump packings and seals; sample purgings; and relief device discharges; discharges from safety showers and rinsing and cleaning of personal safety equipment; rinsate from empty containers or from containers that are rendered empty by that rinsing; and laboratory wastes not exceeding one per cent of the total flow of wastewater into the facility's headworks on an annual basis, or with a combined annualized average concentration not exceeding one part per million in the headworks of the facility's wastewater treatment or pretreatment facility.
*   *   *   *   *

	10. Section 268.4 is amended by revising paragraphs (a)(2)(iv), and (a)(4) introductory text to read as follows:

§ 268.4  Treatment surface impoundment exemption.
	(a) * * *
	(2) * * *
	(iv) Recordkeeping: Sampling and testing and recordkeeping provisions of §§ 264.13 and 265.13 of this chapter apply.
*   *   *   *   *

	(4) The owner or operator submits to the Regional Administrator a written certification that the requirements of § 268.4(a)(3) have been met. The following certification is required:
*   *   *   *   *

	11. Section 268.7 is amended by revising the section heading: revising paragraph (a); by removing paragraph (b)(2) and redesignating paragraphs (b)(3) through (b)(7) as (b)(2) through (b)(6) respectively; and by revising the introductory text of paragraph (b), and revising paragraphs (b)(1), newly designated paragraphs (b)(2) through (b)(4), (c)(1), and (c)(2) to read as follows:

§ 268.7  Testing, tracking, and recordkeeping requirements for generators, treaters, and disposal facilities.

	(a) Requirements for generators: (1) Determine if the waste has to be treated before being land disposed, as follows: A generator of a hazardous waste must determine if the waste has to be treated before it can be land disposed. This is done by determining if the hazardous waste meets the treatment standards in § 268.40 or § 268.45. This determination can be made in either of two ways: testing the waste or using knowledge of the waste. If the generator tests the waste, testing would normally determine the total concentration of hazardous constituents, or the concentration of hazardous constituents in an extract of the waste obtained using test method 1311 in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods," EPA Publication SW‑846, as referenced in § 260.11 of this chapter, depending on whether the treatment standard for the waste is expressed as a total concentration or concentration of hazardous constituent in the waste's extract. In addition, some hazardous wastes must be treated by particular treatment methods before they can be land disposed. These treatment standards are also found in § 268.40, and are described in detail in § 268.42, Table 1. These wastes do not need to be tested (however, if they are
in a waste mixture, other wastes with concentration level treatment standards would have to be tested). If a generator determines they are managing a waste that displays a hazardous characteristic of ignitability, corrosivity, reactivity, or toxicity, they must comply with the special requirements of § 268.9 of this part in addition to any applicable requirements in this section.  
	(2) If the waste does not meet the treatment standard: With the initial shipment of waste to each treatment or storage facility, the generator must send a one‑time written notice to each treatment or storage facility receiving the waste, and place a copy in the file. The notice must include the information in column "268.7(a)(2)" of the Generator Paperwork Requirements Table in § 268.7(a)(4). No further notification is necessary until such time that the waste or facility change, in which case a new notification must be sent and a copy placed in the generator's file.
	(3) If the waste meets the treatment standard at the original point of generation:
	(i) With the initial shipment of waste to each treatment, storage, or disposal facility, the generator must send a one‑time written notice to each treatment, storage, or disposal facility receiving the waste, and place a copy in the file. The notice must include the information indicated in column "268.7(a)(3)" of the Generator Paperwork Requirements Table in § 268.7(a)(4) and the following certification statement, signed by an authorized representative:

	I certify under penalty of law that I personally have examined and am familiar with the waste through analysis and testing or through knowledge of the waste to support this certification that the waste complies with the treatment standards specified in 40 CFR part 268 subpart D. I believe that the information I submitted is true, accurate, and complete. I am aware that there are significant penalties for submitting a false certification, including the possibility of a fine and imprisonment.

	(ii) If the waste changes, the generator must send a new notice and certification to the receiving facility, and place a copy in their files. Generators of hazardous debris excluded from the definition of hazardous waste under § 261.3(f) of this chapter are not subject to  these requirements.
	(4) For reporting, tracking and recordkeeping when exceptions allow certain wastes that do not meet the treatment standards to be land disposed: There are certain exemptions from the requirement that hazardous wastes meet treatment standards before they can be land disposed. These include, but are not limited to case‑by‑case extensions under § 268.5, disposal in a no‑migration unit under § 268.6, or a national capacity variance or case‑by‑case capacity variance under subpart C of this part. If a generator's waste is so exempt, then with the initial shipment of waste, the generator must send a one‑time written notice to each land disposal facility receiving the waste. The notice must include the information indicated in column "268.7(a)(4)" of the Generator Paperwork Requirements Table below. If the waste changes, the generator must send a new notice to the receiving facility, and place a copy in their files.

Generator Paperwork Requirements Table
Require information	§268.7
(a)(2)	§268.7
(a)(3)	§268.7
(a)(4)	§268.7
(a)(9)	
1. EPA Hazardous Waste and Manifest numbers	T	T	T	T	
2. Statement: this waste is not prohibited from land disposal			T		
3. The waste is subject to the LDRs. The constituents of concern for F001‑F005, and F039, and underlying hazardous constituents (for wastes that are not managed in a Clean Water Act (CWA) or CWA‑equivalent facility), unless the waste will be treated and monitored for all  constituents. If all constituents will be treated and monitored, there is no need to put them all on the LDR notice	T	T			
4. The notice must include the applicable wastewater/nonwastewater category (see §§ 268.2(d) and (f)) and subdivisions made within a waste code based on waste‑specific criteria (such as D003 reactive cyanide)	T	T			
5. Waste analysis data (when available)	T	T	T		
6. Date the waste is subject to the prohibition			T		
7. For hazardous debris, when treating with the alternative treatment technologies provided by § 268.45: the contaminants subject to treatment, as described in § 268.45(b); and an indication that these contaminants are being treated to comply with § 268.45 	T		T		
8. A certification is needed (see applicable section for exact wording)		T		T	

	(5) If a generator is managing and treating prohibited waste in tanks, containers, or containment buildings regulated under 40 CFR 262.34 to meet applicable LDR treatment standards found at § 268.40, the generator must develop and follow a written waste analysis plan which describes the procedures they will carry out to comply with the treatment standards. (Generators treating hazardous debris under the alternative treatment standards of Table 1, § 268.45, however, are not subject to these waste analysis requirements.) The plan must be kept on site in the generator's records, and the following requirements must be met:
	(i) The waste analysis plan must be based on a detailed chemical and physical analysis of a representative sample of the prohibited waste(s) being treated, and contain all information necessary to treat the waste(s) in accordance with the requirements of this part, including the selected testing frequency.
	(ii) Such plan must be kept in the facility's on‑site files and made available to inspectors.
	(iii) Wastes shipped off‑site pursuant to this paragraph must comply with the notification requirements of § 268.7(a)(3). 
	(6) If a generator determines that the waste is restricted based solely on his knowledge of the waste, all supporting data used to make this determination must be retained on‑site in the generator's files.  If a generator determines that the waste is restricted based on testing this waste or an extract developed using the test method 1311 in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods," EPA Publication SW‑846, as referenced in § 260.11 of this chapter, and all waste analysis data must be retained on‑site in the generator's files.
	(7) If a generator determines that he is managing a restricted waste that is excluded from the definition of hazardous or solid waste or exempt from Subtitle C regulation, under 40 CFR 261.2 through 261.6 subsequent to the point of generation (including deactivated characteristic hazardous wastes managed in wastewater treatment systems subject to the Clean Water Act (CWA) as specified at 40 CFR 261.4(a)(2), or are CWA‑equivalent), he must place a one‑time notice stating such generation, subsequent exclusion from the definition of hazardous or solid waste or exemption from RCRA Subtitle C regulation, and the disposition of the waste, in the facility's file.
	(8) Generators must retain on‑site a copy of all notices, certifications, waste analysis data, and other documentation produced pursuant to this section for at least three years from  the date that the waste that is the subject of such documentation was last sent to on‑site or off‑site treatment, storage, or disposal. The three year record retention period is automatically extended during the course of any unresolved enforcement action regarding the regulated activity or as requested by the Administrator. The requirements of this paragraph apply to solid wastes even when the hazardous characteristic is removed prior to disposal, or when the waste is excluded from the definition of hazardous or solid waste under 40 CFR 261.2 through 261.6, or exempted from Subtitle C regulation, subsequent to the point of generation.
	(9) If a generator is managing a lab pack containing hazardous wastes and wishes to use the alternative treatment standard for lab packs found at § 268.42(c):
	(i) With the initial shipment of waste to a treatment facility, the generator must submit a notice that provides the information in column "§ 268.7(a)(9)" in the Generator Paperwork Requirements Table of paragraph (a)(4) of this section, and the following certification. The certification, which must be signed by an authorized representative and must be placed in the generator's files, must say the following:

	I certify under penalty of law that I personally have examined and am familiar with the waste and that the lab pack contains only wastes that have not been excluded under appendix IV to 40 CFR part 268 and that this lab pack will be sent to a combustion facility in compliance with the alternative treatment standards for lab packs at 40 CFR 268.42(c). I am aware that there are significant penalties for submitting a false certification, including the possibility of fine or imprisonment.

	(ii) No further notification is necessary until such time that the wastes in the lab pack change, or the receiving facility changes, in which case a new notice and certification must be sent and a copy placed in the generator's file.
	(iii) If the lab pack contains characteristic hazardous wastes (D001‑D043), underlying hazardous constituents (as defined in § 268.2(i)) need not be determined.
	(iv) The generator must also comply with the requirements in paragraphs (a)(6) and (a)(7) of this section.
	(10) Small quantity generators with tolling agreements pursuant to 40 CFR 262.20(e) must comply with the applicable notification and certification requirements of paragraph (a) of this section for the initial shipment of the waste subject to the agreement. Such generators must retain on‑site a copy of the notification and certification, together with the tolling agreement, for at least three years after termination or expiration of the agreement. The three‑year record retention period is automatically extended during the course of any unresolved enforcement action regarding the regulated activity or as requested by the Administrator.
	(b) Treatment facilities must test their wastes according to the frequency specified in their waste analysis plans as required by 40 CFR 264.13 (for permitted TSDs) or 40 CFR  265.13 (for interim status facilities). Such testing must be performed as provided in paragraphs (b)(1), (b)(2) and (b)(3) of this section.
	(1) For wastes with treatment standards expressed as concentrations in the waste extract (TCLP), the owner or operator of the treatment facility must test an extract of the treatment residues, using test method 1311 (the Toxicity Characteristic Leaching Procedure, described in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods," EPA Publication SW‑846 as incorporated by reference in § 260.11 of this chapter), to assure that the treatment residues extract meet the applicable treatment standards.
	(2) For wastes with treatment standards expressed as concentrations in the waste, the owner or operator of the treatment facility must test the treatment residues (not an extract of such residues) to assure that they meet the applicable treatment standards.
	(3) A one‑time notice must be sent with the initial shipment of waste to the land disposal facility. A copy of the notice must be placed in the treatment facility's file.
	(i) No further notification is necessary until such time that the waste or receiving facility change, in which case a new notice must be sent and a copy placed in the treatment facility's file. 
	(ii) The one‑time notice must include these requirements:

Treatment Facility Paperwork Requirements Table
Required information	§268.7(b)	
1. EPA Hazardous Waste and Manifest numbers		T	
2. The waste is subject to the LDRs. The constituents of concern for F001‑F005, and F039, and underlying hazardous constituents (for wastes that are not managed in a Clean Water Act (CWA) or CWA‑equivalent facility), unless the waste will be treated and monitored for all constituents. If all constituents will be treated and monitored, there is no need to put them all on the LDR notice		T	
3. The notice must include the applicable wastewater/nonwastewater category (see §§ 268.2(d) and (f)) and subdivisions made within a waste code based on waste‑specific criteria (such as D003 reactive cyanide)		T	
4. Waste analysis data (when available)		T	
5. A certification statement is needed (see applicable section for exact wording)		T	

	(4) The treatment facility must submit a one‑time certification signed by an authorized representative with the initial shipment of waste or treatment residue of a restricted waste to the land disposal facility. The certification must state:

	I certify under penalty of law that I have personally examined and am familiar with the treatment technology and operation of the treatment process used to support this certification. Based on my inquiry of those individuals immediately responsible for obtaining this information, I believe that the treatment process has been operated and maintained properly so as to comply with the treatment standards specified in 40 CFR 268.40 without impermissible dilution of the prohibited waste. I am aware there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment.

	(i) A copy of the certification must be placed in the treatment facility's on‑site files. If the waste or treatment residue changes, or the receiving facility changes, a new certification must be sent to the receiving facility, and a copy placed in the file.
	(ii) Debris excluded from the definition of hazardous waste under § 261.3(e) of this chapter (i.e., debris treated by an extraction or destruction technology provided by Table 1, § 268.45, and debris that the Director has determined does not contain hazardous waste), however, is subject to the notification and certification requirements of paragraph (d) of this section rather than the certification requirements of this paragraph.
	(iii) For wastes with organic constituents having treatment standards expressed as concentration levels, if compliance with the treatment standards is based in whole or in part on the analytical detection limit alternative specified in § 268.40(d), the certification, signed by an authorized representative, must state the following:

	I certify under penalty of law that I have personally examined and am familiar with the treatment technology and operation of the treatment process used to support this certification. Based on my inquiry of those individuals immediately responsible for obtaining this information, I believe that the nonwastewater organic constituents have been treated by combustion units as specified in 268.42, Table 1. I have been unable to detect the nonwastewater organic constituents, despite having used best good‑faith efforts to analyze for such constituents. I am aware there are significant penalties for submitting a false certification, including the possibility of fine and imprisonment.
*   *   *   *   *

	(c) * * *
	(1) Have copies of the notice and certifications specified in paragraph (a) or (b) of this section.
	(2) Test the waste, or an extract of the waste or treatment residue developed using test method 1311 (the Toxicity Characteristic Leaching Procedure), described in "Test Methods  for Evaluating Solid Waste, Physical/Chemical Methods," EPA Publication SW‑846 as incorporated by reference in § 260.11 of this chapter), to assure that the wastes or treatment residues are in compliance with the applicable treatment standards set forth in subpart D of this part. Such testing must be performed according to the frequency specified in the facility's waste analysis plan as required by § 264.13 or § 265.13 of this chapter.
*   *   *   *   *

	12. Section 268.9 is amended by revising paragraph (a) and (d)(1)(ii) to read as follows:

§ 268.9  Special rules regarding wastes that exhibit a characteristic.

	(a) The initial generator of a solid waste must determine each EPA Hazardous Waste Number (waste code) applicable to the waste in order to determine the applicable treatment standards under subpart D of this part. For purposes of part 268, the waste will carry the waste code for any applicable listed waste (Part 261, Subpart D). In addition, where the waste exhibits a characteristic, the waste will carry one or more of the characteristic waste codes (Part 261, Subpart C), except when the treatment standard for the listed waste operates in lieu of the treatment standard for the characteristic waste, as specified in paragraph (b) of this section. If the generator determines that their waste displays a hazardous characteristic (and is not D001 nonwastewaters treated by CMBST, RORGS, OR POLYM of § 268.42, Table 1), the generator must determine the underlying hazardous constituents (as defined at § 268.2(i)) in the characteristic waste.
*   *   *   *   *

	(d) * * *
	(1) * * *
	(ii) A description of the waste as initially generated, including the applicable EPA  hazardous waste code(s), treatability group(s), and underlying hazardous constituents (as defined in § 268.2(i)), unless the waste will be treated and monitored for all underlying hazardous constituents. If all underlying hazardous constituents will be treated and monitored, there is no requirement to list any of the underlying hazardous constituents on the notice.
*   *   *   *   *

Subpart C‑‑Prohibitions on Land Disposal

	13. Section 268.30 is revised to read as follows:

§ 268.30  Waste specific prohibitions‑‑wood preserving wastes.

(a) Effective August 11, 1997, the following wastes are prohibited from land disposal: the wastes specified in 40 CFR part 261 as EPA Hazardous Waste numbers F032, F034, and F035.
	(b) Effective May 12, 1999, the following wastes are prohibited from land disposal:  soil and debris contaminated with F032, F034, F035; and radioactive wastes mixed with EPA Hazardous waste numbers F032, F034, and F035.
	(c) Between May 12, 1997 and May 12, 1999, soil and debris contaminated with F032, F034, F035; and radioactive waste mixed with F032, F034, and F035 may be disposed in a landfill or surface impoundment only if such unit is in compliance with the requirements specified in § 268.5(h)(2) of this part.
	(d) The requirements of paragraphs (a) and (b) of this section do not apply if:
	(1) The wastes meet the applicable treatment standards specified in Subpart D of this part;
	(2) Persons have been granted an exemption from a prohibition pursuant to a petition under § 268.6, with respect to those wastes and units covered by the petition;
	(3) The wastes meet the applicable alternate treatment standards established pursuant to a petition granted under § 268.44; or 
	(4) Persons have been granted an extension to the effective date of a prohibition pursuant to § 268.5, with respect to those wastes covered by the extension.
	(e) To determine whether a hazardous waste identified in this section exceeds the applicable treatment standards specified in § 268.40, the initial generator must test a sample of the waste extract or the entire waste, depending on whether the treatment standards are expressed as concentrations in the waste extract or the waste, or the generator may use knowledge of the waste. If the waste contains constituents in excess of the applicable Universal Treatment Standard levels of § 268.48 of this part, the waste is prohibited from land disposal, and all requirements of part 268 are applicable, except as otherwise specified.   
§§ 268.32, 268.33, 268.34, 268.35 and 286.36 [Removed and Reserved]

	14. Sections 268.32, 268.33, 268.34, 268.35, and 268.36 are removed and reserved.

Subpart D‑‑Treatment Standards

	15. In § 268.40 the Table of Treatment Standards is amended by adding, in alpha‑numerical order, entries for F032, F034, and F035, and revising entries for D001, F024 to read as follows:

§ 268.40  Applicability of treatment standards.

*   *   *   *   *

Treatment Standards for Hazardous Wastes
[Note: NA means not applicable]
		Regulated hazardous constituent			Wastewaters		Nonwastewaters	
Waste code	Waste description and treatment/regulatory subcategory1	Common name	CAS2 No.		Concentration in mg/l3; or technology code4		Concentration in mg/kg5 unless noted as "mg/l TCLP"; or tech-nology code	
D0019	High TOC Ignitable characteristic  Liquids Subcategory based on 40 CFR 261.21(a)(1)‑‑Greater than or equal to 10% total organic carbon. (Note: This subcategory consists of nonwastewaters only.).	NA		NA		NA			RORGS; CMBST; OR POLYM	
*		*		*		*		*		*								
F024	Process wastes, including but not limited to, distillation residues, heavy ends, tars, and reactor clean‑out wastes, from the production of certain chlorinated aliphatic hydrocarbons by free radical catalyzed processes. These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging  from one to and including five, with varying amounts and positions of chlorine substitution.  (This listing does not include wastewaters, wastewater treatment sludges, spent catalysts, and wastes listed in § 261.31 or § 261.32.).	All F024 wastes	
2‑Chloro‑1,3‑butadiene	
3‑Chloropropylene	
1,1‑Dichloroethane	
1,2‑Dichloroethane	
1,2‑Dichloropropane	
cis‑1,3‑Dichloropropylene	
trans‑1,3‑Dichloropropylene	
bis(2‑Ethylhexyl) phthalate	
Hexachloroethane	
Chromium (Total)	
Nickel		NA
126‑99‑8
107‑05‑1
75‑34‑3
107‑06‑2
78‑87‑5
10061‑01‑5
10061‑02‑6
117‑81‑7
67‑72‑1
7440‑47‑3
7440‑02‑0		CMBST11	
0.057	
0.036	
0.059	
0.21	
0.85	
0.036	
0.036	
0.28	
0.055	
2.77	
3.98			CMBST11
0.28
30
6.0
6.0
18
18
18
28
30
0.86 mg/l TCLP
5.0 mg/l TCLP	
*		*		*		*		*		*								
F032	Wastewaters (except those that have not come into contact with process contaminants), process residuals, preservative drippage, and spent formulations from wood preserving processes generated at plants that currently use or have previously used chlorophenolic formulations (except potentially cross‑ contaminated wastes that have had the F032 waste code deleted in accordance with § 261.35 of this chapter or potentially cross‑contaminated wastes that are otherwise currently regulated as hazardous wastes (i.e., F034 or F035), and where the generator does not resume or initiate use of chlorophenolic formulations).  This listing does not include K001 bottom sediment sludge from the treatment of wastewater from wood preserving processes that use creosote and/or penta‑ chlorophenol.	Acenaphthene	
Anthracene	
Benz(a)anthracene	
Benzo(b)fluoranthene	
  (difficult to distinguish
  from benzo(k)
  fluoranthene) Benzo(k)fluoranthene	
  (difficult to distinguish
  from benzo(b)
  fluoranthene)
Benzo(a)pyrene	
Chrysene	
Dibenz(a,h)anthracene	
2‑4‑Dimethyl phenol	
Fluorene	
Hexaclorodibenzo‑p‑dioxins	
Hexachlorodibenzofurans	
Indeno (1,2,3‑c,d) pyrene	
Naphthalene	
Pentachlorodibenzo‑p‑dioxins	
Pentachlorodibenzofurans	
Pentachlorophenol	
Phenanthrene	
Phenol	
Pyrene	
Tetrachlorodibenzo‑p‑dioxins	
Tetrachlorodibenzofurans	
2,3,4,6‑Tetrachlorophenol	
2,4,6‑Trichlorophenol	
Arsenic	
Chromium (Total)		83‑32‑9
120‑12‑7
56‑55‑3
205‑99‑2

207‑08‑9

50‑32‑8
218‑01‑9
53‑70‑3
105‑67‑9
86‑73‑7
NA
NA
193‑39‑5
91‑20‑3
NA
NA
87‑86‑5
85‑01‑8
108‑95‑2
129‑00‑0
NA
NA
58‑90‑2
88‑06‑2
7440‑38‑2
7440‑47‑3		0.059	
0.059	
0.059	
0.11	

0.11	

0.061	
0.059	
0.055	
0.036	
0.059	
0.000063 or CMBST11	
0.000063 or CMBST11	 
0.0055	
0.059	
0.000063 or CMBST11	
0.000035 or CMBST11	
0.089	
0.059	
0.039	
0.067	
0.000063 or CMBST11	
0.000063 or CMBST11	
0.030	
0.035	
1.4	
2.77			3.4
3.4
3.4
6.8

6.8

3.4
3.4
8.2
14
3.4
0.001 or CMBST11
0.001 or CMBST11
3.4
5.6
0.001 or CMBST11
0.001 or CMBST11
7.4
5.6
6.2
8.2
0.001 or CMBST11
0.001 or CMBST11
7.4
7.4
5.0 mg/l TCLP
0.86 mg/l TCLP	
F034	Wastewaters (except those that have not come into contact with process contaminants), process residuals, preservative drippage, and spent formulations from wood preserving processes generated at plants that use creosote formulations. This listing does not include K001 bottom sediment sludge from the treatment of wastewater from wood preserving processes that use creosote and/or pentachlorophenol.	Acenaphthene	
Anthracene	
Benz(a)anthracene	
Benzo(b)fluoranthene	
  (difficult to
  distinguish from
  benzo(k)fluoranthene).
Benzo(k)fluoranthene	
  (difficult to
  distinguish from
  benzo(b)fluoranthene). 
Benzo(a)pyrene	
Chrysene	
Dibenz(a,h)anthracene	
Fluorene	
Indeno (1,2,3‑c,d) pyrene	
Naphthalene	
Phenanthrene	
Pyrene	
Arsenic	
Chromium (Total)		83‑32‑9
120‑12‑7
56‑55‑3
205‑99‑2

207‑08‑9

50‑32‑8
218‑01‑9
53‑70‑3
86‑73‑7
193‑39‑5
91‑20‑3
85‑01‑8
129‑00‑0
7440‑38‑2
7440‑47‑3		0.059	
0.059	
0.059	
0.11	

0.11	

0.061	
0.059	
0.055	
0.059	
0.0055	
0.059	
0.059	
0.067	
1.4	
2.77			3.4
3.4
3.4
6.8

6.8

3.4
3.4
8.2
3.4
3.4
5.6
5.6
8.2
5.0 mg/l TCLP
0.86 mg/l TCLP	
F035	Wastewaters (except those that have not come into contact with process contaminants), process residuals, preservative drippage, and spent formulations from wood preserving processes processes generated at plants that use inorganic preservatives containing arsenic or chromium. This listing does not include K001 bottom sediment sludge from the treatment of wastewater from wood preserving processes that use creosote and/or pentachlorophenol.	Arsenic	
Chromium (Total)		7440‑38‑2
7440‑47‑3		1.4	
2.77			5.0 mg/l TCLP
0.86 mg/l TCLP	
*		*		*		*		*		*								

FOOTNOTES TO TREATMENT STANDARDS TABLE 268.40:
1   The waste descriptions provided in this table do not replace waste descriptions in 40 CFR part 261. Descriptions of Treatment/Regulatory Subcategories are provided, as needed, to distinguish between applicability of different standards.
2   CAS means Chemical Abstract Services. When the waste code and/or regulated constituents are described as a combination of a chemical with its salts and/or esters, the CAS number is given for the parent compound only.
3   Concentration standards for wastewaters are expressed in mg/l and are based on analysis of composite samples.
4   All treatment standards expressed as a Technology Code or combination of Technology Codes are explained in detail in § 268.42 Table 1‑‑Technology Codes and Descriptions of Technology‑Based Standards.
5   Except for Metals (EP or TCLP) and Cyanides (Total and Amenable) the nonwastewater treatment standards expressed as a concentration were established, in part, based upon incineration in units operated in accordance with the technical requirements of 40 CFR part 264, subpart O, or part 265, subpart O, or based upon combustion in fuel substitution units operating in accordance with applicable technical requirements. A facility may comply with these treatment standards according to provisions in § 268.40(d). All concentration standards for nonwastewaters are based on analysis of grab samples.
6   Where an alternate treatment standard or set of alternate standards has been indicated, a facility may comply with this alternate standard, but only for the Treatment/Regulatory Subcategory or physical form (i.e., wastewater and/or nonwastewater) specified for that alternate standard. 
7   Both Cyanides (Total) and Cyanides (Amenable) for nonwastewaters are to be analyzed using Method 9010 or 9012, found in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods", EPA Publication SW‑846, as incorporated by reference in 40 CFR 260.11, with a sample size of 10 grams and a distillation time of one hour and 15 minutes.
8   These wastes, when rendered nonhazardous and then subsequently managed in CWA, or CWA‑equivalent systems are not subject to treatment standards. (See § 268.1(c) (3) and (4)).
9   These wastes, when rendered nonhazardous and then subsequently injected in a Class I SDWA well are not subject to treatment standards. (See 40 CFR part 148.1(d)).
10  Between August 26, 1996, and August 26, 1997, the treatment standard for this waste may be satisfied by either meeting the constituent concentrations in this table or by treating the waste by the specified technologies: combustion, as defined by the technolgy code CMBST at §268.42 Table 1 of this part, for nonwastewaters; and, biodegradation as definded by the technolgy code BIODG, carbon adsorption as defined by the technology code CARBN, chemical oxidation as defined by the technology code CHOXD, or combustion as defined as technolgy code CMBST at § 268.42 Table 1 of this part, for wastewaters.
11  For these wastes, the definition of CMBST is limited to: (1) combustion units operating under 40 CFR 266, (2) combustion units permitted under 40 CFR Part 264, Subpart O, or (3) combustion units operating under 40 CFR 265, Subpart O, which have obtained a determination of equivalent treatment under 268.42(b).
*   *   *   *   *

§ 268.42  [Amended]

	16. Section 268.42 is amended by adding the entry "POLYM" into Table 1.‑‑ Technology Codes and Description of Technology‑Based
Standards, in alphabetical order, to read as follows:
*   *   *   *   *

Table 1.‑‑Technology Codes and Description of Technology‑Based Standards
Technology code	Description of technology-based standards	
*		*		*		*		*		*		
POLYM:		Formation of complex high‑molecular weight solids through polymerization of monomers in
   high‑TOC D001 non‑wastewaters which are chemical components in the manufacture of
   plastics.	
*		*		*		*		*		*		
*   *   *   *   *

	17. Section 268.44 is amended by revising both entries in the "see also" column of the table in paragraph (o) to read "§ 268.40" and by revising the introductory language of paragraph (o) and the heading of the table in paragraph (o) to read as follows:

§ 268.44  Variance from a treatment standard.
*   *   *   *   *

	(o) The following facilities are excluded from the treatment standards under § 268.40 and are subject to the following constituent concentrations:

	Table‑‑Wastes Excluded from the Treatment Standards Under § 268.40.
*   *   *   *   *

Appendices I, II, III, and X to Part 268 [Removed and Reserved]

	18. Appendices I, II, III, and X to part 268 are removed and reserved.
	19. The introductory language of appendix VI to part 268 is revised to read as follows:

Appendix VI to Part 268‑‑Recommended Technologies to Achieve Deactivation of Characteristics in Section 268.42

	The treatment standard for many characteristic wastes is stated in the § 268.40 Table of Treatment Standards as "Deactivation and meet UTS."  EPA has determined that many technologies, when used alone or in combination, can achieve the deactivation portion of the treatment standard. Characteristic wastes that are not managed in a facility regulated by the Clean Water Act (CWA) or in a CWA‑equivalent facility, and that also contain underlying hazardous constituents (see § 268.2(i)) must be treated not only by a "deactivating" technology to remove the characteristic, but also to achieve the universal treatment standards (UTS) for underlying hazardous constituents. The following appendix presents a partial list of technologies, utilizing the five letter technology codes established in 40 CFR 268.42 Table 1, that may be useful in meeting the treatment standard. Use of these specific technologies is not mandatory and does not preclude direct reuse, recovery, and/or the use of other pretreatment technologies, provided deactivation is achieved and underlying hazardous constituents are treated to achieve the UTS.
*   *   *   *   *

	20. Appendix VII to Part 268 is revised to read as follows:

Appendix VII to Part 268‑‑LDR Effective Dates of Surface Disposed Prohibited Hazardous Wastes

Table 1.‑‑Effective Dates of Surface Disposed Wastes (Non‑Soil and Debris) Regulated in the LDRSa‑‑Comprehensive List
Waste code	Waste category	Effective date	
D001c		All (except High TOC Ignitable Liquids)		Aug. 9, 1993.	
D001		High TOC Ignitable Liquids		Aug. 8, 1990.	
D002c		All		Aug. 9, 1993.	
D003e		All		July 8, 1996.	
D004		Nonwastewater		May 8, 1992.	
D004		Wastewater		Aug. 8, 1992.	
D005		All		Aug. 8, 1990.	
D006		All		Aug. 8, 1990.	
D007		All		Aug. 8, 1990.	
D008		Lead materials before secondary smelting		May 8, 1992.	
D008	 	All others		Aug. 8, 1990.	
D009		Nonwastewater		May 8, 1992.	
D009		All others		Aug. 8, 1990.	
D010		All	 	Aug. 8, 1990.	
D011		All	 	Aug. 8, 1990.	
D012 (that exhibit the toxicity characteristic based on the TCLP)d		All		Dec. 14, 1994.	
D013 (that exhibit the toxicity  characteristic based on the TCLP)d		All		Dec. 14, 1994.	
D014 (that exhibit the toxicity  characteristic based on the TCLP)d		All		Dec. 14, 1994.	
D015 (that exhibit the toxicity  characteristic based on the TCLP)d		All		Dec. 14, 1994.	
D016 (that exhibit the toxicity  characteristic based on the TCLP)d		All		Dec. 14, 1994.	
D017 (that exhibit the toxicity  characteristic based on the TCLP)d		All		Dec. 14, 1994.	
D018		Mixed with radioactive wastes		Sept. 19, 1996.	
D018		All others		Dec. 19, 1994.	
D019		Mixed with radioactive wastes		Sept. 19, 1996.	
D019		All others		Dec. 19, 1994.	
D020		Mixed with radioactive wastes		Sept. 19, 1996.	
D020		All others		Dec. 19, 1994.	
D021		Mixed with radioactive wastes		Sept. 19, 1996.	
D021		All others		Dec. 19, 1994.	
D022		Mixed with radioactive wastes		Sept. 19, 1996.	
D022		All others		Dec. 19, 1994.	
D023		Mixed with radioactive wastes		Sept. 19, 1996.	
D023		All others		Dec. 19, 1994.	
D024		Mixed with radioactive wastes		Sept. 19, 1996.	
D024		All others		Dec. 19, 1994.	
D025		Mixed with radioactive wastes		Sept. 19, 1996.	
D025		All others		Dec. 19, 1994.	
D026		Mixed with radioactive wastes		Sept. 19, 1996.	
D026		All others		Dec. 19, 1994.	
D027		Mixed with radioactive wastes		Sept. 19, 1996.	
D027		All others		Dec. 19, 1994.	
D028		Mixed with radioactive wastes		Sept. 19, 1996.	
D028		All others		Dec. 19, 1994.	
D029		Mixed with radioactive wastes		Sept. 19, 1996.	
D029		All others		Dec. 19, 1994.	
D030		Mixed with radioactive wastes		Sept. 19. 1996.	
D030		All others		Dec. 19, 1994.	
D031		Mixed with radioactive wastes		Sept. 19, 1996.	
D031		All others		Dec. 19, 1994.	
D032		Mixed with radioactive wastes		Sept. 19, 1996.	
D032		All others		Dec. 19, 1994.	
D033		Mixed with radioactive wastes		Sept. 19, 1996.	
D033		All others		Dec. 19, 1994.	
D034		Mixed with radioactive wastes		Sept. 19, 1996.	
D034		All others		Dec. 19, 1994.	
D035		Mixed with radioactive wastes		Sept. 19, 1996.	
D035		All others		Dec. 19, 1994.	
D036		Mixed with radioactive wastes		Sept. 19, 1996.	
D036		All others		Dec. 19, 1994.	
D037		Mixed with radioactive wastes		Sept. 19, 1996.	
D037		All others		Dec. 19, 1994.	
D038		Mixed with radioactive wastes		Sept. 19, 1996.	
D038		All others		Dec. 19, 1994.	
D039		Mixed with radioactive wastes		Sept. 19, 1996.	
D039		All others		Dec. 19, 1994.	
D040		Mixed with radioactive wastes		Sept. 19, 1996.	
D040		All others		Dec. 19, 1994.	
D041		Mixed with radioactive wastes		Sept. 19, 1996.	
D041		All others		Dec. 19, 1994.	
D042		Mixed with radioactive wastes		Sept. 19, 1996.	
D042		All others		Dec. 19, 1994.	
D043		Mixed with radioactive wastes		Sept. 19, 1996.	
D043		All others		Dec. 19, 1994.	
F001		Small quantity generators, CERCLA response/RCRA corrective action, initial generator's solvent‑water mixtures, solvent-containing sludges and solids.	Nov. 8, 1988.	
F001	 	All others		Nov. 8, 1986.	
F002 (1,1,2‑trichloroethane)		Wastewater and Nonwastewater		Aug. 8, 1990.	
F002		Small quantity generators, CERCLA response/RCRA corrective action, initial generator's solvent‑water mixtures, solvent‑containing sludges and solids.	Nov. 8, 1988.	
F002		All others		Nov. 8, 1986.	
F003		Small quantity generators, CERCLA response/RCRA corrective action, initial generator's solvent‑water mixtures, solvent‑containing sludges and solids.	Nov. 8, 1988.	
F003		All others		Nov. 8, 1986.	
F004		Small quantity generators, CERCLA response/RCRA corrective action, initial generator's solvent‑water mixtures, solvent‑containing sludges and solids.	Nov. 8, 1988.	
F004		All others		Nov. 8, 1986.	
F005 (benzene, 2‑ethoxy ethanol, 2‑nitropropane)		Wastewater and Nonwastewater		Aug. 8, 1990.	
F005		Small quantity generators, CERCLA response/RCRA corrective action, initial generator's solvent‑water mixtures, solvent‑containing sludges and solids.	Nov. 8, 1988.	
F005		All others		Nov. 8, 1986.	
F006		Wastewater		Aug. 8, 1990.	
F006		Nonwastewater		Aug. 8, 1988.	
F006 (cyanides)		Nonwastewater		July 8, 1989.	
F007		All		July 8, 1989.	
F008		All		July 8, 1989.	
F009		All		July 8, 1989.		
F010		All		June 8, 1989.	
F011 (cyanides)		Nonwastewater		Dec. 8, 1989.	
F011		All others		July 8, 1989.	
F012 (cyanides)		Nonwastewater		Dec. 8, 1989.	
F012		All others		July 8, 1989.	
F019		All		Aug. 8, 1990.	
F020		All		Nov. 8, 1988.	
F021		All		Nov. 8, 1988.	
F025		All		Aug. 8, 1990.	
F026		All		Nov. 8, 1988.	
F027		All		Nov. 8, 1988.	
F028		All		Nov. 8, 1988.	
F032		Mixed with radioactive wastes		May 12, 1999	
F032		All others		May 12, 1997	
F033		Mixed with radioactive wastes		May 12, 1999	
F033		All others		May 12, 1997	
F034		Mixed with radioactive wastes		May 12, 1999	
F034		All others		May 12, 1997	
F037		Not generated from surface impoundment cleanouts or closures		June 30, 1993.	
F037		Generated from surface impoundment cleanouts or closures		June 30, 1994.	
F037		Mixed with radioactive wastes		June 30, 1994.	
F038		Not generated from surface impoundment cleanouts or closures		June 30, 1993.	
F038		Generated from surface impoundment cleanouts or closures		June 30, 1994.	
F038		Mixed with radioactive wastes		June 30, 1994.	
F039		Wastewater		Aug. 8, 1990.	
F039		Nonwastewater		May 8, 1992.	
K001 (organics)b		Al		Aug. 8, 1988.	
K001		All others		Aug. 8, 1988.		
K002		All			Aug. 8, 1990.	
K003		All 		Aug. 8, 1990.	
K004		Wastewater		Aug. 8, 1990.	
K004		Nonwastewater		Aug. 8, 1988.	
K005		Wastewater		Aug. 8, 1990.	
K005		Nonwastewater		June 8, 1989.	
K006		All 		Aug. 8, 1990.	
K007		Wastewater		Aug. 8, 1990.	
K007		Nonwastewater		June 8, 1989.	
K008		Wastewater		Aug. 8, 1990.	
K008		Nonwastewater		Aug. 8, 1988.	
K009		All 		June 8, 1989.	
K010		All 		June 8, 1989.	
K011		Wastewater		Aug. 8, 1990.	
K011		Nonwastewate		June 8, 1989.	
K013		Wastewater		Aug. 8, 1990.	
K013		Nonwastewater		June 8, 1989.	
K014		Wastewater		Aug. 8, 1990.	
K014		Nonwastewater		June 8, 1989.	
K015		Wastewater		Aug. 8, 1988.	
K015		Nonwastewater		Aug. 8, 1990.	
K016		Al		Aug. 8, 1988.	
K017		All		Aug. 8, 1990.	
K018		All		Aug. 8, 1988.	
K019		Al		Aug. 8, 1988.	
K020		Al		Aug. 8, 1988.	
K021		Wastewater		Aug. 8, 1990.	
K021		Nonwastewater		Aug. 8, 1988.	
K022		Wastewater		Aug. 8, 1990.	
K022		Nonwastewater		Aug. 8, 1988.	
K023		All		June 8, 1989.	
K024		All		Aug. 8, 1988.	
K025		Wastewater		Aug. 8, 1990.	
K025		Nonwastewater		Aug. 8, 1988.	
K026		All		Aug. 8, 1990.	
K027		All		June 8, 1989.	
K028 (metals)		Nonwastewater		Aug. 8, 1990.	
K028		All others		June 8, 1989.	
K029		Wastewater		Aug. 8, 1990.	
K029		Nonwastewater		June 8, 1989.	
K030		All		Aug. 8, 1988.	
K031		Wastewater		Aug. 8, 1990.	
K031		Nonwastewater		May 8, 1992.	
K032		All		Aug. 8, 1990.	
K033		All		Aug. 8, 1990.	
K034		All		Aug. 8, 1990.	
K035		All		Aug. 8, 1990.	
K036		Wastewater		June 8, 1989.	
K036		Nonwastewater		Aug. 8, 1988.	
K037		Wastewater		Aug. 8, 1988.	
K037		Nonwastewater		Aug. 8, 1988.	
K038		All		June 8, 1989.	
K039		All		June 8, 1989.	
K040		All		June 8, 1989.	
K041		All		Aug. 8, 1990.	
K042		All		Aug. 8, 1990.	
K043		All		June 8, 1989.	
K044		All		Aug. 8, 1988.	
K045		All		Aug. 8, 1988.	
K046 (Nonreactive)		Nonwastewater		Aug. 8, 1988.	
K046		All others		Aug. 8, 1990.	
K047		All		Aug. 8, 1988.	
K048		Wastewater		Aug. 8, 1990.	
K048		Nonwastewater		Nov. 8, 1990.	
K049		Wastewater		Aug. 8, 1990.	
K049		Nonwastewater		Nov. 8, 1990.	
K050		Wastewater		Aug. 8, 1990.	
K050		Nonwastewater		Nov. 8, 1990.	
K051		Wastewater		Aug. 8, 1990.	
K051		Nonwastewater		Nov. 8, 1990.	
K052		Wastewater		Aug. 8, 1990.	
K052		Nonwastewater		Nov. 8, 1990.	
K060		Wastewater		Aug. 8, 1990.	
K060		Nonwastewater		Aug. 8, 1988.	
K061		Wastewater		Aug. 8, 1990.	
K061		Nonwastewater		June 30, 1992.	
K062		All		Aug. 8, 1988.	
K069 (Non‑Calcium Sulfate)		Nonwastewater		Aug. 8, 1988.	
K069		All others		Aug. 8, 1990.	
K071		All		Aug. 8, 1990.	
K073		All		Aug. 8, 1990.	
K083		All		Aug. 8, 1990.	
K084		Wastewater		Aug. 8, 1990.	
K084		Nonwastewater		May 8, 1992.	
K085		All		Aug. 8, 1990.	
K086 (organics)b		All		Aug. 8, 1988.	
K086		All others		Aug. 8, 1988	
K087		All 		Aug. 8, 1988.	
K088		Mixed with radioactive waste		Apr. 8, 1998.	
K088		All others		Jan. 8, 1997.	
K093		All 		June 8, 1989.	
K094		All		June 8, 1989.	
K095		Wastewater		Aug. 8, 1990.	
K095		Nonwastewate		June 8, 1989.	
K096		Wastewater		Aug. 8, 1990.	
K096		Nonwastewater		June 8, 1989.	
K097		All 		Aug. 8, 1990.	
K098		All 		Aug. 8, 1990.	
K099		All 		Aug. 8, 1988.	
K100		Wastewater		Aug. 8, 1990.	
K100		Nonwastewater		Aug. 8, 1988.	
K101 (organics)		Wastewater		Aug. 8, 1988.	
K101 (metals)		Wastewater		Aug. 8, 1990.	
K101 (organics)		Nonwastewater		Aug. 8, 1988.	
K101 (metals)		Nonwastewater		May 8, 1992.	
K102 (organics)		Wastewater		Aug. 8, 1988.	
K102 (metals)		Wastewater		Aug. 8, 1990.	
K102 (organics)		Nonwastewater		Aug. 8, 1988.	
K102 (metals)		Nonwastewater		May 8, 1992.	
K103		Al		Aug. 8, 1988.	
K104		All		Aug. 8, 1988.	
K105		All		Aug. 8, 1990.	
K106		Wastewater		Aug. 8, 1990.	
K106		Nonwastewater		May 8, 1992.	
K107		Mixed with radioactive wastes		June 30, 1994.	
K107		All others		Nov. 9, 1992.	
K108		Mixed with radioactive wastes		June 30, 1994.	
K108		All others		Nov. 9, 1992.	
K109		Mixed with radioactive wastes		June 30, 1994.	
K109		All others		Nov. 9, 1992.	
K110		Mixed with radioactive wastes		June 30, 1994.	
K110		All others		Nov. 9, 1992.	
K111		Mixed with radioactive wastes		June 30, 1994.	
K111		All other		Nov. 9, 1992.	
K112		Mixed with radioactive wastes		June 30, 1994.	
K112		All other		Nov. 9, 1992.	
K113		All		June 8, 1989.	
K114		Al		June 8, 1989.	
K115		All		June 8, 1989.	
K116		All		June 8, 1989.	
K117		Mixed with radioactive wastes		June 30, 1994.	
K117		All others		Nov. 9, 1992.	
K118		Mixed with radioactive wastes		June 30, 1994.	
K118		All others		Nov. 9, 1992.	
K123		Mixed with radioactive wastes		June 30, 1994.	
K123		All others		Nov. 9, 1992.	
K124		Mixed with radioactive wastes		June 30, 1994.	
K124		All others		Nov. 9, 1992.	
K125		Mixed with radioactive wastes		June 30, 1994.	
K125		All others		Nov. 9, 1992.	
K126		Mixed with radioactive wastes		June 30, 1994.	
K126		All others		Nov. 9, 1992.	
K131		Mixed with radioactive wastes		June 30, 1994.	
K131		All others		Nov. 9, 1992.	
K132		Mixed with radioactive wastes		June 30, 1994.	
K132		All others		Nov. 9, 1992.	
K136		Mixed with radioactive wastes		June 30, 1994.	
K136		All others		Nov. 9, 1992.	
K141		Mixed with radioactive wastes		Sep. 19, 1996.	
K141		All others		Dec. 19, 1994.	
K142		Mixed with radioactive wastes		Sep. 19, 1996..	
K142		All others		Dec. 19, 1994.	
K143		Mixed with radioactive wastes		Sep. 19, 1996.	
K143		All others		Dec. 19, 1994.	
K144		Mixed with radioactive wastes		Sep. 19, 1996.	
K144		All others		Dec. 19, 1994.	
K145		Mixed with radioactive wastes		Sep. 19, 1996.	
K145		All others		Dec. 19, 1994.	
K147		Mixed with radioactive wastes		Sep. 19, 1996.	
K147		All others		Dec. 19, 1994.	
K148		Mixed with radioactive wastes		Sep. 19, 1996.	
K148		All others		Dec. 19, 1994.	
K149		Mixed with radioactive wastes		Sep. 19, 1996.	
K149		All others		Dec. 19, 1994.	
K150		Mixed with radioactive wastes		Sep. 19, 1996.	
K150		All others		Dec. 19, 1994.	
K151		Mixed with radioactive wastes		Sep. 19, 1996.	
K151		All others		Dec. 19, 1994.	
K156		Mixed with radioactive wastes		Apr. 8, 1998.	
K156		All others		July 8, 1996.	
K157		Mixed with radioactive wastes		Apr. 8, 1998.	
K157		All others		July 8, 1996.	
K158		Mixed with radioactive wastes		Apr. 8, 1998.	
K158		All others		July 8, 1996.	
K159		Mixed with radioactive wastes		Apr. 8, 1998.	
K159		All others		July 8, 1996.	
K160		Mixed with radioactive wastes		Apr. 8, 1998.	
K160		All others		July 8, 1996.	
K161		Mixed with radioactive wastes		Apr. 8, 1998.	
K161		All others		July 8, 1996.	
P001		All		Aug. 8, 1990.	
P002		All		Aug. 8, 1990.	
P003		All 		Aug. 8, 1990.	
P004		All 		Aug. 8, 1990.	
P005		All		Aug. 8, 1990.	
P006		All 		Aug. 8, 1990.	
P007		All		Aug. 8, 1990.	
P008		All		Aug. 8, 1990.	
P009		All 		Aug. 8, 1990.	
P010		Wastewater		Aug. 8, 1990.	
P010		Nonwastewater		May 8, 1992.	
P011		Wastewater		Aug. 8, 1990.	
P011		Nonwastewater		May 8, 1992.	
P012		Wastewater		Aug. 8, 1990.	
P012		Nonwastewater		May 8, 1992.	
P013 (barium)		Nonwastewater		Aug. 8, 1990.	
P013		All 		June 8, 1989.	
P014		All		Aug. 8, 1990.	
P015		All		Aug. 8, 1990.	
P016		All		Aug. 8, 1990.	
P017		All		Aug. 8, 1990.	
P018		All		Aug. 8, 1990.	
P020		All		Aug. 8, 1990.	
P021		All		June 8, 1989.	
P022		All		Aug. 8, 1990.	
P023		All		Aug. 8, 1990.	
P024		All		Aug. 8, 1990.	
P026		All		Aug. 8, 1990.	
P027		All		Aug. 8, 1990.	
P028		All		Aug. 8, 1990.	
P029		All		June 8, 1989.	
P030		All		June 8, 1989.	
P031		All		Aug. 8, 1990.	
P033		All		Aug. 8, 1990.	
P034		All		Aug. 8, 1990.	
P036		Wastewater		Aug. 8, 1990.	
P036		Nonwastewater		May 8, 1992.		
P037		All		Aug. 8, 1990.	
P038		Wastewater		Aug. 8, 1990.	
P038		Nonwastewater		May 8, 1992.	
P039		All		June 8, 1989.	
P040		All		June 8, 1989.	
P041		All		June 8, 1989.	
P042		All		Aug. 8, 1990.	
P043		All		June 8, 1989.	
P044		All		June 8, 1989.	
P045		All		Aug. 8, 1990.	
P046		All		Aug. 8, 1990.	
P047		All		Aug. 8, 1990.	
P048		All		Aug. 8, 1990.	
P049		All		Aug. 8, 1990.	
P050		All		Aug. 8, 1990.	
P051		All		Aug. 8, 1990.	
P054		All		Aug. 8, 1990.	
P056		All		Aug. 8, 1990.	
P057		All		Aug. 8, 1990.	
P058		All		Aug. 8, 1990.	
P059		All		Aug. 8, 1990.	
P060		All		Aug. 8, 1990.	
P062		All		June 8, 1989.	
P063		All		June 8, 1989.	
P064		All		Aug. 8, 1990.	
P065		Wastewater		Aug. 8, 1990.	
P065		Nonwastewater		May 8, 1992.	
P066		All		Aug. 8, 1990.	
P067		All		Aug. 8, 1990.	
P068		All		Aug. 8, 1990.	
P069		All		Aug. 8, 1990.	
P070		All		Aug. 8, 1990.	
P071		All		June 8, 1989.	
P072		All		Aug. 8, 1990.	
P073		All		Aug. 8, 1990.	
P074		All		June 8, 1989.	
P075		All		Aug. 8, 1990.	
P076		All		Aug. 8, 1990.	
P077		All		Aug. 8, 1990.	
P078		All		Aug. 8, 1990.	
P081		All		Aug. 8, 1990.	
P082		All		Aug. 8, 1990.	
P084		All		Aug. 8, 1990.	
P085		All		June 8, 1989.	
P087		All		May 8, 1992.	
P088		All		Aug. 8, 1990.	
P089		All		June 8, 1989.	
P092		Wastewater		Aug. 8, 1990.	
P092		Nonwastewater		May 8, 1992.	
P093		All		Aug. 8, 1990.	
P094		All		June 8, 1989.	
P095		All		Aug. 8, 1990.	
P096		All		Aug. 8, 1990.	
P097		All		June 8, 1989.	
P098		All		June 8, 1989.	
P099 (silver)		Wastewater		Aug. 8, 1990.	
P099		All others		June 8, 1989.	
P101		All		Aug. 8, 1990.	
P102		All		Aug. 8, 1990.	
P103		All		Aug. 8, 1990.	
P104 (silver)		Wastewater		Aug. 8, 1990.	
P104		All others		June 8, 1989.	
P105		All		Aug. 8, 1990.	
P106		All		June 8, 1989.	
P108		All		Aug. 8, 1990.	
P109		All		June 8, 1989.	
P110		All		Aug. 8, 1990.	
P111		All		June 8, 1989.	
P112		All		Aug. 8, 1990.	
P113		All		Aug. 8, 1990.	
P114		All		Aug. 8, 1990.	
P115		All		Aug. 8, 1990.	
P116		All		Aug. 8, 1990.	
P118		All		Aug. 8, 1990.	
P119		All		Aug. 8, 1990.	
P120		All		Aug. 8, 1990.	
P121		All		June 8, 1989.	
P122		All		Aug. 8, 1990.	
P123		All		Aug. 8, 1990.	
P127		Mixed with radioactive waste		Apr. 8, 1998.	
P127		All others		July 8, 1996.	
P128		Mixed with radioactive wastes		Apr. 8, 1998.	
P128		All others		July 8, 1996.	
P185		Mixed with radioactive wastes		Apr. 8, 1998.	
P185		All others		July 8, 1996.	
P188		Mixed with radioactive wastes		Apr. 8, 1998.	
P188		All others		July 8, 1996.	
P189		Mixed with radioactive wastes		Apr. 8, 1998.	
P189		All others		July 8, 1996.	
P190		Mixed with radioactive wastes		Apr. 8, 1998.	
P190		All others		July 8, 1996.	
P191		Mixed with radioactive wastes		Apr. 8, 1998.	
P191		All others		July 8, 1996.	
P192		Mixed with radioactive wastes		Apr. 8, 1998.	
P192		All others		July 8, 1996.	
P194		Mixed with radioactive wastes		Apr. 8, 1998.	
P194		All others		July 8, 1996.	
P196		Mixed with radioactive wastes		Apr. 8, 1998.	
P196		All others		July 8, 1996.	
P197		Mixed with radioactive wastes		Apr. 8, 1998.	
P197		All others		July 8, 1996.	
P198		Mixed with radioactive wastes		Apr. 8, 1998.	
P198		All others		July 8, 1996.	
P199		Mixed with radioactive wastes		Apr. 8, 1998.	
P199		All others		July 8, 1996.	
P201		Mixed with radioactive wastes		Apr. 8, 1998.	
P201		All others		July 8, 1996.	
P202		Mixed with radioactive wastes		Apr. 8, 1998.	
P202		All others		July 8, 1996.	
P203		Mixed with radioactive wastes		Apr. 8, 1998.	
P203		All others		July 8, 1996.	
P204		Mixed with radioactive wastes		Apr. 8, 1998.	
P204		All others		July 8, 1996.	
P205		Mixed with radioactive wastes		Apr. 8, 1998.	
P205		All others		July 8, 1996.	
U001		All		Aug 8, 1990.	
U002		All		Aug 8, 1990.	
U003		All		Aug 8, 1990.	
U004		All		Aug 8, 1990.	
U005		All		Aug. 8, 1990.	
U006		All		Aug. 8, 1990.	
U007		All		Aug. 8, 1990.	
U008		All		Aug. 8, 1990.	
U009		All		Aug. 8, 1990.	
U010		All		Aug. 8, 1990.	
U011		All		Aug. 8, 1990.	
U012		All		Aug. 8, 1990.	
U014		All		Aug. 8, 1990.	
U015		All		Aug. 8, 1990.	
U016		All		Aug. 8, 1990.	
U017		All		Aug. 8, 1990.	
U018		All		Aug. 8, 1990.	
U019		All		Aug. 8, 1990.	
U020		All		Aug. 8, 1990.	
U021		All		Aug. 8, 1990.	
U022		All		Aug. 8, 1990.	
U023		All		Aug. 8, 1990.	
U024		All		Aug. 8, 1990.	
U025		All		Aug. 8, 1990.	
U026		All		Aug. 8, 1990.	
U027		All		Aug. 8, 1990.	
U028		All		June 8, 1989.	
U029		All		Aug. 8, 1990.	
U030		All		Aug. 8, 1990.	
U031		All		Aug. 8, 1990.	
U032		All		Aug. 8, 1990.	
U033		All		Aug. 8, 1990.	
U034		All		Aug. 8, 1990.	
U035		All		Aug. 8, 1990.	
U036		All		Aug. 8, 1990.	
U037		All		Aug. 8, 1990.	
U038		All		Aug. 8, 1990.	
U039		All		Aug. 8, 1990.	
U041		All		Aug. 8, 1990.	
U042		All		Aug. 8, 1990.	
U043		All		Aug. 8, 1990.	
U044		All		Aug. 8, 1990.	
U045		All		Aug. 8, 1990.	
U046		All		Aug. 8, 1990.	
U047		All		Aug. 8, 1990.	
U048		All		Aug. 8, 1990.	
U049		All		Aug. 8, 1990.	
U050		All		Aug. 8, 1990.	
U051		All		Aug. 8, 1990.	
U052		All		Aug. 8, 1990.	
U053		All		Aug. 8, 1990.	
U055		All		Aug. 8, 1990.	
U056		All		Aug. 8, 1990.	
U057		All		Aug. 8, 1990.	
U058		All		June 8, 1989.	
U059		All		Aug. 8, 1990.	
U060		All		Aug. 8, 1990.	
U061		All		Aug. 8, 1990.	
U062		All		Aug. 8, 1990.	
U063		All		Aug. 8, 1990.	
U064		All		Aug. 8, 1990.	
U066		All		Aug. 8, 1990.	
U067		All		Aug. 8, 1990.	
U068		All		Aug. 8, 1990.	
U069		All		June 30, 1992.	
U070		All		Aug. 8, 1990.	
U071		All		Aug. 8, 1990.	
U072		All		Aug. 8, 1990.	
U073		All		Aug. 8, 1990.	
U074		All		Aug. 8, 1990.	
U075		All		Aug. 8, 1990.	
U076		All		Aug. 8, 1990.	
U077		All		Aug. 8, 1990.	
U078		All		Aug. 8, 1990.	
U079		All		Aug. 8, 1990.	
U080		All		Aug. 8, 1990.	
U081		All		Aug. 8, 1990.	
U082		All		Aug. 8, 1990.	
U083		All		Aug. 8, 1990.	
U084		All		Aug. 8, 1990.	
U085		All		Aug. 8, 1990.	
U086		All		Aug. 8, 1990.	
U087		All		June 8, 1989.	
U088		All		June 8, 1989.	
U089		All		Aug. 8, 1990.	
U090		All		Aug. 8, 1990.	
U091		All		Aug. 8, 1990.	
U092		All		Aug. 8, 1990.	
U093		All		Aug. 8, 1990.	
U094		All		Aug. 8, 1990.	
U095		All		Aug. 8, 1990.	
U096		All		Aug. 8, 1990.	
U097		All		Aug. 8, 1990.	
U098		All		Aug. 8, 1990.	
U099		All		Aug. 8, 1990.	
U101		All		Aug. 8, 1990.	
U102		All		June 8, 1989.	
U103		All		Aug. 8, 1990.	
U105		All		Aug. 8, 1990.	
U106		All		Aug. 8, 1990.	
U107		All		June 8, 1989.	
U108		All		Aug. 8, 1990.	
U109		All		Aug. 8, 1990.	
U110		All		Aug. 8, 1990.	
U111		All		Aug. 8, 1990.	
U112		All		Aug. 8, 1990.	
U113		All		Aug. 8, 1990.	
U114		All		Aug. 8, 1990.	
U115		All		Aug. 8, 1990.	
U116		All		Aug. 8, 1990.	
U117		All		Aug. 8, 1990.	
U118		All		Aug. 8, 1990.	
U119		All		Aug. 8, 1990.	
U120		All		Aug. 8, 1990.	
U121		All		Aug. 8, 1990.	
U122		All		Aug. 8, 1990.	
U123		All		Aug. 8, 1990.	
U124		All		Aug. 8, 1990.	
U125		All		Aug. 8, 1990.	
U126		All		Aug. 8, 1990.	
U127		All		Aug. 8, 1990.	
U128		All		Aug. 8, 1990.	
U129		All		Aug. 8, 1990.	
U130		All		Aug. 8, 1990.	
U131		All		Aug. 8, 1990.	
U132		All		Aug. 8, 1990.	
U133		All		Aug. 8, 1990.	
U134		All		Aug. 8, 1990.	
U135		All		Aug. 8, 1990.	
U136		Wastewater		Aug. 8, 1990.	
U136		Nonwastewater		May 8, 1992.	
U137		All		Aug. 8, 1990.	
U138		All		Aug. 8, 1990.	
U140		All		Aug. 8, 1990.	
U141		All		Aug. 8, 1990.	
U142		All		Aug. 8, 1990.	
U143		All		Aug. 8, 1990.	
U144		All		Aug. 8, 1990.	
U145		All		Aug. 8, 1990.	
U146		All		Aug. 8, 1990.	
U147		All		Aug. 8, 1990.	
U148		All		Aug. 8, 1990.	
U149		All		Aug. 8, 1990.	
U150		All		Aug. 8, 1990.	
U151		Wastewater		Aug. 8, 1990.	
U151		Nonwastewater		May 8, 1992.	
U152		All		Aug. 8, 1990.	
U153		All		Aug. 8, 1990.	
U154		All		Aug. 8, 1990.	
U155		All		Aug. 8, 1990.	
U156		All		Aug. 8, 1990.	
U157		All		Aug. 8, 1990.	
U158		All		Aug. 8, 1990.	
U159		All		Aug. 8, 1990.	
U160		All		Aug. 8, 1990.	
U161		All		Aug. 8, 1990.	
U162		All		Aug. 8, 1990.	
U163		All		Aug. 8, 1990.	
U164		All		Aug. 8, 1990.	
U165		All		Aug. 8, 1990.	
U166		All		Aug. 8, 1990.	
U167		All		Aug. 8, 1990.	
U168		All		Aug. 8, 1990.	
U169		All		Aug. 8, 1990.	
U170		All		Aug. 8, 1990.	
U171		All		Aug. 8, 1990.	
U172		All		Aug. 8, 1990.	
U173		All		Aug. 8, 1990.	
U174		All		Aug. 8, 1990.	
U176		All		Aug. 8, 1990.	
U177		All		Aug. 8, 1990.	
U178		All		Aug. 8, 1990.	
U179		All		Aug. 8, 1990.	
U180		All		Aug. 8, 1990.	
U181		All		Aug. 8, 1990.	
U182		All		Aug. 8, 1990.	
U183		All		Aug. 8, 1990.	
U184		All		Aug. 8, 1990.	
U185		All		Aug. 8, 1990.	
U186		All		Aug. 8, 1990.	
U187		All		Aug. 8, 1990.	
U188		All		Aug. 8, 1990.	
U189		All		Aug. 8, 1990.	
U190		All		June 8, 1989.	
U191		All		Aug. 8, 1990.	
U192		All		Aug. 8, 1990.	
U193		All		Aug. 8, 1990.	
U194		All		June 8, 1989.	
U196		All		Aug. 8, 1990.	
U197		All		Aug. 8, 1990.	
U200		All		Aug. 8, 1990.	
U201		All		Aug. 8, 1990.	
U202		All		Aug. 8, 1990.	
U203		All		Aug. 8, 1990.	
U204		All		Aug. 8, 1990.	
U205		All		Aug. 8, 1990.	
U206		All		Aug. 8, 1990.	
U207		All		Aug. 8, 1990.	
U208		All		Aug. 8, 1990.	
U209		All		Aug. 8, 1990.	
U210		All		Aug. 8, 1990.	
U211		All		Aug. 8, 1990.	
U213		All		Aug. 8, 1990.	
U214		All		Aug. 8, 1990.	
U215		All		Aug. 8, 1990.	
U216		All		Aug. 8, 1990.	
U217		All		Aug. 8, 1990.	
U218		All		Aug. 8, 1990.	
U219		All		Aug. 8, 1990.	
U220		All		Aug. 8, 1990.	
U221		All		June 8, 1989.	
U222		All		Aug. 8, 1990.	
U223		All		June 8, 1989.	
U225		All		Aug. 8, 1990.	
U226		All		Aug. 8, 1990.	
U227		All		Aug. 8, 1990.	
U228		All		Aug. 8, 1990.	
U234		All		Aug. 8, 1990.	
U235		All		June 8, 1989.	
U236		All		Aug. 8, 1990.	
U237		All		Aug. 8, 1990.	
U238		All		Aug. 8, 1990.	
U239		All		Aug. 8, 1990.	
U240		All		Aug. 8, 1990.	
U243		All		Aug. 8, 1990.	
U244		All		Aug. 8, 1990.	
U246		All		Aug. 8, 1990.	
U247		All		Aug. 8, 1990.	
U248		All		Aug. 8, 1990.	
U249		All		Aug. 8, 1990.	
U271		Mixed with radioactive wastes		Apr. 8, 1998.	
U271		All others 		July 8, 1996.	
U277		Mixed with radioactive wastes		Apr. 8, 1998.	
U277		All others 		July 8, 1996.	
U278		Mixed with radioactive wastes		Apr. 8, 1998.	
U278		All others 		July 8, 1996.	
U279		Mixed with radioactive wastes		Apr. 8, 1998.	
U279		All others 		July 8, 1996.	
U280		Mixed with radioactive wastes		Apr. 8, 1998.	
U280		All others 		July 8, 1996.	
U328		Mixed with radioactive wastes		June 30, 1994.	
U328		All others 		Nov. 9, 1992.	
U353		Mixed with radioactive wastes		June 30, 1994.	
U353		All others 		Nov. 9, 1992.	
U359		Mixed with radioactive wastes		June 30, 1994.	
U359		All others 		Nov. 9, 1992.	
U364		Mixed with radioactive wastes		Apr. 8, 1998.	
U364		All others 		July 8, 1996.	
U365		Mixed with radioactive wastes		Apr. 8, 1998.	
U365		All others 		July 8, 1996.	
U366		Mixed with radioactive wastes		Apr. 8, 1998.	
U366		All others 		July 8, 1996.	
U367		Mixed with radioactive wastes		Apr. 8, 1998.	
U367		All others 		July 8, 1996.	
U372		Mixed with radioactive wastes		Apr. 8, 1998.	
U372		All others 		July 8, 1996.	
U373		Mixed with radioactive wastes		Apr. 8, 1998.	
U373		All others 		July 8, 1996.	
U375		Mixed with radioactive wastes		Apr. 8, 1998.	
U375		All others 		July 8, 1996.	
U376		Mixed with radioactive wastes		Apr. 8, 1998.	
U376		All others 		July 8, 1996.	
U377		Mixed with radioactive wastes		Apr. 8, 1998.	
U377		All others 		July 8, 1996.	
U378		Mixed with radioactive wastes		Apr. 8, 1998.	
U378		All others 		July 8, 1996.	
U379		Mixed with radioactive wastes		Apr. 8, 1998.	
U379		All others 		July 8, 1996.	
U381		Mixed with radioactive wastes		Apr. 8, 1998.	
U381		All others 		July 8, 1996.	
U382		Mixed with radioactive wastes		Apr. 8, 1998.	
U382		All others		July 8, 1996.	
U383		Mixed with radioactive wastes		Apr. 8, 1998.	
U383		All others		July 8, 1996.	
U384		Mixed with radioactive wastes		Apr. 8, 1998.	
U384		All others		July 8, 1996.	
U385		Mixed with radioactive wastes		Apr. 8, 1998.	
U385		All others		July 8, 1996.	
U386		Mixed with radioactive wastes		Apr. 8, 1998.	
U386		All others		July 8, 1996.	
U387		Mixed with radioactive wastes		Apr. 8, 1998.	
U387		All others		July 8, 1996.	
U389		Mixed with radioactive wastes		Apr. 8, 1998.	
U389		All others		July 8, 1996.	
U390		Mixed with radioactive wastes		Apr. 8, 1998.	
U390		All others		July 8, 1996.	
U391		Mixed with radioactive wastes		Apr. 8, 1998.	
U391		All others		July 8, 1996.	
U392		Mixed with radioactive wastes		Apr. 8, 1998.	
U392		All others		July 8, 1996.	
U393		Mixed with radioactive wastes		Apr. 8, 1998.	
U393		All others		July 8, 1996.	
U394		Mixed with radioactive wastes		Apr. 8, 1998.	
U394		All others		July 8, 1996.	
U395		Mixed with radioactive wastes		Apr. 8, 1998.	
U395		All others		July 8, 1996.	
U396		Mixed with radioactive wastes		Apr. 8, 1998.	
U396		All others		July 8, 1996.	
U400		Mixed with radioactive wastes		Apr. 8, 1998.	
U400		All others		July 8, 1996.	
U401		Mixed with radioactive wastes		Apr. 8, 1998.	
U401		All others		July 8, 1996.	
U402		Mixed with radioactive wastes		Apr. 8, 1998.	
U402		All others		July 8, 1996.	
U403		Mixed with radioactive wastes		Apr. 8, 1998.	
U403		All others		July 8, 1996.	
U404		Mixed with radioactive wastes		Apr. 8, 1998.	
U404		All others		July 8, 1996.	
U407		Mixed with radioactive wastes		Apr. 8, 1998.	
U407		All others		July 8, 1996.	
U409		Mixed with radioactive wastes		Apr. 8, 1998.	
U409		All others		July 8, 1996.	
U410		Mixed with radioactive wastes		Apr. 8, 1998.	
U410		All others		July 8, 1996.	
U411		Mixed with radioactive wastes		Apr. 8, 1998.	
U411		All others		July 8, 1996.	

a  This table does not include mixed radioactive wastes (from the First, Second, and Third Third rules) which received national capacity variance until May 8, 1992. This table also does not include contaminated soil and debris wastes.
b  The standard was revised in the Third Third Final Rule (55 FR 22520, June 1, 1990).
c  The standard was revised in the Third Third Emergency Rule (58 FR 29860, May 24, 1993); the original effective date was August 8, 1990.
d  The standard was revised in the Phase II Final Rule (59 FR 47982, Sept. 19, 1994); the original effective date was August 8, 1990.
e  The standards for selected reactive wastes was revised in the Phase III Final Rule (61 FR 15566, Apr. 8, 1996); the original effective date was August 8, 1990.

Table 2.‑‑Summary of Effective Dates of Land Disposal Restrictions for Contaminated Soil and Debris (CSD)
Restricted hazardous waste in CSD	Effective date	
1.  Solvent‑(F001‑F005) and dioxin‑(F020‑F023 and F026‑F028) containing soil and debris from CERCLA response or RCRA corrective  actions.		Nov. 8, 1988.	
2.  Soil and debris not from CERCLA response or RCRA corrective actions contaminated with less than 1% total solvents (F001‑F005) or dioxins (F020‑F023 and F026‑F028).		Nov. 8, 1988.	
3.  All soil and debris contaminated with First Third wastes for which treatment standards are based on incineration.		Aug. 8, 1990.	
4.  All soil and debris contaminated with Second Third wastes for which treatment standards are based on incineration.		June 8, 1991.	
5.  All soil and debris contaminated with Third Third wastes or, First or Second Third "soft hammer wastes which had treatment standards promulgated in the Third Third rule, for which treatment standards are based on incineration, vitrification, or mercury retorting, acid leaching followed by chemical precipitation, or thermal recovery of metals; as well as all inorganic solids debris contaminated with D004‑D011 wastes, and all soil and debris contaminated with mixed RCRA/radioactive wastes.		

May 8, 1992.	
6.  Soil and debris contaminated with D012‑D043, K141‑K145, and K147‑151 wastes.		Dec. 19, 1994.	
7. Debris (only) contaminated with F037, F038, K107‑K112, K117, K118, K123‑K126, K131, K132, K136, U328, U353, U359.		Dec. 19, 1994	
8. Soil and debris contaminated with K156‑K161, P127, P128, P188‑P192, P194, P196‑P199, P201‑P205, U271, U277‑U280, U364‑U367, U372, U373, U375‑U379, U381‑U387, U389‑U396, U400‑U404, U407, and U409‑U411 wastes.		July 8, 1996.	
9. Soil and debris contaminated with K088 wastes.		Jan. 8, 1997.	
10. Soil and debris contaminated with radioactive wastes mixed with K088, K156‑K161, P127, P128, P188‑P192, P194, P196‑P199, P201‑P205, U271, U277‑U280, U364‑U367, U372, U373, U375‑U379, U381‑U387, U389‑U396, U400‑U404, U407, and U409‑U411 wastes.		April 8, 1998.	
11. Soil and debris contaminated with F032, F034, and F035.		May 12, 1997.	
	Note: Appendix VII is provided for the convenience of the reader.

	21. Appendix VIII to Part 268 is revised to read as follows:

Appendix VIII to Part 268‑‑LDR Effective Dates of Surface Disposed Prohibited Hazardous Wastes 

National Capacity LDR Variances for UIC Wastesa
Waste code	Waste category	Effective date	
F001‑F005		All spent F001‑F005 solvent containing less than 1 percent total F001‑F005 solvent constituents.	Aug. 8, 1990.	
D001 (except High TOC Ignitable Liquids Subcategory)c.	All		Feb. 10, 1994.	
D001 (High TOC Ignitable Characteristic Liquids Subcategory).	Nonwastewater		Sept. 19, 1995.	
D002b		All		May 8, 1992.	
D002c		All		Feb. 10, 1994.	
D003 (cyanides		All		May 8, 1992.	
D003 (sulfides)		All		May 8, 1992.	
D003 (explosives, reactives)		All		May 8, 1992.	
D007		All		May 8, 1992.	
D009		Nonwastewater		May 8, 1992.	
D012		All		Sept. 19, 1995.	
D013		All		Sept. 19, 1995.	
D014		All		Sept. 19, 1995.	
D015		All		Sept. 19, 1995.	
D016		All		Sept. 19, 1995.	
D017		All		Sept. 19, 1995.	
D018		All, including mixed with radioactive wastes.		Apr. 8, 1998.	
D019		All, including mixed with radioactive wastes.		Apr. 8, 1998.	
D020		All, including mixed with radioactive wastes.		Apr. 8, 1998.	
D021		All, including mixed with radioactive wastes.		Apr. 8, 1998.	
D022		All, including mixed with radioactive wastes.		Apr. 8, 1998.	
D023		All, including mixed radioactive wastes		Apr. 8, 1998.	
D024		All, including mixed radioactive wastes		Apr. 8, 1998.	
D025		All, including mixed radioactive wastes		Apr. 8, 1998.	
D026		All, including mixed radioactive wastes		Apr. 8, 1998.	
D027		All, including mixed radioactive wastes		Apr. 8, 1998.	
D028		All, including mixed radioactive wastes		Apr. 8, 1998.	
D029		All, including mixed radioactive wastes		Apr. 8, 1998.	
D030		All, including mixed radioactive wastes		Apr. 8, 1998.	
D031		All, including mixed radioactive wastes		Apr. 8, 1998.	
D032		All, including mixed radioactive wastes		Apr. 8, 1998.	
D033		All, including mixed radioactive wastes		Apr. 8, 1998.	
D034		All, including mixed radioactive wastes		Apr. 8, 1998.	
D035		All, including mixed radioactive wastes		Apr. 8, 1998.	
D036		All, including mixed radioactive wastes		Apr. 8, 1998.	
D037		All, including mixed radioactive wastes		Apr. 8, 1998.	
D038		All, including mixed radioactive wastes		Apr. 8, 1998.	
D039		All, including mixed radioactive wastes		Apr. 8, 1998.	
D040		All, including mixed radioactive wastes		Apr. 8, 1998.	
D041		All, including mixed radioactive wastes		Apr. 8, 1998.	
D042		All, including mixed radioactive wastes		Apr. 8, 1998.	
D043		All, including mixed radioactive wastes		Apr. 8, 1998.	
F007		All		June 8, 1991.	
F032		All, including mixed radioactive wastes		May 12, 1999.	
F034		All, including mixed radioactive wastes		May 12,1999.	
F035		All, including mixed radioactive wastes		May 12, 1999.	
F037		All		Nov. 8, 1992.	
F038		All		Nov. 8, 1992.	
F039		Wastewater		May 8, 1992.	
K009		Wastewater		June 8, 1991.	
K011		Nonwastewater		June 8, 1991.	
K011		Wastewater		May 8, 1992.	
K011		Nonwastewater		June 8, 1991.	
K011		Wastewater		May 8, 1992.	
K013		Nonwastewater		June 8, 1991.	
K013		Wastewater		May 8, 1992.	
K014		All		May 8, 1992.	
K016 (dilute)		All		June 8, 1991.	
K049		All		Aug. 8, 1990.	
K050		All		Aug. 8, 1990.	
K051		All		Aug. 8, 1990.	
K052		All		Aug. 8, 1990.	
K062		All		Aug. 8, 1990.	
K071		All		Aug. 8, 1990.	
K088		All		Jan. 8, 1997.	
K104		All		Aug. 8, 1990.	
K107		All		Nov. 8, 1992.	
K108		All		Nov. 9, 1992.	
K109		All		Nov. 9, 1992.	
K110		All		Nov. 9, 1992.	
K111		All		Nov. 9, 1992.	
K112		All		Nov. 9, 1992.	
K117		All		June 30, 1995.	
K118		All		June 30, 1995.	
K123		All		Nov. 9, 1992.	
K124		All		Nov. 9, 1992.	
K125		All		Nov. 9, 1992.	
K126		All		Nov. 9, 1992.	
K131		All		June 30, 1995.	
K132		All		June 30, 1995.	
K136		All		Nov. 9, 1992.	
K141		All		Dec. 19, 1994.	
K142		All		Dec. 19, 1994.	
K143		All		Dec. 19, 1994.	
K144		All		Dec. 19, 1994.	
K145		All		Dec. 19, 1994.	
K147		All		Dec. 19, 1994.	
K148		All		Dec. 19, 1994.	
K149		All		Dec. 19, 1994.	
K150		All		Dec. 19, 1994.	
K151		All		Dec. 19, 1994.	
K156		All		July 8, 1996.	
K157		All		July 8, 1996.	
K158		All		July 8, 1996.	
K159		All		July 8, 1996.	
K160		All		July 8, 1996.	
K161		All		July 8, 1996.	
P127		All		July 8, 1996.	
P128		All		July 8, 1996.	
P185		All		July 8, 1996.	
P188		All		July 8, 1996.	
P189		All		July 8, 1996.	
P190		All		July 8, 1996.	
P191		All		July 8, 1996.	
P192		All		July 8, 1996.	
P194		All		July 8, 1996.	
P196		All		July 8, 1996.	
P197		All		July 8, 1996.	
P198		All		July 8, 1996.	
P199		All		July 8, 1996.	
P201		All		July 8, 1996.	
P202		All		July 8, 1996.	
P203		All		July 8, 1996.	
P204		All		July 8, 1996.	
P205		All		July 8, 1996.	
U271		All		July 8, 1996.	
U277		All		July 8, 1996.	
U278		All		July 8, 1996.	
U279		All		July 8, 1996.	
U280		All		July 8, 1996.	
U328		All		Nov. 9, 1992.	
U353		All		Nov. 9, 1992.	
U359		All		Nov. 9, 1992.	
U364		All		July 8, 1996.	
U365		All		July 8, 1996.	
U366		All		July 8, 1996.	
U367		All		July 8, 1996.	
U372		All		July 8, 1996.	
U373		All		July 8, 1996.	
U375		All		July 8, 1996.	
U376		All		July 8, 1996.	
U377		All		July 8, 1996.	
U378		All		July 8, 1996.	
U379		All		July 8, 1996.	
U381		All		July 8, 1996.	
U382		All		July 8, 1996.	
U383		All		July 8, 1996.	
U384		All		July 8, 1996.	
U385		All		July 8, 1996.	
U386		All		July 8, 1996.	
U387		All		July 8, 1996.	
U389		All		July 8, 1996.	
U390		All		July 8, 1996.	
U391		All		July 8, 1996.	
U392		All		July 8, 1996.	
U395		All		July 8, 1996.	
U396		All		July 8, 1996.	
U400		All		July 8, 1996.	
U401		All		July 8, 1996.	
U402		All		July 8, 1996.	
U403		All		July 8, 1996.	
U404		All		July 8, 1996.	
U407		All		July 8, 1996.	
U409		All		July 8, 1996.	
U410		All		July 8, 1996.	
U411		All		July 8, 1996.	

a  Wastes that are deep well disposed on‑site receive a six‑month variance, with restrictions effective in November 1990.
b  Deepwell injected D002 liquids with a pH less than 2 must meet the California List treatment standards on August 8, 1990.
c  Managed in systems defined in 40 CFR 144.6(e) and 14.6(e) as Class V injection wells, that do not engage in CWA‑equivalent treatment before injection.
Note: This table is provided for the convenience of the reader.

>>>> Part 271 has not been included because it is not required as part of a State's Hazardous Waste
Program. <<<<

[FR Doc. 97‑11636 Filed 5‑9‑97; 8:45 am]
BILLING CODE 6560‑50‑P