Vol. 56 No. 21 Thursday, January 31, 1991 p 3864 

This article, FR83, is divided into three files.
This is File A:  Preamble and changes to federal regulations, part 148 through 268.42.

NOTE:  This article contained several typographical errors when it was published in the Federal Register.  Some of these errors in Table CCWE (268.41), Table 2 (268.42), and Table CCW (268.43) have been corrected in this electronic version of the article, based on information from EPA State and Regional Programs Branch.

ENVIRONMENTAL PROTECTION AGENCY

40 CFR Parts 148, 261, 268, and 270

[FRL-3866-4]

Land Disposal Restrictions for Third Third Scheduled Wastes

AGENCY: Environmental Protection Agency (EPA).

ACTION: Final rule; technical amendment.

SUMMARY: On June 1, 1990, EPA published regulations promulgating congressionally-mandated prohibitions on land disposal of certain hazardous wastes. This notice corrects errors and clarifies the language in the preamble and regulations of the June 1, 1990 final rule.

EFFECTIVE DATE: This rule is effective on January 31, 1991.

ADDRESSES: The RCRA docket is open from 9:30 to 3:30, Monday through Friday, excluding Federal holidays, and is located at the following address: EPA RCRA Docket (OS-305), Room M-2427, 401 M Street, SW., Washington, DC 20460. The public must make an appointment to review docket materials by calling (202) 475-9327. Refer to Docket number F-90-L13A-FFFFF when making appointments to review any background documentation for this rulemaking. The public may copy a maximum of 100 pages of material from any one regulatory docket at no cost; additional copies cost $0.15 per page.

FOR FURTHER INFORMATION CONTACT: For general information contact the RCRA Hotline at (800) 424-9346 (toll-free) or (202) 382-3000 in the Washington, DC metropolitan area. For technical information contact Rhonda Craig, Office of Solid Waste (OS-320W), U.S. Environmental Protection Agency, 401 M Street, SW., Washington, DC 20460, (703) 308-8462.

>>>>  Preamble has not been included in this file.  <<<<

	For the reasons set out in the preamble, title 40, chapter I of the Code of Federal Regulations is amended as follows:

PART 148-HAZARDOUS WASTE INJECTION RESTRICTIONS

	1. The authority citation for part 148 continues to read as follows:

	Authority: Section 3004, Resource Conservation and Recovery Act, 42 U.S.C. 6901 et seq.

	2. Section 148.10 is amended by redesignating paragraph (c) as (e), and adding new paragraphs (c) and (d), and Tables A and B to the end of the section to read as follows:
§ 148.10 Waste specific prohibitions-solvent wastes.
*   *   *   *   *

	(c) Effective August 8, 1990, all spent F002 and F005 wastes containing solvent constituents listed in Table B of this section are prohibited from underground injection at off-site injection facilities.

	(d) Effective November 8, 1990, the wastes specified in paragraph (c) of this section are prohibited from underground injection at on-site injection facilities.

	(e) * * *

Table A

Acetone
n-Butyl alcohol
Carbon disulfide
Carbon tetrachloride
Chlorobenzene
Cresols and cresylic acid
Cyclohexanone
1,2-dichlorobenzene
Ethyl acetate
Ethyl benzene
Isobutanol
Methanol
Methylene chloride
Methylene chloride (from the pharmaceutical industry)
Methyl ethyl ketone
Nitrobenzene
Pyridine
Tetrachloroethylene
Toulene
1,1,1-Trichloroethane
1,2,2-Trichloro-1,2,2-trifluoroethane
Trichloroethylene
Trichlorofluoromethane
Xylene

Table B

Benzene
2-Ethoxyethanol
2-Nitropropane
1,1,2-Trichloroethane

	3. In § 148.16 paragraph (c) is revised to read as follows:

§ 148.16  Waste specific prohibitions-third third wastes.
*   *   *   *   *

	(c) Effective August 8, 1990, the wastes identified in 40 CFR 261.31 as EPA Hazardous Waste Number F039 (nonwastewaters); the wastes specified in 40 CFR 261.32 as EPA Hazardous Waste Numbers K002, K003, K005 (wastewaters), K006, K007 (wastewaters), K026, K032, K033, K034, and K100 (wastewaters); the wastes specified in 40 CFR 261.33 as P006, P009, P017, P022, P023, P024, P028, P031, P033, P034, P038, P042, P045, P046, P047, P051, P056, P064, P065, P073, P075, P076, P077, P078, P088, P093, P095, P096, P101, P103, P116, P118, P119, U001, U004, U006, U017, U024, U027, U030, U033, U034, U038, U039, U042, U045, U048, U052, U055, U056, U068, U071, U072, U075, U076, U079, U081, U082, U084, U085, U090, U091, U096, U112, U113, U117, U118, U120, U121, U123, U125, U126, U132, U136, U141, U145, U148, U152, U153, U156, U160, U166, U167, U181, U182, U183, U184, U186, U187, U191, U194, U197, U201, U202, U204, U207, U222, U225, U234, U236, U240, U243, U246, and U247; and the wastes identified in 40 CFR 261.21, 261.23 or 261.24 as hazardous based on a characteristic alone, designated as D001, D004, D005, D006, D008, D009 (wastewaters), D010, D011, D012, D013, D014, D015, D016, D017, and newly listed waste F025 are prohibited from underground injection at off-site injection facilities.
*   *   *   *   * 

PART 261-IDENTIFICATION AND LISTING OF HAZARDOUS WASTES

	1. The authority citation for part 261 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921, 6922, and 6938.

Subpart C-Characteristics of Hazardous Waste

	2. Section 261.3 is amended by revising paragraph (d)(1) to read as follows:

§ 261.3  Definition of hazardous waste.
*   *   *   *   *

	(d) * * *

	(1) In the case of any solid waste, it does not exhibit any of the characteristics of hazardous waste identified in Subpart C. (However, wastes that exhibit a characteristic at the point of generation may still be subject to the requirements of Part 268, even if they no longer exhibit a characteristic at the point of land disposal.)
*   *   *   *   *

	3. Section 261.20, paragraph (b) is revised to read as follows:

§ 261.20  General.
*   *   *   *   *

	(b) A hazardous waste which is identified by a characteristic in this Subpart is assigned every EPA Hazardous Waste Number that is applicable as set forth in this Subpart. This number must be used in complying with the notification requirements of section 3010 of the Act and all applicable recordkeeping and reporting requirements under Parts 262 through 265, 268, and 270 of this chapter.
*   *   *   *   *

	4. Section 261.31(a), the table is amended by revising the entry for F039 to read as follows:

Industry and EPA hazardous waste No.
Hazardous waste
Hazard code

*		*		*		*		*		*		*

F039
Leachate (liquids that have percolated through land disposed wastes) resulting from the disposal of more than one restricted waste classified as hazardous under Subpart D of this Part. (Leachate resulting from the disposal of one or more of the following EPA Hazardous Wastes and no other Hazardous Wastes retains its EPA Hazardous Waste Number(s): F020, F021, F022, F026, F027, and/or F028.)
(T)

*   *   *   *   * 

PART 262-STANDARDS APPLICABLE TO GENERATORS OF HAZARDOUS WASTE

	1. The authority citation for part 262 continues to read as follows:

	Authority: 42 U.S.C. 6906, 6912, 6922, 6923, 6924, 6925, and 6937.

	2. Note 2 in § 262.10 is revised to read as follows:

§ 262.10  Purpose, scope, and applicability.
*   *   *   *   *

	Note 2: A generator who treats, stores, or disposes of hazardous waste on-site must comply with the applicable standards and permit requirements set forth in 40 CFR parts 264, 265, 266, 268, and 270.

	3. Section 262.11 is amended by revising the introductory text of paragraph (c) to read as follows:

§ 262.11  Hazardous waste determination.
*   *   *   *   *

	(c) For purposes of compliance with 40 CFR part 268, or if the waste is not listed in subpart D of 40 CFR part 261, the generator must then determine whether the waste is identified in subpart C of 40 CFR part 261 by either:
*   *   *   *   *

	4. Section 262.34 is amended by revising paragraph (d)(4) to read as follows:

§ 262.34  Accumulation time.
*   *   *   *   *

	(d) * * *

	(4) The generator complies with the requirements of paragraphs (a)(2) and (a)(3) of this section, the requirements of subpart C of part 265, the requirements of 40 CFR 268.7(a)(4); and
*   *   *   *   * 

PART 268-LAND DISPOSAL RESTRICTIONS

	1. The authority citation for part 268 continues to read as follows:

	Authority: 42 U.S.C. 6905, 6912(a), 6921, and 6924.

	2. Section 268.2 is amended by revising paragraphs (d), (f)(1), (f)(2), and (g) to read as follows:

§ 268.2  Definitions applicable in this part.
*   *   *   *   *

	(d) Nonwastewaters are wastes that do not meet the criteria for wastewaters in paragraph (f) of this section.
*   *   *   *   *

	(f) * * *

	(1) F001, F002, F003, F004, F005, wastewaters are solvent-water mixtures that contain less than 1% by weight TOC or less than 1% by weight total F001, F002, F003, F004, F005 solvent constituents listed in § 268.41, Table CCWE.

	(2) K011, K013, K014 wastewaters contain less than 5% by weight TOC and less than 1% by weight TSS, as generated.
*   *   *   *   *
	(g) Inorganic Solid Debris means nonfriable inorganic solids contaminated with D004-D011 hazardous wastes that are incapable of passing through a 9.5 mm standard sieve; and that require cutting, or crushing and grinding in mechanical sizing equipment prior to stabilization; and, are limited to the following inorganic or metal materials:

	(1) Metal slags (either dross or scoria);

	(2) Glassified slag;

	(3) Glass;

	(4) Concrete (excluding cementitious or pozzolanic stabilized hazardous wastes);

	(5) Masonry and refractory bricks;

	(6) Metal cans, containers, drums, or tanks;

	(7) Metal nuts, bolts, pipes, pumps, valves, appliances, or industrial equipment;

	(8) Scrap metal as defined in 40 CFR 261.1(c)(6);

	3. Section 268.7 is amended by redesignating paragraphs (a)(6) through (a)(9) as paragraphs (a)(7) through (a)(10); by revising paragraphs (a) introductory text, (a)(1)(ii), (a)(2)(i)(B), (a)(3)(ii), (a)(7), (b)(4)(ii), and the section heading; and by adding paragraph (a)(6) to read as follows:

§ 268.7  Waste analysis and recordkeeping.

	(a) Except as specified in § 268.32 of this part, if a generator's waste is listed in 40 CFR part 261, subpart D, the generator must test his waste, or test an extract using the test method described in part 261, appendix II, or use knowledge of the waste, to determine if the waste is restricted from land disposal under this part. Except as specified in § 268.32 of this part, if a generator's waste exhibits one or more of the characteristics set out at 40 CFR part 261, subpart C, the generator must test an extract using the test method described in appendix IX of this part, or use knowledge of the waste, to determine if the waste is restricted from land disposal under this Part.

	(1) * * *

	(ii) The corresponding treatment standards for wastes F001-F005, F039, and wastes prohibited pursuant to § 268.32 or RCRA section 3004(d). Treatment standards for all other restricted wastes must either be included, or be referenced by including on the notification the applicable wastewater (as defined in § 268.2(f)) or nonwastewater (as defined in § 268.2(d)) category, the applicable subdivisions made within a waste code based on waste-specific criteria (such as D003 reactive cyanides), and the CFR section(s) and paragraph(s) where the applicable treatment standard appears. Where the applicable treatment standards are expressed as specified technologies in § 268.42, the applicable five-letter treatment code found in Table 1 of § 268.42 (e.g., INCIN, WETOX) also must be listed on the notification.
*   *   *   *   *

	(2) * * *

	(i) * * *

	(B) The corresponding treatment standards for wastes F001-F005, F039, and wastes prohibited pursuant to § 268.32 or RCRA section 3004(d). Treatment standards for all other restricted wastes must either be included, or be referenced by including on the notification the applicable wastewater (as defined in § 268.2(f)) or nonwastewater (as defined in § 268.2(d)) category, the applicable subdivisions made within a waste code based on waste-specific criteria (such as D003 reactive cyanides), and the CFR section(s) and paragraph(s) where the applicable treatment standard appears. Where the applicable treatment standards are expressed as specified technologies in § 268.42, the applicable five-letter treatment code found in Table 1 of § 268.42 (e.g., INCIN, WETOX) also must be listed on the notification.
*   *   *   *   *

	(3) * * *

	(ii) The corresponding treatment standards for wastes F001-F005, F039, and wastes prohibited pursuant to § 268.32 or RCRA section 3004(d). Treatment standards for all other restricted wastes must either be included, or be referenced by including on the notification the applicable wastewater (as defined in § 268.2(f)) or nonwastewater (as defined in § 268.2(d)) category, the applicable subdivisions made within a waste code based on waste-specific criteria (such as D003 reactive cyanides), and the CFR section(s) and paragraph(s) where the applicable treatment standard appears. Where the applicable treatment standards are expressed as specified technologies in § 268.42, the applicable five-letter treatment code found in Table 1 of § 268.42 (e.g., INCIN, WETOX) also must be listed on the notification.
*   *   *   *   *

	(6) If a generator determines that he is managing a restricted waste that is excluded from the definition of hazardous or solid waste or exempt from Subtitle C regulation, under 40 CFR 261.2-261.6 subsequent to the point of generation, he must place a one-time notice stating such generation, subsequent exclusion from the definition of hazardous or solid waste or exemption from Subtitle C regulation, and the disposition of the waste, in the facility's file.

	(7) Generators must retain on-site a copy of all notices, certifications, demonstrations, waste analysis data, and other documentation produced pursuant to this section for at least five years from the date that the waste that is the subject of such documentation was last sent to on-site or off-site treatment, storage, or disposal. The five year record retention period is automatically extended during the course of any unresolved enforcement action regarding the regulated activity or as requested by the Administrator. The requirements of this paragraph apply to solid wastes even when the hazardous characteristic is removed prior to disposal, or when the waste is excluded from the definition of hazardous or solid waste under 40 CFR 261.2-261.6, or exempted from Subtitle C regulation, subsequent to the point of generation.
*   *   *   *   *

	(b) * * *

	(4) * * *

	(ii) The corresponding treatment standards for wastes F001-F005, F039, and wastes prohibited pursuant to § 268.32 or RCRA section 3004(d). Treatment standards for all other restricted wastes must either be included, or be referenced by including on the notification the applicable wastewater (as defined in § 268.2(f)) or nonwastewater (as defined in § 268.2(d)) category, the applicable subdivisions made within a waste code based on waste-specific criteria (such as D003 reactive cyanides), and the CFR section(s) and paragraph(s) where the applicable treatment standard appears. Where the applicable treatment standards are expressed as specified technologies in § 268.42, the applicable five-letter treatment code found in Table 1 of § 268.42 (e.g., INCIN, WETOX) also must be included on the notification.
*   *   *   *   *

	4. Section 268.9 is amended by revising paragraphs (a) and (d)(1)(ii) to read as follows:

§ 268.9  Special rules regarding wastes that exhibit a characteristic.

	(a) The initial generator of a solid waste must determine each EPA Hazardous Waste Number (waste code) applicable to the waste in order to determine the applicable treatment standards under subpart D of this part. For purposes of part 268, the waste will carry the waste code for any applicable listing under 40 CFR part 261, subpart D. In addition, the waste will carry one or more of the waste codes under 40 CFR part 261, subpart C, where the waste exhibits a characteristic, except in the case when the treatment standard for the waste code listed in 40 CFR part 261, subpart D operates in lieu of the standard for the waste code under 40 CFR part 261, subpart C, as specified in paragraph (b) of this section.
*   *   *   *   *

	(d) * * *

	(1) * * *

	(ii) A description of the waste as initially generated, including the applicable EPA Hazardous Waste Number(s), the applicable wastewater (as defined in § 268.2(f)) or nonwastewater (as defined in § 268.2(d)) category, and the subdivisions made within a waste code based on waste-specific criteria (such as D003 reactive cyanides).
*   *   *   *   * 

§ 268.10  [Amended]

	5. Section 268.10 is amended by removing the entries for the following hazardous wastes: K048, K049, K050, K051, and K052.

	6. Section 268.12(a) is amended by adding the following hazardous wastes in alphanumeric order:

§ 268.12  Identification of wastes to be evaluated by May 8, 1990.

	(a) * * *

§ 261.32  Wastes.
*   *   *   *   *

	K048-Dissolved air flotation (DAF) float from the petroleum refining industry.

	K049-Slop oil emulsion solids from the petroleum refining industry.

	K050-Heat exchanger bundle cleaning sludge from the petroleum refining industry.

	K051-API separator sludge from the petroleum refining industry.

	K052-Tank bottoms (leaded) from the petroleum refining industry.
*   *   *   *   * 

Subpart C-Prohibitions on Land Disposal

	7. Section 268.33 is amended by revising paragraph (b) to read as follows:

§ 268.33  Waste specific prohibitions-First Third wastes.
*   *   *   *   *

	(b) Effective August 8, 1990, the waste specified in 40 CFR 261.32 as EPA Hazardous Waste Nos. K071 is prohibited from land disposal.
*   *   *   *   *

	8. Section 268.35 is amended by revising paragraphs (a), (c), (d), and (e) to read as follows:

§ 268.35  Waste specific prohibitions-Third Third wastes.

	(a) Effective August 8, 1990, the following wastes specified in 40 CFR 261.31 as EPA Hazardous Waste Numbers F002 (1,1,2-trichloroethane), F005 (benzene), F005 (2-ethoxy ethanol) F005 (2-nitropropane), F006 (wastewaters), F019, F025, and F039 (wastewaters); the wastes specified in 40 CFR 261.32 as EPA Hazardous Waste Numbers K002; K003; K004 (wastewaters); K005 (wastewaters); K006; K008 (wastewaters); K011 (wastewaters); K013 (wastewaters); K014 (wastewaters); K015 (nonwastewaters); K017; K021 (wastewaters); K022 (wastewaters); K025 (wastewaters); K026; K029 (wastewaters); K031 (wastewaters); K032; K033; K034; K035; K041; K042; K046 (wastewaters, reactive nonwastewaters); K048 (wastewaters); K049 (wastewaters); K050 (wastewaters); K051 (wastewaters); K052 (wastewaters); K060 (wastewaters); K061 (wastewaters) and (high zinc subcategory > 15% zinc); K069 (wastewaters, calcium sulfate nonwastewaters); K073, K083; K084 (wastewaters); K085; K095 (wastewaters); K096 (wastewaters); K097; K098; K100 (wastewaters); K101 (wastewaters); K102 (wastewaters); K105; and K106 (wastewaters); the wastes specified in 40 CFR 261.33(e) as EPA Hazardous Waste Numbers P001; P002; P003; P004; P005; P006; P007; P008; P009; P010 (wastewaters); P011 (wastewaters); P012 (wastewaters); P014; P015; P016; P017; P018; P020; P022; P023; P024; P026; P027; P028; P031; P033; P034; P036 (wastewaters); P037; P038 (wastewaters); P042; P045; P046; P047; P048; P049; P050; P051; P054; P056; P057; P058; P059; P060; P064; P065 (wastewaters); P066; P067; P068; P069; P070; P072; P073; P075; P076; P077; P078; P081; P082; P084; P088; P092 (wastewaters); P093; P095; P096; P101; P102; P103; P105; P108; P110; P112; P113; P114; P115; P116; P118; P119; P120; P122; and P123; and the wastes specified in 40 CFR 261.33(f) as EPA Hazardous Waste Numbers U001; U002; U003; U004; U005; U006; U007; U008; U009; U010; U011; U012; U014; U015; U016; U017; U018; U019; U020; U021; U022; U023; U024; U025; U026; U027; U029; U030; U031; U032; U033; U034; U035; U036; U037; U038; U039; U041; U042; U043; U044; U045; U046; U047; U048; U049; U050; U051; U052; U053; U055; U056; U057; U059; U060; U061; U062; U063; U064; U066; U067; U068; U070; U071; U072; U073; U074; U075; U076; U077; U078; U079; U080; U081; U082; U083; U084; U085; U086; U089; U090; U091; U092; U093; U094; U095; U096; U097; U098; U099; U101; U103; U105; U106; U108; U109; U110; U111; U112; U113; U114; U115; U116; U117; U118; U119; U120; U121; U122; U123; U124; U125; U126; U127; U128; U129; U130; U131; U132; U133; U134; U135; U136 (wastewaters); U137; U138; U140; U141; U142; U143; U144; U145; U146; U147; U148; U149; U150; U151 (wastewaters); U152; U153; U154; U155; U156; U157; U158; U159; U160; U161; U162; U163; U164; U165; U166; U167; U168; U169; U170; U171; U172; U173; U174; U176; U177; U178; U179; U180; U181; U182; U183; U184; U185; U186; U187; U188; U189; U191; U192; U193; U194; U196; U197; U200; U201; U202; U203; U204; U205; U206; U207; U208; U209; U210; U211; U213; U214; U215; U216; U217; U218; U219; U220; U222; U225; U226; U227; U228; U234; U236; U237; U238; U239; U240; U243; U244; U246; U247; U248; U249; and the following wastes identified as hazardous based on a characteristic alone: D001; D002, D003, D004 (wastewaters), D005, D006; D007; D008 (except for lead materials stored before secondary smelting), D009 (wastewaters), D010, D011, D012, D013, D014, D015, D016, and D017 are prohibited from land disposal.
*   *   *   *   *

	(c) Effective May 8, 1992, the following waste specified in 40 CFR 261.31 as EPA Hazardous Waste Numbers F039 (nonwastewaters); the wastes specified in 40 CFR 261.32 as EPA Hazardous Waste Numbers K031 (nonwastewaters); K084 (nonwastewaters); K101 (nonwastewaters); K102 (nonwastewaters); K106 (nonwastewaters); the wastes specified in 40 CFR 261.33(e) as EPA Hazardous Waste Numbers P010 (nonwastewaters); P011 (nonwastewaters); P012 (nonwastewaters); P036 (nonwastewaters); P038 (nonwastewaters); P065 (nonwastewaters); P087; and P092 (nonwastewaters); the wastes specified in 40 CFR 261.33(f) as EPA Hazardous Waste Numbers U136 (nonwastewaters); and U151 (nonwastewaters); the following wastes identified as hazardous based on a characteristic alone: D004 (nonwastewaters); D008 (lead materials stored before secondary smelting); and D009 (nonwastewaters); inorganic solid debris as defined in 40 CFR 268.2(g) (which also applies to chromium refractory bricks carrying the EPA Hazardous Waste Numbers K048-K052); and RCRA hazardous wastes that contain naturally occurring radioactive materials are prohibited from land disposal.

	(d) Effective May 8, 1992, hazardous wastes listed in 40 CFR 268.10, 268.11, and 268.12 that are mixed radioactive/hazardous wastes, and soil or debris contaminated with hazardous wastes listed in 40 CFR 268.10, 268.11, and 268.12 that are mixed radioactive/hazardous wastes, are prohibited from land disposal.

	(e) Effective May 8, 1992, the wastes specified in this section having a treatment standard in Subpart D of this Part based on incineration, mercury retorting, vitrification, acid leaching followed by chemical precipitation, or thermal recovery of metals, and which are contaminated soil or debris, are prohibited from land disposal.
*   *   *   *   * 

Subpart D-Treatment Standards

	9. Section 268.40 is amended by revising paragraph (a) to read as follows:

§ 268.40  Applicability of treatment standards.

	(a) A restricted waste identified in § 268.41 may be land disposed only if an extract of the waste or of the treatment residue of the waste developed using the test method in Appendix II of part 261 does not exceed the value shown in Table CCWE of § 268.41 for any hazardous constituent listed in Table CCWE for that waste, with the following exceptions: D004, D008, K031, K084, K101, K102, P010, P011, P012, P036, P038, and U136. These wastes may be land disposed only if an extract of the waste or of the treatment residue of the waste developed using either the test method in 40 CFR part 261, appendix II, or the test method in appendix IX of this part, does not exceed the concentrations shown in Table CCWE of § 268.41 for any hazardous constituent listed in Table CCWE for that waste.
*   *   *   *   *

	10. Table CCWE in § 268.41(a) is revised to read as follows:

§ 268.41  Treatment standards expressed as concentrations in waste extract.

	(a) * * *

268.41 Table CCWE.-Constituent Concentrations in Waste Extract

	

	Wastewaters		Nonwastewaters

Waste code
Commercial chemical name
See also
Regulated hazardous constituent
CAS No. for regulated hazardous constituent
Concentration (mg/l)
Notes
Concentration (mg/l)
Notes

D004 
NA 
Table CCW in 268.43
Arsenic 
7440-38-2
NA

5.0
(1)
D005 
NA 
Table CCW in 268.43
Barium 
7440-39-3
NA

100

D006 
NA 
Table CCW in 268.43
Cadmium 
7440-43-9
NA

1.0

D007 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

5.0

D008 
NA 
Table CCW in 268.43
Lead 
7439-92-1
NA

5.0
(1)
D009 (Low Mercury Subcategory-less than 260 mg/kg Mercury)
NA 
Table 2 in 268. 42 and Table CCW in 268.43
Mercury 
7439-97-6
NA

0.20

D010 
NA 
Table CCW in 268.43
Selenium 
7782-49-2
NA

5.7

D011 
NA 
Table CCW in 268.43
Silver 
7440-22-4
NA

5.0

F001-F005 spent solvents.
NA 
Table 2 in 268.42 and Table CCW in 268.43
Acetone 
67-64-1
0.05

0.59

n-Butyl alcohol
71-36-3
5.0

5.0

Carbon disulfide
75-15-0
1.05

4.81

Carbon tetrachloride
56-23-5
0.05

0.96

Chlorobenzene
108-90-7
0.15

0.05

Cresols (and cresylic acid)

2.82

0.75

Cyclohexanone
108-94-1
0.125

0.75

1,2-Dichlorobenzene
95-50-1
0.65

0.125

Ethyl acetate
141-78-6
0.05

0.75

Ethylbenzene
100-41-4
0.05

0.053

Ethyl ether
60-29-7
0.05

0.75

Isobutanol
78-83-1
5.0

5.0

Methanol
67-56-1
0.25

0.75

Methylene chloride
75-9-2
0.20

0.96

Methyl ethyl ketone
78-93-3
0.05

0.75

Methyl isobutyl ketone
108-10-1
0.05

0.33

Nitrobenzene
98-95-3
0.66

0.125

Pyridine
110-86-1
1.12

0.33

Tetrachloroethylene
127-18-4
0.079

0.05

Toluene
108-88-3
1.12

0.33

1,1,1,-Trichloroethane
71-55-6
1.05

0.41

1,1,2-Trichloro-1,2,2-Trifluor- ethane
76-13-1
1.05

0.96

Trichloroethylene
79-01-6
0.062

0.091

Trichlorofluoromethane
75-69-4
0.05

0.96

Xylene

0.05

0.15

F006 
NA 
Table CCW in 268.43
Cadmium 
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

Nickel
7440-02-0
NA

0.32

Silver
7440-22-4
NA

0.072

F007 
NA 
Table CCW in 268.43
Cadmium 
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

Nickel
7440-02-0
NA

0.32

Silver
7440-22-4
NA

0.072

F008 
NA 
Table CCW in 268.43
Cadmium 
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

Nickel
7440-02-0
NA

0.32

Silver
7440-22-4
NA

0.072

F009 
NA 
Table CCW in 268.43
Cadmium 
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

Nickel
7440-02-0
NA

0.32

Silver
7440-22-4
NA

0.072

F011 
NA 
Table CCW in 268.43
Cadmium 
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

Nickel
7440-02-0
NA

0.32

Silver
7440-22-4
NA

0.072

F012 
NA 
Table CCW in 268.43
Cadmium 
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

Nickel
7440-02-0
NA

0.32

Silver
7440-22-4
NA

0.072

F019 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

5.2

F020-F023 and F026-F028 dioxin containing wastes2
NA 
NA 
HxCDD-All Hexachloro-dibenzo-p- dioxins

<1 ppb

<1 ppb

HxCDF-All Hexachloro-dibenzofurans

<1 ppb

<1 ppb

PeCDD-All Pentachloro-dibenzo-p-dioxins

<1 ppb

<1 ppb

PeCDF-All Pentachloro-dibenzofurans

<1 ppb

<1 ppb

TCDD-All Tetrachloro-dibenzo-p-dioxins

TCDF-All Tetrachloro-dibenzofurans

<1 ppb

<1 ppb

2,4,5-Trichlorophenol
95-95-4
<0.05 ppm

<0.05 ppm

2,4,6-Trichlorophenol
88-06-2
<0.05 ppm

<0.05 ppm

2,3,4,6-Tetrachlorophenol
58-90-2
<0.05 ppm

<0.05 ppm

Pentachlorophenol
87-86-5
<0.01 ppm

<0.01 ppm

F024 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.073

Lead
7439-92-1
NA

[Reserved]

Nickel
7440-02-0
NA

0.088

F039 
NA 
Table CCW in 268.43
Antimony 
7440-36-0
NA

0.23

Arsenic
7440-38-2
NA

5.0

Barium
7440-39-3
NA

52

Cadmium
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

Mercury
7439-97-6
NA

0.025

Nickel
7440-02-0
NA

0.32

Selenium
7782-49-2
NA

5.7

Silver
7440-22-4
NA

0.072

K001 
NA 
Table CCW in 268.43
Lead 
7439-92-1
NA

0.51

K002 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K003 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K004 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K005 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K006 (anhydrous)
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K006 (hydrated)
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

5.2

K007 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K008 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K015 
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

1.7

Nickel
7440-02-0
NA

0.2

K021 
NA 
Table CCW in 268.43
Antimony 
7440-36-0
NA

0.23

K022 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

5.2

Nickel
7440-02-0
NA

0.32

K028 
NA 
Table CCW in 268.43
Chromium (Total) 
7440-47-32
NA

0.073

Lead
7439-92-1
NA

0.021

Nickel
7440-02-0
NA

0.088

K031 
NA 
Table CCW in 268.43
Arsenic 
7440-38-2
NA

5.6
(1)
K046 
NA 
Table CCW in 268.43
Lead 
7439-92-1
NA

0.18

K048 
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

1.7

Nickel
7440-02-0
NA

0.20

K049 
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

1.7

Nickel
7440-02-0
NA

0.20

K050 
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

1.7

Nickel
7440-02-0
NA

0.20

K051 
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

1.7

Nickel
7440-02-0
NA

0.20

K052 
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

1.7

Nickel
7440-02-0
NA

0.20

K061 (Low Zinc Subcategory-less than 15% Total Zinc)
NA 
Table CCW in 268.43
Cadmium
7440-43-9
NA

0.14

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.24

Nickel
7440-02-0
NA

0.32

K061 (High Zinc Subcategory-greater than 15% Total Zinc)-Effective until August 7th 1991).
 NA 
 Table CCW in 268.43
Cadmium
7440-43-9
NA

0.14

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.24

Nickel
7440-02-0
NA

0.32

K062 
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K069 (Calcium Sulfate Subcategory).
NA 
Table 2 in 268.42 and Table CCW in 268.43
Cadmium
7440-43-9
NA

0.14

Lead
7439-92-1
NA

0.24

K071 
NA 
Table CCW in 268.43
Mercury 
7439-97-6
NA

0.025

K083 
NA 
Table CCW in 268.43
Nickel 
7440-02-2
NA

0.088

K084 
NA 
Table CCW in 268.43
Arsenic 
7440-38-2
NA

5.6
(1)
K086
NA 
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

0.094

Lead
7439-92-1
NA

0.37

K087 
NA 
Table CCW in 268.43
Lead 
7439-92-1
NA

0.51

K100 
NA 
Table CCW in 268.43
Cadmium
7440-43-9
NA

0.066

Chromium (Total)
7440-47-32
NA

5.2

Lead
7439-92-1
NA

0.51

K101 
NA 
Table CCW in 268.43
Arsenic 
7440-38-2
NA

5.6
(1)
K102 
NA 
Table CCW in 268.43
Arsenic 
7440-38-2
NA

5.6
(1)
K106 (Low Mercury Subcategory- less than 260 mg/kg Mercury -residues from RMERC).
NA 
Table 2 in 268.42 and Table CCW in 268.43
Mercury 
7439-97-6
NA

0.020

K106 (Low Mercury Subcategory- less than 260 mg/kg Mercury-that are not residues from RMERC).
NA 
Table 2 in 268.42 and Table CCW in 268.43
Mercury 
7439-97-6
NA

0.025

K115 
NA 
Table CCW in 268.43
Nickel 
7440-02-0
NA

0.32

P010
Arsenic acid
Table CCW in 268.43
Arsenic
7440-38-2
NA

5.6
(1)
P011
Arsenic pentoxide
Table CCW in 268.43
Arsenic
7440-38-2
NA

5.6
(1)
P012
Arsenic trioxide
Table CCW in 268.43
Arsenic
7440-38-2
NA

5.6
(1)
P013
Barium cyanide
Table CCW in 268.43
Barium
7440-39-3
NA

52

P036
Dichlorophenylarsine
Table CCW in 268.43
Arsenic
7440-38-2
NA

5.6
(1)
P038
Diethylarsine
Table CCW in 268.43
Arsenic
7440-38-2
NA

5.6
(1)
P065 (Low Mercury Subcategory- Less than 260 mg/kg Mercury -residues from RMERC).
Mercury fulminate
Table 2 in 268.42 and Table CCW in 268.43
Mercury
7439-97-6
NA

0.20

P065 (Low Mercury Subcategory- Less than 260 mg/kg Mercury-incinerator residues (and are not residues from RMERC)).
Mercury fulminate
Table 2 in 268.42 and Table CCW in 268.43
Mercury
7439-97-6
NA

0.025

P073
Nickel carbonyl
Table CCW in 268.43
Nickel
7440-02-0
NA

0.32

P074
Nickel cyanide
Table CCW in 268.43
Nickel
7440-02-0
NA

0.32

P092 (Low Mercury Subcategory- Less than 260 mg/kg Mercury-residues from RMERC).
Phenyl mercury acetate
Table 2 in 268.42 and Table CCW in 268.43
Mercury
7439-97-6
NA

0.20

P092 (Low Mercury Subcategory- Less than 260 mg/kg Mercury-incinerator residues (and are not residues from RMERC)).
Phenyl mercury acetate
Table 2 in 268.42 and Table CCW in 268.43
Mercury
7439-97-6
NA

0.025

P099
Potassium silver cyanide
Table CCW in 268.43
Silver
7440-22-4
NA

0.072

P103
Selenourea
Table CCW in 268.43
Selenium
7782-49-2
NA

5.7

P104
Silver cyanide
Table CCW in 268.43
Silver
7440-22-4
NA

0.072

P110
Tetraethyl lead
Table CCW in 268.43
Lead
7439-92-1
NA

0.51

P114
Thallium selenite
Table CCW in 268.43
Selenium
7782-49-2
NA

5.7

U032
Calcium chromate
Table CCW in 268.43
Chromium (Total)
7440-47-32
NA

0.094

U051
Creosote
Table CCW in 268.43
Lead
7439-92-1
NA

0.51

U136
Cacodylic acid
Table CCW in 268.43
Arsenic
7440-38-2
NA

5.6
(1)
U144
Lead acetate
Table CCW in 268.43
Lead
7439-92-1
NA

0.51

U145
Lead phosphate
Table CCW in 268.43
Lead
7439-92-1
NA

0.51

U146
Lead subacetate
Table CCW in 268.43
Lead
7439-92-1
NA

0.51

U151 (Low Mercury Subcategory- Less than 260 mg/kg Mercury-residues from RMERC).
Mercury
Table CCW in 268.43 and Table 2 in 268.42
Mercury
7439-97-6
NA

0.20

U151 (Low Mercury Subcategory- Less than 260 mg/kg Mercury-that are not residues from RMERC.
Mercury
Table CCW in 268.43 and Table 2 in 268.42
Mercury
7439-97-6
NA

0.025

U204
Selenium dioxide
Table CCW in 268.43
Selenium
7782-49-2
NA

5.7

U205
Selenium sulfide
Table CCW in 268.43
Selenium
7782-49-2
NA

5.7

	

1These treatment standards have been based on EP Leachate analysis but this does not preclude the use of TCLP analysis.
2These waste codes are not subcategorized into wastewaters and nonwastewaters.
Note: NA means Not Applicable.

*   *   *   *   *

	11. In § 268.42 paragraph (a)(2), Table 1, Table 2, and Table 3 in paragraph (a) are revised, and paragraph (a)(3) is added preceding Tables 1-3 to read as follows:

§ 268.42  Treatment standards expressed as specified technologies.

	(a) * * *

	(2) Nonliquid hazardous wastes containing halogenated organic compounds (HOCs) in total concentration greater than or equal to 1,000 mg/kg and liquid HOC-containing wastes that are prohibited under § 268.32(e)(1) of this part must be incinerated in accordance with the requirements of 40 CFR part 264, subpart O, or 40 CFR part 265, subpart O. These treatment standards do not apply where the waste is subject to a part 268, subpart D, treatment standard for a specific HOC (such as a hazardous waste chlorinated solvent for which a treatment standard is established under § 268.41(a)).

	(3) A mixture consisting of wastewater, the discharge of which is subject to regulation under either section 402 or section 307(b) of the Clean Water Act, and de minimis losses of materials from manufacturing operations in which these materials are used as raw materials or are produced as products in the manufacturing process, and that meet the criteria of the D001 ignitable liquids containing greater than 10% total organic constituents (TOC) subcategory, is subject to the DEACT treatment standard described in Table 1 of this section. For purposes of this paragraph, de minimis losses include those from normal material handling operations (e.g., spills from the unloading or transfer of materials from bins or other containers, leaks from pipes, valves or other devices used to transfer materials); minor leaks from process equipment, storage tanks, or containers; leaks from well-maintained pump packings and seals; sample purgings; and relief device discharges.

Table 1._Technology Codes and Description of Technology_Based Standards

Technology code
Description of technology_based standards

ADGAS:
Venting of compressed gases into an absorbing or reacting media (i.e., solid or liquid)-venting can be accomplished through physical release utilizing valves/piping; physical penetration of the container; and/or penetration through detonation.

AMLGM:
Amalgamation of liquid, elemental mercury contaminated with radioactive materials utilizing inorganic reagents such as copper, zinc, nickel, gold, and sulfur that result in a nonliquid, semi_solid amalgam and thereby reducing potential emissions of elemental mercury vapors to the air.

BIODG:
Biodegradation of organics or non_metallic inorganics (i.e., degradable inorganics that contain the elements of phosphorus, nitrogen, and sulfur) in units operated under either aerobic or anaerobic conditions such that a surrogate compound or indicator parameter has been substantially reduced in concentration in the residuals (e.g., Total Organic Carbon can often be used as an indicator parameter for the biodegradation of many organic constituents that cannot be directly analyzed in wastewater residues).

CARBN:
Carbon adsorption (granulated or powdered) of non_metallic inorganics, organo_metallics, and/or organic constituents, operated such that a surrogate compound or indicator parameter has not undergone breakthrough (e.g., Total Organic Carbon can often be used as an indicator parameter for the adsorption of many organic constituents that cannot be directly analyzed in wastewater residues).  Breakthrough occurs when the carbon has become saturated with the constituent (or indicator parameter) and substantial change in adsorption rate associated with that constituent occurs.

CHOXD:

Chemical or electrolytic oxidation utilizing the following oxidation reagents (or waste reagents) or combinations of reagents: (1) Hypochlorite (e.g. bleach); (2) chlorine; (3) chlorine dioxide; (4) ozone or UV (ultraviolet light) assisted ozone; (5) peroxides; (6) persulfates; (7) perchlorates; (8) permangantes; and/or (9) other oxidizing reagents of equivalent efficiency, performed in units operated such that a surrogate compound or indicator parameter has been substantially reduced in concentration in the residuals (e.g., Total Organic Carbon can often be used as an indicator parameter for the oxidation of many organic constituents that cannot be directly analyzed in wastewater residues). Chemical oxidation specifically includes what is commonly referred to as alkaline chlorination.
CHRED:

Chemical reduction utilizing the following reducing reagents (or waste reagents) or combinations of reagents: (1) Sulfur dioxide; (2) sodium, potassium, or alkali salts or sulfites, bisulfites, metabisulfites, and polyethylene glycols (e.g., NaPEG and KPEG); (3) sodium hydrosulfide; (4) ferrous salts; and/or (5) other reducing reagents of equivalent efficiency, performed in units operated such that a surrogate compound or indicator parameter has been substantially reduced in concentration in the residuals (e.g., Total Organic Halogens can often be used as an indicator parameter for the reduction of many halogenated organic constituents that cannot be directly analyzed in wastewater residues).  Chemical reduction is commonly used for the reduction of hexavalent chromium to the trivalent state.
DEACT:

Deactivation to remove the hazardous characteristics of a waste due to is ignitability, corrosivity, and/or reactivity.
FSUBS:

Fuel substitution in units operated in accordance with applicable technical operating requirements.
HLVIT:

Vitrification of high level mixed radioactive wastes in units in compliance with all applicable radioactive protection requirements under control of the Nuclear Regulatory Commission.
IMERC:

Incineration of wastes containing organics and mercury in units operated in accordance with the technical operating requirements of 40 CFR part 264 subpart 0 and part 265 subpart 0.  All wastewater and nonwastewater residues derived from this process must then comply with the corresponding treatment standards per waste code with consideration of any applicable subcategories (e.g., High or Low Mercury Subcategories).
INCIN:

Incineration in units operated in accordance with the technical operating requirements of 40 CFR part 264 subpart 0 and part 265 subpart 0.
LLEXT:

Liquid_liquid extraction (often referred to as solvent extraction) of organics from liquid wastes into an immiscible solvent for which the hazardous constituents have a greater solvent affinity, resulting in an extract high in organics that must undergo either incineration, reuse as a fuel, or other recovery/reuse and a raffinate (extracted liquid waste) proportionately low in organics that must undergo further treatment as specified in the standard.
MACRO:

Macroencapsulation with surface coating materials such as polymeric organics (e.g. resins and plastics) or with a jacket of inert inorganic materials to substantially reduce surface exposure to potential leaching media.  Macroencapsulation specifically does not include any material that would be classified as a tank or container according to 40 CFR 260.10.
NEUTR:

Neutralization with the following reagents (or waste reagents) or combinations of reagents: (1) Acids; (2) bases; or (3) water (including wastewaters) resulting in a pH greater than 2 but less than 12.5 as measured in the aqueous residuals.
NLDBR:

No land disposal based on recycling.
PRECP:

Chemical precipitation of metals and other inorganics as insoluble precipitates of oxides, hydroxides, carbonates, sulfides, sulfates, chlorides, flourides, or phosphates.  The following reagents (or waste reagents) are typically used alone or in combination: (1) Lime (i.e., containing oxides and/or hydroxides of calcium and/or magnesium; (2) caustic (i.e., sodium and/or potassium hydroxides; (3) soda ash (i.e., sodium carbonate); (4) sodium sulfide; (5) ferric sulfate or ferric chloride; (6) alum; or (7) sodium sulfate.  Additional floculating, coagulation or similar reagents/processes that enhance sludge dewatering characteristics are not precluded from use.
RBERY:

Thermal recovery of Beryllium.
RCGAS:

Recovery/reuse of compressed gases including techniques such as reprocessing of the gases for reuse/resale; filtering/adsorption of impurities; remixing for direct reuse or resale; and use of the gas as a fuel source.
RCORR:

Recovery of acids or bases utilizing one or more of the following recovery technologies: (1) Distillation (i.e., thermal concentration); (2) ion exchange; (3) resin or solid adsorption; (4) reverse osmosis; and/or (5) incineration for the recovery of acid_Note: this does not preclude the use of other physical phase separation or concentration techniques such as decantation, filtration (including ultrafiltration), and centrifugation, when used in conjunction with the above listed recovery technologies.
RLEAD:

Thermal recovery of lead in secondary lead smelters.
RMERC:

Retorting or roasting in a thermal processing unit capable of volatilizing mercury and subsequently condensing the volatilized mercury for recovery. The retorting or roasting unit (or facility) must be subject to one or more of the following: (a) a National Emissions Standard for Hazardous Air Pollutants (NESHAP) for mercury; (b) a Best Available Control Technology (BACT) or a Lowest Achievable Emission Rate (LAER) standard for mercury imposed pursuant to a Prevention of Significant Deterioration (PSD) permit; or (c) a state permit that establishes emission limitations (within meaning of section 302 of the Clean Air Act) for mercury.  All wastewater and nonwastewater residues derived from this process must then comply with the corresponding treatment standards per waste code with consideration of any applicable subcategories (e.g., High or Low Mercury Subcategories).
RMETL:

Recovery of metals or inorganics utilizing one or more of the following direct physical/removal technologies: (1) Ion exchange; (2) resin or solid (i.e., zeolites) adsorption; (3) reverse osmosis; (4) chelation/solvent extraction; (5) freeze crystalization; (6) ultrafiltration and/or (7) simple precipitation (i.e., crystalization) - Note: This does not preclude the use of other physical phase separation or concentration techniques such as decantation, filtration (including ultrafiltration), and centrifugation, when used in conjunction with the above listed recovery technologies.
RORGS:

Recovery of organics utilizing one or more of the following technologies: (1) Distillation; (2) thin film evaporation; (3) steam stripping; (4) carbon adsorption; (5) critical fluid extraction; (6) liquid_ liquid extraction; (7) precipitation/crystalization (including freeze crystallization); or (8) chemical phase separation techniques (i.e., addition of acids, bases, demulsifiers, or similar chemicals); - Note: this does not preclude the use of other physical phase separation techniques such as a decantation, filtration (including ultrafiltration), and centrifugation, when used in conjunction with the above listed recovery technologies.
RTHRM:

Thermal recovery of metals or inorganics from nonwastewaters in units identified as industrial furnaces according to 40 CFR 260.10 (1), (6), (7), (11), and (12) under the definition of ``industrial furnaces''.
RZINC:

Resmelting in high temperature metal recovery units for the purpose of recovery of zinc.
STABL:

Stabilization with the following reagents (or waste reagents) or combinations of reagents: (1) Portland cement; or (2) lime/pozzolans (e.g., fly ash and cement kiln dust) - this does not preclude the addition of reagents (e.g., iron salts, silicates, and clays) designed to enhance the set/cure time and/or compressive strength, or to overall reduce the leachability of the metal or inorganic.
SSTRP:

Steam stripping of organics from liquid wastes utilizing direct application of steam to the wastes operated such that liquid and vapor flow rates, as well as, temperature and pressure ranges have been optimized, monitored, and maintained. These operating parameters are dependent upon the design parameters of the unit such as, the number of separation stages and the internal column design.  Thus, resulting in a condensed extract high in organics that must undergo either incineration, reuse as a fuel, or other recovery/reuse and an extracted wastewater that must undergo further treatment as specified in the standard.
WETOX:

Wet air oxidation performed in units operated such that a surrogate compound or indicator parameter has been substantially reduced in concentration in the residuals (e.g., Total Organic Carbon can often be used as an indicator parameter for the oxidation of many organic constituents that cannot be directly analyzed in wastewater residues).
WTRRX:

Controlled reaction with water for highly reactive inorganic or organic chemicals with precautionary controls for protection of workers from potential violent reactions as well as precautionary controls for potential emissions of toxic/ignitable levels of gases released during the reaction.

	Note 1:  When a combination of these technologies (i.e., a treatment train) is specified as a single treatment standard, the order of application is specified in § 268.42, Table 2 by indicating the five letter technology code that must be applied first, then the designation "fb." (an abbreviation for "followed by"), then the five letter technology code for the technology that must be applied next, and so on.

	Note 2:  When more than one technology (or treatment train) are specified as alternative treatment standards, the five letter technology codes (or the treatment trains) are separated by a semicolon (;) with the last technology preceded by the word "OR". This indicates that any one of these BDAT technologies or treatment trains can be used for compliance with the standard.

268.42 Table 2._Technology_Based Standards by RCRA Waste Code

	Technology code

Waste code
See also
Waste descriptions and/or treatment subcategory
CAS No.
for regulated
hazardous constituents
Wastewaters
Nonwastewaters

D001
NA
Ignitable Liquids based on 261.21(a)(1)-Wastewaters
NA
DEACT
NA

D001
NA
Ignitable Liquids based on 261.21(a)(1)-Low TOC Ingitable Liquids Subcategory-Less than 10% total organic carbon.
NA
NA

DEACT
D001
NA
Ignitable Liquids based on 261.21(a)(1)-High TOC Ingitable Liquids Subcategory-Greater than or equal to 10% total organic carbon.
NA
NA

FSUBS; RORGS; or INCIN
D001
NA
Ignitable compressed gases based on 261.21(a)(3)
NA
NA

DEACT2
D001
NA
Ignitable reactives based on 261.21(a)(2) 
NA
NA

DEACT
D001
NA
Oxidizers based on 261.21(a)(4)
NA
DEACT

DEACT
D002
NA
Acid subcategory based on 261.22(a)(1)
NA
DEACT

DEACT
D002
NA
Alkaline subcategory based on 261.22(a)(1)
NA
DEACT

DEACT
D002
NA
Other corrosives based on 261.22(a)(2)
NA
DEACT

DEACT
D003
NA
Reactive sulfides based on 261.23(a)(5)
NA
DEACT (may not be diluted)

DEACT (may not be diluted)
D003
NA
Explosives based on 261.23(a)(6),(7), and (8)
NA
DEACT

DEACT
D003
NA
Water reactives based on 261.23(a)(2), (3), and (4)
NA
NA

DEACT
D003
NA
Other reactives based on 261.23(a)(1)
NA
DEACT

DEACT
D006
NA
Cadmium containing batteries
7440_43_9
NA

RTHRM
D008
NA
Lead acid batteries (Note: This standard only applies to lead acid batteries that are identified as RCRA hazardous wastes and that are not excluded elsewhere from regulation under the land disposal restrictions of 40 CFR 268 or exempted under other EPA regulations (see 40 CFR 266.80.)
7439_92_1
NA

RLEAD
D009
Table CCWE in 268.41 and Table CCW in 268.43
Mercury: (High Mercury Subcategory_greater than or equal to 260 mg/kg total Mercury_contains mercury and organics (and are not incinerator residues))
7439_97_6
NA

IMERC; or RMERC
D009
Table CCWE in 268.41 and Table CCW in 268.43
Mercury: (High Mercury Subcategory-greater than or equal to 260 mg/kg total Mercury_inorganics (including
incinerator residues from RMERC))
7439_97_6
NA

RMERC
D012
Table CCW in 268.43
Endrin
72_20_8
BIODG; or INCIN

NA
D013
Table CCW in 268.43
Lindane
58_89_9
CARBN; or INCIN

NA
D014
Table CCW in 268.43
Methoxychlor
72_43_5
WETOX; or INCIN

NA
D015
Table CCW in 268.43
Toxaphene
8001_35_1
BIODG; or INCIN

NA
D016
Table CCW in 268.43
2,4_D
94_75_7
CHOXD; BIODG; or INCIN

NA
D017
Table CCW in 268.43
2,4,5_TP
93_72_1
CHOXD; or INCIN

NA
F005
Table CCWE in 268.41 and Table CCW in 268.43
2_Nitropropane
79_46_9
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
F005
Table CCWE in 268.41 and Table CCW in 268.43
2_Ethoxyethanol
110_80_5
BIODG; or INCIN

INCIN
F024
Table CCWE in 268.41 and Table CCW in 268.43

NA
INCIN

INCIN
K025
NA
Distillation bottoms from the production of nitrobenzene by the nitration of benzene
NA
LLEXT fb SSTRP fb CARBN; or INCIN

INCIN
K026
NA
Stripping still tails from the production of methyl ethyl pyridines
NA
INCIN

INCIN
K027
NA
Centrifuge and distillation residues from toluene diisocyanate production
NA
CARBN; or INCIN

FSUBS; or INCIN
K039
NA
Filter cake from the filtration of diethylphosphorodithioic acid in the production of phorate
NA
CARBN; or INCIN

FSUBS; or INCIN
K044
NA
Wastewater treatment sludges from the manufacturing and processing of explosives
NA
DEACT

DEACT
K045
NA
Spent carbon from the treatment of wastewater containing explosives
NA
DEACT

DEACT
K047
NA
Pink/red water from TNT operations
NA
DEACT

DEACT
K069
Table CCWE in 268.41 and Table CCW in 268.43
Emission control dust/sludge from secondary lead smelting: Non_Calcium Sulfate Subcategory

NA
NA
RLEAD
K106
Table CCWE in 268.41 and Table CCW in 268.43
Wastewater treatment sludge from the mercury cell process in chlorine production: (High Mercury Subcategory_greater than or equal to 260 mg/kg total mercury)

NA
NA
RMERC
K113
NA
Condensed liquid light ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene

NA
CARBN; or INCIN
FSUBS; or INCIN
K114
NA
Vicinals from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene

NA
CARBN; or INCIN
FSUBS; or INCIN
K115
NA
Heavy ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotolueme

NA
CARBN; or INCIN
FSUBS; or INCIN
K116
NA
Organic condensate from the solvent recovery colunm in the production of toluene diisocyanate via phosgenation of toluenediamine

NA
CARBN; or INCIN
FSUBS; or INCIN
P001
NA
Warfarin (>0.3%)

81_81_2
(WETOX or CHOXD) fb CARBN; or
INCIN
FSUBS; or INCIN
P002
NA
1_Acetyl_2_thiourea

591_08_2
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P003
Table CCW in 268.43
Acrolein

107_02_8
NA
FSUBS; or INCIN
P005
NA
Allyl alcohol

107_18_6
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

P006
NA
Aluminum phosphide

20859_73_8
CHOXD; CHRED; or INCIN
CHOXD; CHRED; or
INCIN
P007
NA
5_Aminoethyl 3_isoxazolol

2763_96_4
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P008
NA
4_Aminopyridine

504_24_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P009
NA
Ammonium picrate

131_74_8
CHOXD; CHRED, CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN
P014

NA
Thiophenol (Benzene thiol)
108_98_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P015

NA
Beryllium dust
7440_41_7
RMETL; or RTHRM
RMETL; or RTHRM
P016

NA
Bis(chloromethyl) ether
542_88_1
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P017

NA
Bromoacetone
598_31_2
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P018

NA
Brucine
357_57_3
(WETOX or CHOXD) fb CARBN; or
INCIN
INCIN
P022

Table CCW in 268.43
Carbon disulfide 
75_15_0
NA
INCIN
P023

NA
Chloroacetaldehyde
107_20_0
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P026

NA
1_(o_Chlorophenyl) thiourea
5344_82_1
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P027

NA
3_Chloropropionitrile
542_76_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P028

NA
Benzyl chloride
100_44_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P031

NA
Cyanogen
460_19_5
CHOXD; WETOX or INCIN
CHOXD; WETOX; or INCIN
P033

NA
Cyanogen chloride
506_77_4
CHOXD; WETOX or INCIN
CHOXD; WETOX; or
INCIN
P034

NA
2_Cyclohexyl_4,6_dinitrophenol
131_89_5
(WETOX or CHOXD) fb CARBN; or
INCIN
INCIN
P040

NA
O,O_Diethyl O_pyrazinyl phosphorothioate
297_97_2
CARBN; or INCIN
FSUBS; or INCIN
P041

NA
Diethyl_p_nitrophenyl phosphate
311_45_5
CARBN; or INCIN
FSUBS; or INCIN
P042

NA
Epinephrine
51_43_4
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P043
NA
Diisopropyl fluorophosphate (DFP)
55_91_4
CARBN; or INCIN
FSUBS; or INCIN

P044
NA
Dimethoate
60_51_5
CARBN; or INCIN
FSUBS or INCIN

P045
NA
Thiofanox
39196_18_4
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P046
NA
alpha,alpha_Dimethylphenethylamine
122-09_8
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P047
NA
4,6_Dinitro_o_cresol salts
534_52_1
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P049
NA
2,4_Dithiobiuret
541_53_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P054
NA
Aziridine
151_56_4
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P056
Table CCW in 268.43
Fluorine
7782_41_4
NA
ADAS fb NEUTR

P057
NA
Fluoroacetamide
640_19_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P058
NA
Fluoroacetic acid, sodium salt
62_74_8
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P062
NA
Hexaethyltetraphosphate
757_58_4
CARBN; or INCIN
FSUBS; or INCIN

P064
NA
Isocyanic acid, ethyl ester
624_83_9
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

P065
Table CCWE in 268.41 and Table CCW in 268.43
Mercury fulminate: (High Mercury Subcategory_greater than or equal to 260 mg/kg total Mercury_either incinerator residues or residues from RMERC)
628_86_4
NA
RMERC

P065
Table CCWE in 268.41 and Table CCW in 268.43
Mercury fulminate: (All Nonwastewasters that are not incinerator residues or are not residues from RMERC; regardless of Mercury Content)
628_86_4
NA
IMERC

P066
NA
Methomyl
16752_77_5
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
P067
NA
2_Methylaziridine
75_55_8
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
P068
NA
Methyl hydrazine
60_34_4
CHOXD; CHRED; CARBN; BIODG; or INCIN

FSUBS; CHOXD; CHRED; or INCIN
P069
NA
Methyllactonitrile
75_86_5
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
P070
NA
Aldicarb
116_06_3
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
P072
NA
1-Naphthyl-2-thiourea
86-88-4
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
P075
NA
Nicotine and salts
154_11_5
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
P076
NA
Nitric oxide
10102_43_9
ADGAS

ADGAS
P078
NA
Nitrogen dioxide
10102_44_0
ADGAS

ADGAS
P081
NA
Nitroglycerin
55_63_0
CHOXD; CHRED; CARBN; BIODG; or INCIN

FSUBS; CHOXD; CHRED; or INCIN
P082
Table CCW in 268.43
N_Nitrosodimethylamine
62_75_9
NA

INCIN
P084
NA
N_Nitrosomethylvinylamine
4549_40_0
(WETOX or CHOXD) fb CARBN; OR INCIN

INCIN
P085
NA
Octamethylpyrophosphoramide
152_16_9
CARBN; or INCIN

FSUBS; or INCIN
P087
NA
Osmium tetroxide
20816_12_0
RMETL; or RTHRM

RMETL; or RTHRM
P088
NA
Endothall
145_73_3
(WETOX or CHOXD) fb CARBN; or INCIN

FSUBS; or INCIN
P092
Table CCWE in 268.41 and Table CCW in 268.43
Phenyl mercury acetate: (High Mercury Subcategory_greater than or equal to 260 mg/kg total Mercury_either incinerator residues or residues from RMERC)
62_38_4
NA

RMERC
P092
Table CCWE in 268.41 and Table CCW in 268.43
Phenyl mercury acetate: (All nonwastewaters that are not incinerator residues and are not residues from RMERC: regardless of Mercury Content)

62_38_4
NA
IMERC; or RMERC
P093
NA
N_Phenylthiouea

103_85_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P095
NA
Phosgene

75_44_5
(WETOX or CHOXD) fb CARBN; or
INCIN
INCIN
P096
NA
Phosphine

7803_51_2
CHOXD; CHRED; or INCIN
CHOXD; CHRED; or
INCIN
P102
NA
Propargyl alcohol

107_19_7
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
P105
NA
Sodium azide

26628_22_8
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS, CHOXD; CHRED; or INCIN
P108
NA
Strychnine and salts

157_24_9
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P109
NA
Tetraethyldithiopyrophosphate

3689_24_5
CARBN; or INCIN
FSUBS; or INCIN
P112
NA
Tetranitromethane

509_14_8
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS, CHOXD; CHRED; or INCIN
P113
Table CCW in 268.43
Thallic oxide

1314_32_5
NA
RTHRM; or STABL
P115
Table CCW in 268.43
Thallium (1) sulfate

7446_18_6
NA
RTHRM; or STABL
P116
NA
Thiosemicarbazide

79_19_6
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P118
NA
Thrichloromethanethiol

75_70_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
P119
Table CCW in 268.43
Ammonium vanadate

7803_55_6
NA
STABL
P120
Table CCW in 268.43
Vanadium pentoxide

1314_62_1
NA
STABL
P122
NA
Zinc Phosphide (>10%)

1314_84_7
CHOXD; CHRED; or INCIN
CHOXD; CHRED; or INCIN
U001
NA
Acetaldehyde

75_07_0
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U003
Table CCW in 268.43

Acetonitrile
75_05_8
NA
INCIN
U006
NA

Acetyl Chloride
75_36_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U007
NA

Acrylamide
79_06_1
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U008
NA

Acrylic acid
79_10_7
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U010
NA

Mitomycin C
50_07_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U011
NA

Amitrole
61_82_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U014
NA

Auramine
492_80_8
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U015
NA

Azaserine
115_02_6
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U016
NA

Benz(c)acridine
225-51_4
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U017
NA

Benzal chloride
98_87_3
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U020
NA

Benzenesulfonyl chloride
98_09_9
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U021
NA

Benzidine
92_87_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U023
NA

Benzotrichloride
98_07_7
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN
U026
NA

Chlornaphazin
494_03_1
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U033
NA

Carbonyl fluoride
353_50_4
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U034
NA

Trichloroacetaldehyde (Chloral)
75_87_6
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U035
NA

Chlorambucil
305_03_3
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U038
Table CCW in 268.43

Chlorobenzilate
510_15_6
NA
INCIN
U041
NA

1_Chloro_2,3_epoxypropane (Epichlorohydrin)
106_89_8
(WETOX or CHOXD) fb CARBN; or
INCIN
INCIN
U042
Table CCW in 268.43

2_Chloroethyl vinyl ether
110_75_8
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U046
NA

Chloromethyl methyl ether
107_30_2
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U049
NA

4_Chloro_o_toluidine hydrochloride
3165_93_3
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U053
NA

Crotonaldehyde
4170_30_3
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U055
NA

Cumene
98_82_8
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U056
NA

Cyclohexane
110_82_7
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U057
Table CCW in 268.43

Cyclohexanone
108_94_1
NA
FSUBS; or INCIN
U058
NA

Cyclophosphamide
50_18_0
CARBN; or INCIN
FSUBS; or INCIN
U059
NA

Daunomycin
20830_81_3
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U062
NA

Diallate
2303_16_4
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U064
NA

1,2,7,8_Dibenzopyrene
189_55_9
(WETOX or CHOXD) fb CARBN or INCIN
FSUBS; or INCIN
U073
NA

3,3'_Dichlorobenzidine
91_94_1
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U074
NA

cis_1,4_Dichloro_2_butylene trans-1,4-Dichloro-2-butylene
1476_11_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U085
NA

1,2:3,4_Diepoxybutane
1464_53_5
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U086
NA

N,N_Diethylhydrazine
1615__80_1
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN
U087
NA

0,0_Diethyl S_methyldithiophosphate
3288_58_2
CARBN; or INCIN 
FSUBS; or INCIN
U089
NA

Diethyl stilbestrol
56_53_1
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U090
NA

Dihydrosafrole
94_58_6
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U091
NA

3,3'_Dimethoxybenzidine
119_90_4
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U092
NA

Dimethylamine
124_40_3
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U093
Table CCW in 268.43

p_Dimethylaminoazobenzene
621_90_9
NA
INCIN

U094
NA

7,12_Dimethyl benz(a)anthracene
57_97_6
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN
U095
NA

3,3'_Dimethylbenzidine
119_93_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U096
NA

a,a_Dimethyl benzyl hydroperoxide
80_15_9
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN
U097
NA

Dimethylcarbomyl chloride
79_44_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN
U098
NA

1,1_Dimethylhydrazine
57_14_7
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN

U099
NA
1,2_Dimethylhydrazine
540_73_8
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN

U103
NA
Dimethyl sulfate
77_78_1
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN

U109
NA
1,2_Diphenylhydrazine
122_66_7
CHOXD; CHRED; CARBN; BIODG; or INCIN
FSUBS; CHOXD; CHRED; or INCIN

U110
NA
Dipropylamine
142_84_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U113
NA
Ethyl acrylate
140_88_5
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U114
NA
Ethylene bis_dithiocarbamic acid
111_54_6
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U115
NA
Ethylene oxide
75_21_8
(WETOX or CHOXD) fb CARBN; or INCIN
CHOXD; or INCIN

U116
NA
Ethylene thiourea
96_45_7
(WETOX or CHOXD) fb CARBN; or
INCIN
INCIN

U119
NA
Ethyl methane sulfonate
62_50_0
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U122
NA
Formaldehyde
50_00_0
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U123
NA
Formic acid
64_18_6
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U124
NA
Furan
110_00_9
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U125
NA
Furfural
98_01_1
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U126
NA
Glycidaldehyde
765_34_4
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U132
NA
Hexachlorophenene
70_30_4
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U133
NA
Hydrazine
302_01_2
CHOXD; CHRED; CARBN; BIODG; or INCIN

FSUBS; CHOXD; CHRED; or INCIN
U134
Table CCW in 268.43
Hydrogen Flouride
7664_39_3
NA

ADGAS fb NEUTR; or NEUTR
U135
NA
Hydrogen Sulfide
7783_06_4
CHOXD; CHRED; or INCIN

CHOXD; CHRED; or INCIN
U143
NA
Lasiocarpine
303_34_4
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U147
NA
Maleic anhydride
108_31_6
(WETOX or CHOXD) fb CARBN; or INCIN

FSUBS; or INCIN
U148
NA
Maleic hydrazide
123_33_1
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U149
NA
Malononitrile
109_77_3
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U150
NA
Melphalan
148_82_3
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U151
Table CCWE in 268.41 and Table CCW in 268.43
Mercury: (High Mercury Subcategory_greater than or equal to 260 mg/kg total Mercury)
7439_97_6
NA

RMERC
U153
NA
Methane thiol
74_93_1
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U154
Table CCW in 268.43
Methanol
67_56_1
NA

FSUBS; or INCIN
U156
NA
Methyl chlorocarbonate
79_22_1
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U160
NA
Methyl ethyl ketone peroxide
1338_23_4
CHOXD; CHRED; CARBN; BIODG; or INCIN

FSUBS; CHOXD; CHRED; or INCIN

U163
NA
N_Methyl N'_nitro N_Nitrosoguanidine
70_25_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U164
NA
Methylthiouracil
56_04_2
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U166
NA
1,4_Naphthoquinone
130_15_4
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U167
NA
1_Naphthylamine
134_32_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U168
Table CCW in 268.43
2_Naphthlyamine
91_59_8
NA
INCIN

U171
NA
2_Nitropropane
79_46_9
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U173
NA
N_Nitroso_di_n_ethanolamine
1116_54_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U176
NA
N_Nitroso_N_ethylurea
759_73_9
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U177
NA
N_Nitroso_N_methylurea
684_93_5
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U178
NA
N_Nitroso_N_methylurethane
615_53_2
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U182
NA
Paraldehyde
123_63_7
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U184
NA
Pentachloroethane
76_01_7
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U186
NA
1,3_Pentadiene
504_60_9
(WETOX or CHOXD) fb CARBN; or INCIN
FSUBS; or INCIN

U189
NA
Phosphorus sulfide
1314_80_3
CHOXD; CHRED; or INCIN
CHOXD; CHRED; or INCIN

U191
NA
2_Picoline
109_06_8
(WETOX or CHOXD) fb CARBN; or INCIN
INCIN

U193
NA
1,3_Propane sultone
1120_71_4
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U194
NA
n_Propylamine
107_10_8
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U197
NA
p_Benzoquinone
106_51_4
(WETOX or CHOXD)

FSUBS; or INCIN
U200
NA
Reserpine
50_55_5
(WETOX or CHOXD) fb CARBN orINCIN

INCIN
U201
NA
Resorcinol
108_46_3
(WETOX or CHOXD) fb CARBN; or INCIN

FSUBS: or INCIN
U202
NA
Saccharin and salts
181_07_2
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U206
NA
Streptozatocin
18883_66_4
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U213
NA
Tetrahydrofuran
109_99_9
(WETOX or CHOXD) fb CARBN; or INCIN

FSUBS; or INCIN
U214
Table CCW in 268.43
Thallium (I) acetate
563_68_8
NA

RTHRM; or STABL
U215
Table CCW in 268.43
Thallium (I) carbonate
6533_73_9
NA

RTHRM; or STABL
U216
Table CCW in 268.43
Thallium (I) chloride
7791_12_0
NA

RTHRM; or STABL
U217
Table CCW in 268.43
Thallium (I) nitrate
10102_45_1
NA

RTHRM; or STABL
U218
NA
Thioacetamide
62_55_5
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U219
NA
Thiourea
62_56_6
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U221
NA
Toluenediamine
25376_45_8
CARBN; or INCIN

FSUBS; or INCIN
U222
NA
o_Toluidine hydrochloride
636_21_5
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U223
NA
Toluene diisocyanate
26471_62_5
CARBN; or INCIN

FSUBS; or INCIN
U234
NA
sym_Trinitrobenzene
99_35_4
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U236
NA
Trypan Blue
72_57_1
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U237
NA
Uracil mustard
66_75_1
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U238
NA
Ethyl carbamate
51_79_6
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U240
NA
2,4_Dichlorophenoxyacetic (salts and esters)
194_75_7
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U244
NA
Thiram
137_26_8
(WETOX or CHOXD) fb CARBN; or INCIN

INCIN
U246
NA
Cyanogen bromide
506_68_3
CHOXD; WETOX; or INCIN

CHOXD; WETOX; or
INCIN
U248
NA
Warfarin (.3% or less)
81_81_2
(WETOX or CHOXD) fb CARBN; or INCIN

FSUBS; or INCIN
U249
NA
Zinc Phosphide (<10%)
1314_84_7
CHOXD; CHRED; or INCIN

CHOXD; CHRED; or
INCIN

1CAS Number given for parent compound only.
2This waste code exists in gaseous form and is not categorized as wastewater or nonwastewater forms.
Note: NA means Not Applicable.

268.42 Table 3._Technology_Based Standards for Specific Radioactive Hazardous Mixed Waste

	Technology Code

Waste code
Waste descriptions and/or treatment category
CAS No.
Wastewaters
Nonwastewaters

D002
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA
HLVIT

D004
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT
D005
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT
D006
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT

D007
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT
D008
Radioactive lead solids subcategory (Note: these lead solids include, but are not limited to, all forms of lead shielding, and other elemental forms of lead. These lead solids do not include treatment residuals such as hydroxide sludges, other wastewater treatment residuals, or incinerator ashes that can undergo conventional pozzolanic stabilization, nor do they include organolead materials that can be incinerated and stabilized as ash).
7439_92_1
NA

MACRO
D008
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT
D009
Elemental mercury contaminated with radioactive materials
7439_97_6
NA

AMLGM
D009
Hydraulic oil contaminated with mercury; radioactive materials subcategory
7439_97_6
NA

IMERC
D009
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT
D010
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT
D011
Radioactive high level wastes generated during the reprocessing of fuel rods subcategory
NA
NA

HLVIT
U151
Mercury: Elemental mercury contaminated with radioactive materials
7439_97_6
NA

AMLGM

Note: NA means Not Applicable.
*   *   *   *   *