Vol. 61 No. 133 Wednesday, July 10, 1996 p. 36419

ENVIRONMENTAL PROTECTION AGENCY

40 CFR Part 268

[EPA #530_Z_96_002; FRL_5438_3]_

RIN 2050_AD38

Land Disposal Restrictions Phase III_Decharacterized Wastewaters, Carbamate Wastes, and Spent Potliners

AGENCY:   Environmental Protection Agency (EPA).

ACTION:   Corrections

Land Disposal Restrictions Phase III_Decharacterized Wastewaters,  Carbamate Wastes, and Spent Potliners  

Correction  

    In rule document 96_7597 beginning on page 15566 in the issue of Monday, April 8, 1996 make the following corrections:  
    
Sec. 268.40  [Corrected]  
  
    1. Beginning on page 15601, in the table Treatment Standards for Hazardous Wastes, the following entries are reprinted to correct typographical errors.  
* * * * *  

Note:  Amendments to the § 268.40 table "Treatment Standards for Hazardous Wastes" made April 8, 1996 (61 FR 15565 and 61 FR 15660), June 28, 1996 (61 FR 33680), and July 10, 1996 (61 FR 36419) are combined in the table published below.

TREATMENT STANDARDS FOR HAZARDOUS WASTES
[Note:  NA means not applicable]						
Waste Code	Waste Description and Treatment/Regulatory Subcategory1	REGULATED HAZARDOUS CONSTITUENT		WASTEWATERS	NONWASTEWATERS	
		Common Name	CAS2 No.	Concentration mg/l3; or Technology Code4	Concentration in mg/kg5 unless noted as "mg/l TCLP"; or Technology Code	
D001	Ignitable Characteristic Wastes, except for the § 261.21(a)(1) High TOC Subcategory.	NA	NA	DEACT and meet § 268.48 standards;8 or RORGS;9 or CMBST9	DEACT and meet § 268.48 standards;8 or RORGS;9 or CMBST9	
	High TOC Ignitable Characteristic Liquids Subcategory based on 40 CFR 261.21(a)(1) - Greater than or equal to 10% total organic carbon.  (Note:  This subcategory consists of nonwastewaters only).	NA	NA	NA	RORGS;9 or CMBST9	
D002	Corrosive Characteristic Wastes.	NA	NA	DEACT
and meet § 268.48 standards8	DEACT
and meet § 268.48 standards8	
D002, D004, D005, D006, D007, D008, D009, D010, D011	Radioactive high level wastes generated during the reprocessing of fuel rods.  (Note:  This subcategory consists of nonwastewaters only.)	Corrosivity (pH)	NA	NA	HLVIT	
		Arsenic	7440-38-2	NA	HLVIT	
		Barium	7440-39-3	NA	HLVIT	
		Cadmium	7440-43-9	NA	HLVIT	
		Chromium (Total)	7440-47-3	NA	HLVIT	
		Lead	7439-92-1	NA	HLVIT	
		Mercury	7439-97-6	NA	HLVIT	
		Selenium	7782-49-2	NA	HLVIT	
		Silver	7440-22-4	NA	HLVIT	
D003	Reactive Sulfides Subcategory based on 261.23(a)(5).	NA	NA	DEACT and meet §268.48 standards8	DEACT and meet §268.48 standards8	
	Explosives Subcategory based on 261.23(a)(6), (7), and (8).	NA	NA	DEACT and meet §268.48 standards8	DEACT and meet §268.48 standards8	
	Unexploded ordnance and other explosive devices which have been the subject of an emergency response.	NA	NA	DEACT	DEACT	
	Other Reactives Subcategory based on 261.23(a)(1).	NA	NA	DEACT and meet §268.48 standards8	DEACT and meet §268.48 standards8	
	Water Reactive Subcategory based on 261.23(a)(2), (3), and (4).  (Note:  This subcategory consists of nonwastewaters only).	NA	NA	NA	DEACT and meet §268.48 standards8	
	Reactive Cyanides Subcategory based on 261.23(a)(5).	Cyanides (Total)7	57-12-5	Reserved	590.9	
		Cyanides (Amenable).7	57-12-5	0.869	30.9	
D004	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for arsenic based on the extraction procedure (EP) in SW846 Methods 1310.	Arsenic	7440-38-2	5.0	5.0 mg/l EP	
		Arsenic; alternate6 standard for nonwastewaters only.	7440-38-2	NA	5.0 mg/l TCLP	
D005	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for barium based on the extraction procedure (EP) in SW846 Method 1310.	Barium	7440-39-3	100	100 mg/l TCLP	
D006	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for cadmium based on the extraction procedure (EP) in SW846 Method 1310.	Cadmium	7440-43-9	1.0	1.0 mg/l TCLP	
	Cadmium Containing Batteries Subcategory
(Note:  This subcategory consists of nonwastewaters only).	Cadmium	7440-43-9	NA	RTHRM	
D007	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for chromium based on the extraction procedure (EP) in SW846 Method 1310.	Chromium (Total)	7440-47-3	5.0	5.0 mg/l TCLP	
D008	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for lead based on the extraction procedure (EP) in SW846 Method 1310.	Lead	7439-92-1	5.0	5.0 mg/l EP	
		Lead; alternate6 standard for nonwastewaters only	7439-92-1	NA	5.0 mg/l TCLP	
	Lead Acid Batteries Subcategory (Note:  This standard only applies to lead acid batteries that are identified as RCRA hazardous wastes and that are not excluded elsewhere from regulation under the land disposal restrictions of 40 CFR 268 or exempted under other EPA regulations (see 40 CFR 266.80). This subcategory consists of nonwastewaters only.).	Lead	7439-92-1	NA	RLEAD	
	Radioactive Lead Solids Subcategory (Note:  these lead solids include, but are not limited to, all forms of lead shielding and other elemental forms of lead.  These lead solids do not include treatment residuals such as hydroxide sludges, other wastewater treatment residuals, or incinerator ashes that can undergo conventional pozzolanic stabilization, nor do they include organo-lead materials that can be incinerated and stabilized as ash.  This subcategory consists of nonwastewaters only).	Lead	7439-92-1	NA	MACRO	
D009	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain greater than or equal to 260 mg/kg total mercury that also contain organics and are not incinerator residues.  (High Mercury-Organic Subcategory)	Mercury	7439-97-6	NA	IMERC; OR RMERC	
	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain greater than or equal to 260 mg/kg total mercury that are inorganic, including incinerator residues and residues from RMERC.  (High Mercury-Inorganic Subcategory)	Mercury	7439-97-6	NA	RMERC	
	Nonwastewaters that exhibit, or are expected to exhibit, the characteristic of toxicity for mercury based on the extraction procedure (EP) in SW846 Method 1310; and contain less than 260 mg/kg total mercury.  (Low Mercury Subcategory.).	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	All D009 wastewaters.	Mercury	7439-97-6	0.20	NA	
	Elemental mercury contaminated with radioactive materials.
(Note:  This subcategory consists of nonwastewaters only.).	Mercury	7439-97-6	NA	AMLGM	
	Hydraulic oil contaminated with Mercury Radioactive Materials Subcategory.  (Note:  This subcategory consists of nonwastewaters only.).	Mercury	7439-97-6	NA	IMERC	
D010	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for selenium based on the extraction procedure (EP) in SW846 Method 1310.	Selenium	7782-49-2	1.0	5.7 mg/l TCLP	
D011	Wastes that exhibit, or are expected to exhibit, the characteristic of toxicity for silver based on the extraction procedure (EP) in SW846 Method 1310.	Silver	7440-22-4	5.0	5.0 mg/l TCLP	
D012	Wastes that are TC for Endrin based on the TCLP in SW846 Method 1311.	Endrin	72-20-8	BIODG;9 or CMBST9.	0.13
and meet § 268.48 standards8	
		Endrin aldehyde	7421-93-4	BIODG;9 or  CMBST9.	0.13
and meet § 268.48 standards8	
D013	Wastes that are TC for Lindane based on the TCLP in SW846 Method 1311.	alpha-BHC	319-84-6	CARBN;9 or  CMBST9.	0.066
and meet § 268.48 standards8	
		beta-BHC	319-85-7	CARBN;9 or  CMBST9.	0.066
and meet § 268.48 standards8	
		delta-BHC	319-86-8	CARBN;9 or  CMBST9.	0.066
and meet § 268.48 standards8	
		gamma-BHC (Lindane).	58-89-9	CARBN;9 or  CMBST9.	0.066
and meet § 268.48 standards8	
D014	Wastes that are TC for Methoxychlor based on the TCLP in SW846 Method 1311.	Methoxychlor	72-43-5	WETOX9 or  CMBST9.	0.18
and meet § 268.48 standards8	
D015	Wastes that are TC for Toxaphene based on the TCLP in SW846 Method 1311.	Toxaphene	8001-35-2	BIODG9 or  CMBST9.	2.6
and meet § 268.48 standards8	
D016	Wastes that are TC for 2,4-D(2,4-Dichlorophenoxyacetic acid) based on the TCLP in SW846 Method 1311.	2,4-D(2,4-Dichlorophenoxyacetic acid)	94-75-7	CHOXD;9 BIODG;9 or  CMBST9.	10
and meet § 268.48 standards8	
D017	Wastes that are TC for 2,4,5-TP (Silvex) based on the TCLP in SW846 Method 1311.	2,4,5-TP(Silvex)	93-72-1	CHOXD9 or  CMBST9.	7.9
and meet § 268.48 standards8	
D018	Wastes that are TC for Benzene based on the TCLP in SW846 Method 1311.	Benzene	71-43-2	0.14
and meet § 268.48 standards8.	10
and meet § 268.48 standards8	
D019	Wastes that are TC for Carbon tetrachloride based on the TCLP in SW846 Method 1311.	Carbon tetrachloride	56-23-5	0.057
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards8	
D020	Wastes that are TC for Chlordane based on the TCLP in SW846 Method 1311.	Chlordane (alpha and gamma isomers).	57-74-9	0.0033
and meet § 268.48 standards8.	0.26
and meet § 268.48 standards8	
D021	Wastes that are TC for Chlorobenzene based on the TCLP in SW846 Method 1311.	Chlorobenzene	108-90-7	0.057
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
D022	Wastes that are TC for Chloroform based on the TCLP in SW846 Method 1311.	Chloroform	67-66-3	0.046
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
D023	Wastes that are TC for o-Cresol based on the TCLP in SW846 Method 1311.	o-Cresol	95-48-7	0.11
and meet § 268.48 standards8.	5.6
and meet § 268.48 standards.8	
D024	Wastes that are TC for m-Cresol based on the TCLP in SW846 Method 1311.	M-Cresol
(difficult to distinguish from p-cresol).	108-39-4	0.77
and meet § 268.48 standards8.	5.6
and meet § 268.48 standards.8	
D025	Wastes that are TC for p-Cresol based on the TCLP in SW846 Method 1311.	p-Cresol
(difficult to distinguish from m-cresol).	106-44-5	0.77
and meet § 268.48 standards8.	5.6
and meet § 268.48 standards.8	
D026	Wastes that are TC for Cresols (Total) based on the TCLP in SW846 Method 1311.	Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations).	1319-77-3	0.88
and meet § 268.48 standards8.	11.2
and meet § 268.48 standards.8	
D027	Wastes that are TC for p-Dichloro- benzene based on the TCLP in SW846 Method 1311.	p-Dichlorobenzene (1,4-Dichlorobenzene)	106-46-7	0.090
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
D028	Wastes that are TC for 1,2-Dichloroethane based on the TCLP in SW846 Method 1311.	1,2-Dichloroethane	107-06-2	0.21
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
D029	Wastes that are TC for 1,1-Dichloroethylene based on the TCLP in SW846 Method 1311.	1,1-Dichlorethylene	75-35-4	0.025
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
D030	Wastes that are TC for 2,4-Dinitrotoluene based on the TCLP in SW846 Method 1311.	2,4-Dinitrotoluene	121-14-2	0.32
and meet § 268.48 standards8.	140
and meet § 268.48 standards.8	
D031	Wastes that are TC for Heptachlor based on the TCLP in SW846 Method 1311.	Heptachlor	76-44-8	0.0012
and meet § 268.48 standards8.	0.066
and meet § 268.48 standards.8	
		Heptachlor epoxide	1024-57-3	0.016
and meet § 268.48 standards8.	0.066
and meet § 268.48 standards.8	
D032	Wastes that are TC for Hexachloro- benzene based on the TCLP in SW846 Method 1311.	Hexachlorobenzene	118-74-1	0.055
and meet § 268.48 standards8.	10
and meet § 268.48 standards.8	
D033	Wastes that are TC for Hexachlorobutadiene based on the TCLP in SW846 Method 1311.	Hexachlorobutadiene	87-68-3	0.055
and meet § 268.48 standards8.	5.6
and meet § 268.48 standards.8	
D034	Wastes that are TC for Hexachloroethane based on the TCLP in SW846 Method 1311.	Hexachloroethane	67-72-1	0.055
and meet § 268.48 standards8.	30
and meet § 268.48 standards.8	
D035	Wastes that are TC for Methyl ethyl ketone based on the TCLP in SW846 Method 1311.	Methyl ethyl ketone	78-93-3	0.28
and meet § 268.48 standards8.	36
and meet § 268.48 standards.8	
D036	Wastes that are TC for Nitrobenzene based on the TCLP in SW846 Method 1311.	Nitrobenzene	98-95-3	0.068
and meet § 268.48 standards8.	14
and meet § 268.48 standards.8	
D037	Wastes that are TC for Pentachlorophenol based on the TCLP in SW846 Method 1311.	Pentachlorophenol	87-86-5	0.089
and meet § 268.48 standards8.	7.4
and meet § 268.48 standards.8	
D038	Wastes that are TC for Pyridine based on the TCLP in SW846 Method 1311.	Pyridine	110-86-1	0.014
and meet § 268.48 standards8.	16
and meet § 268.48 standards.8	
D039	Wastes that are TC for Tetrachloroethylene based on the TCLP in SW846 Method 1311.	Tetrachloroethylene	127-18-4	0.056
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
D040	Wastes that are TC for Trichloroethylene based on the TCLP in SW846 Method 1311.	Trichloroethylene	79-01-6	0.054
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
D041	Wastes that are TC for 2,4,5-Trichlorophenol based on the TCLP in SW846 Method 1311.	2,4,5-Trichlorophenol	95-95-4	0.18
and meet § 268.48 standards8.	7.4
and meet § 268.48 standards.8	
D042	Wastes that are TC for 2,4,6-Trichlorophenol based on the TCLP in SW846 Method 1311.	2,4,6-Trichlorophenol	88-06-2	0.035
and meet § 268.48 standards8.	7.4
and meet § 268.48 standards.8	
D043	Wastes that are TC for Vinyl chloride based on the TCLP in SW846 Method 1311.	Vinyl chloride	75-01-4	0.27
and meet § 268.48 standards8.	6.0
and meet § 268.48 standards.8	
F001, F002, F003, F004, & F005	F001, F002, F003, F004 and/or F005 solvent wastes that contain any combination of one or more of the following spent solvents:  acetone, benzene, n-butyl alcohol, carbon disulfide, carbon tetrachloride, chlorinated fluorocarbons, chlorobenzene, o-cresol, m-cresol, p-cresol, cyclohexanone, o-dichlorobenzene, 2-ethoxyethanol, ethyl acetate, ethyl benzene, ethyl ether, isobutyl alcohol, methanol, methylene chloride, methyl ethyl ketone, methyl isobutyl ketone, nitrobenzene, 2-nitropropane, pyridine, tetrachloroethylene, toluene, 1,1,1-trichloroethane, 1,1,2-trichloroethane, 1,1,2-trichloro-1,2,2-trifluorethane, trichloroethylene, trichloromonofluoromethane, and/or xylenes [except as specifically noted in other subcategories].  See further details of these listings in § 261.31.	Acetone	67-64-1	0.28	160	
		Benzene	71-42-2	0.14	10	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Carbon disulfide	75-15-0	3.8	NA	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chlorobenzene	108-90-7	0.057	6.0	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol).	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol).	106-44-5	0.77	5.6	
		Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations.	1319-77-3	0.88	11.2	
		Cyclohexanone	108-94-1	0.36	NA	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		Ethyl acetate	141-78-6	0.34	33	
		Ethyl benzene	100-41-4	0.057	10	
		Ethyl ether	60-29-7	0.12	160	
		Isobutyl alcohol	78-83-1	5.6	170	
		Methanol	67-56-1	5.6	NA	
		Methylene chloride	75-9-2	0.089	30	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Nitrobenzene	98-95-3	0.068	14	
		Pyridine	110-86-1	0.014	16	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		Toluene	108-88-3	0.080	10	
		1,1,1-Trichlorethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		1,1,2-Trichloro-1,2,2-trifluoroethane.	76-13-1	0.057	30	
		Trichloroethylene	79-01-6	0.054	6.0	
		Trichloromonofluoromethane	75-69-4	0.020	30	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations.	1330-20-7	0.32	30	
	F003 and/or F005 solvent wastes that contain any combination of one or more of the following three solvents as the only listed F001-5 solvents:  carbon disulfide, cyclohexanone, and/or methanol.  (formerly 268.41(c)).	Carbon disulfide	75-15-0	3.8	4.8 mg/l TCLP	
		Cyclohexanone	108-94-1	0.36	0.75 mg/l TCLP	
		Methanol	67-56-1	5.6	0.75 mg/l TCLP	
	F005 solvent waste containing 2-Nitropropane as the only listed F001-5 solvent..	2-Nitropropane	79-46-9	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
	F005 solvent waste containing 2-Ethoxyethanol as the only listed F001-5 solvent..	2-Ethoxyethanol	110-80-5	BIODG; or  CMBST	 CMBST	
F006	Wastewater treatment sludges from electroplating operations except from the following processes:  (1) Sulfuric acid anodizing of aluminum; (2) tin plating on carbon steel; (3) zinc plating (segregated basis) on carbon steel; (4) aluminum or zinc-aluminum plating on carbon steel; (5) cleaning/stripping associated with tin, zinc and aluminum plating on carbon steel; and (6) chemical etching and milling of aluminum.	Cadmium	7440-43-9	.069	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amendable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F007	Spent cyanide plating bath solutions from electroplating operations.	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F008	Plating bath residues from the bottom of plating baths from electroplating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F009	Spent stripping and cleaning bath solutions from electroplating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F010	Quenching bath residues from oil baths from metal heat treating operations where cyanides are used in the process.	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	NA	
F011	Spent cyanide solutions from salt bath pot cleaning from metal heat treating operations.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F012	Quenching wastewater treatment sludges from metal heat treating operations where cyanides are used in the process.	Cadmium	7440-43-9	NA	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
F019	Wastewater treatment sludges from the chemical conversion coating of aluminum except from zirconium phosphating in aluminum can washing when such phosphating is an exclusive conversion coating process.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
F020, F021, F022, F023, F026	Wastes (except wastewater and spent carbon from hydrogen chloride purification) from the production or manufacturing use (as a reactant, chemical intermediate, or component in a formulating process) of:  (1) tri- or tetrachlorophenol, or of intermediates used to produce their pesticide derivatives, excluding wastes from the production of Hexachlorophene from highly purified 2,4,5-trichlorophenol (F020); (2) pentachlorophenol, or of intermediates used to produce its derivatives (i.e., F021); (3) tetra-, penta-, or hexachlorobenzenes under alkaline conditions (i.e., F022); and from the production of materials on equipment previously used for the production or manufacturing use (as a reactant, chemical intermediate, or component in a formulating process) of:  (1) tri- or tetrachlorophenols, excluding wastes from equipment used only for the production of Hexachlorophene from highly purified 2,4,5-trichlorophenol (F023); (2) tetra-, penta-, or hexachlorobenzenes under alkaline conditions (i.e., F026).	HxCDDs (All Hexachlorodibenzo-p-dioxins).	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans).	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins).	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans).	NA	0.000035	0.001	
		Pentachlorophenol	87-86-5	0.089	7.4	
		TCDDs (All Tetrachlorodibenzo-p-dioxins).	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans).	NA	0.000063	0.001	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
F024	Process wastes, including but not limited to, distillation residues, heavy ends, tars, and reactor clean-out wastes, from the production of certain chlorinated aliphatic hydrocarbons by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.  (This listing does not include wastewaters, wastewater treatment sludges, spent catalysts, and wastes listed in § 261.31 or § 261.32.).	All F024 wastes	NA	 CMBST	 CMBST	
		2-Chloro-1,3-butadiene	126-99-8	0.057	0.28	
		3-Chloropropylene	107-05-1	0.036	30	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,2-Dichloropropane	78-87-5	0.85	18	
		cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Hexachloroethane	67-72-1	0.055	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
F025	Condensed light ends from the production of certain chlorinated aliphatic hydrocarbons, by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.
F025 - Light Ends Subcategory	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		Methylene chloride	75-9-2	0.089	30	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
	Spent filters and filter aids, and spent desiccant wastes from the production of certain chlorinated aliphatic hydrocarbons, by free radical catalyzed processes.  These chlorinated aliphatic hydrocarbons are those having carbon chain lengths ranging from one to and including five, with varying amounts and positions of chlorine substitution.
F025 - Spent Filters/Aids and Desiccants Subcategory	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Methylene chloride	75-9-2	0.089	30	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
F027	Discarded unused formulations containing tri-, tetra-, or pentachlorophenol or discarded unused formulations containing compounds derived from these chlorophenols.  (This listing does not include formulations containing hexachlorophene synthesized from prepurified 2,4,5-trichlorophenol as the sole component).	HxCDDs (All Hexachlorodibenzo-p-dioxins).	NA	 0.059	NA	
		HxCDFs (All Hexachlorodibenzofurans).	NA	0.059	3.4	
		PeCDDs (All Pentachlorodibenzo-p-dioxins).	NA	0.14	10	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.059	3.4	
		Pentachlorophenol	87-86-5	0.061	3.4	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.28	28	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.059	3.4	
		2,4,5-Trichlorophenol	95-95-4	0.057	28	
		2,4,6-Trichlorophenol	88-06-2	0.057	10	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.059	NA	
F028	Residues resulting from the incineration or thermal treatment of soil contaminated with EPA Hazardous Wastes Nos. F020, F021, F023, F026, and F027.	HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.059	5.6	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.059	5.6	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.039	6.2	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.067	8.2	
		Pentachlorophenol	87-86-5	0.080	10	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.32	30	
		TCDFs (All Tetrachlorodibenzofurans)	NA	2.77	0.86 mg/l TCLP	
		2,4,5-Trichlorophenol	95-95-4	1.2	590	
		2,4,6-Trichlorophenol	88-06-2	0.69	NA	
		2,3,4,6-Tetrachlorophenol	58-90-2	3.98	5.0 mg/l TCLP	
F037	Petroleum refinery primary oil/water/solids separation sludge-Any sludge generated from the gravitational separation of oil/water/solids during the storage or treatment of process wastewaters and oily cooling wastewaters from petroleum refineries.  Such sludges include, but are not limited to, those generated in:  oil/water/solids separators; tanks and impoundments; ditches and other conveyances; sumps; and stormwater units receiving dry weather flow.  Sludge generated in stormwater units that do not receive dry weather flow, sludges generated from non-contact once-through cooling waters segregated for treatment from other process or oily cooling waters, sludges generated in aggressive biological treatment units as defined in § 261.31(b)(2) (including sludges generated in one or more additional units after wastewaters have been treated in aggressive biological treatment units) and K051 wastes are not included in this listing.	Acenaphthene	83-32-9	0.059	3.4	
		Anthracene	120-12-7	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
F038	Petroleum refinery secondary (emulsified) oil/water/solids separation sludge and/or float generated from the physical and/or chemical separation of oil/water/solids in process wastewaters and oily cooling wastewaters from petroleum refineries.  Such wastes include, but are not limited to, all sludges and floats generated in:  induced air floatation (IAF) units, tanks and impoundments, and all sludges generated in DAF units.  Sludges generated in stormwater units that do not receive dry weather flow, sludges generated from non-contact once-through cooling waters segregated for treatment from other process or oily cooling waters, sludges and floats generated in aggressive biological treatment units as defined in § 261.31(b)(2) (including sludges and floats generated in one or more additional units after wastewaters have been treated in aggressive biological units) and F037, K048, and K051 are not included in this listing.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations).	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
F039	Leachate (liquids that have percolated through land disposed wastes) resulting from the disposal of more than one restricted waste classified as hazardous under subpart D of this part.  (Leachate resulting from the disposal of one or more of the following EPA Hazardous Wastes and no other Hazardous Wastes retains its EPA Hazardous Waste Number(s):  F020, F021, F022, F026, F027, and/or F028.).	Acenaphthylene	208-96-8	0.059	3.4	
		Acenaphthene	83-32-9	0.059	3.4	
		Acetone	67-64-1	0.28	160	
		Acetonitrile	75-05-8	5.6	NA	
		Acetophenone	96-86-2	0.010	9.7	
		2-Acetylaminofluorene	53-96-3	0.059	140	
		Acrolein	107-02-8	0.29	NA	
		Acrylonitrile	107-13-1	0.24	84	
		Aldrin	309-00-2	0.021	0.066	
		4-Aminobiphenyl	92-67-1	0.13	NA	
		Aniline	62-53-3	0.81	14	
		Anthracene	120-12-7	0.059	3.4	
		Aramite	140-57-8	0.36	NA	
		alpha-BHC	319-84-6	0.00014	0.066	
		beta-BHC	319-85-7	0.00014	0.066	
		delta-BHC	319-86-8	0.023	0.066	
		gamma-BHC	58-89-9	0.0017	0.066	
		Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Benzo(g,h,i)perylene	191-24-2	0.0055	1.8	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Bromodichloromethane	75-27-4	0.35	15	
		Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		4-Bromophenyl phenyl ether	101-55-3	0.055	15	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Butyl benzyl phthalate	85-68-7	0.017	28	
		2-sec-Butyl-4,6-dinitrophenol (Dinoseb).	88-85-7	0.066	2.5	
		Carbon disulfide	75-15-0	3.8	NA	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chlordane (alpha and gamma isomers).	57-74-9	0.0033	0.26	
		p-Chloroaniline	106-47-8	0.46	16	
		Chlorobenzene	108-90-7	0.057	6.0	
		Chlorobenzilate	510-15-6	0.10	NA	
		2-Chloro-1,3-butadiene	126-99-8	0.057	NA	
		Chlorodibromomethane	124-48-1	0.057	15	
		Chloroethane	75-00-3	0.27	6.0	
		bis(2-Chloroethoxy)methane	111-91-1	0.036	7.2	
		bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		Chloroform	67-66-3	0.046	6.0	
		bis(2-Chloroisopropyl)ether	39638-32-9	0.055	7.2	
		p-Chloro-m-cresol	59-50-7	0.018	14	
		Chloromethane (Methyl chlorida)	74-87-3	0.19	30	
		2-Chloronaphthalene	91-58-7	0.055	5.6	
		2-Chlorophenol	95-57-8	0.044	5.7	
		3-Chloropropylene	107-05-1	0.036	30	
		Chrysene	218-01-9	0.059	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol).	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol).	106-44-5	0.77	5.6	
		Cyclohexanone	108-94-1	0.36	NA	
		1,2-Dibromo-3-chloropropane	96-12-8	0.11	15	
		Ethylene dibromide (1,2-Dibromoethane).	106-93-4	0.028	15	
		Dibromomethane	74-95-3	0.11	15	
		2,4-D (2,4-Dichlorophenoxyacetic acid).	94-75-7	0.72	10	
		o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
		o,p'-DDE	3424-82-6	0.031	0.087	
		p,p'-DDE	72-55-9	0.031	0.087	
		o,p'-DDT	789-02-6	0.0039	0.087	
		p,p'-DDT	50-29-3	0.0039	0.087	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Dibenz(a,e)pyrene	192-65-4	0.061	NA	
		m-Dichlorobenzene	541-73-1	0.036	6.0	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Dichlorodifluoromethane	75-71-8	0.23	7.2	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		trans-1,2-Dichloroethylene	156-60-5	0.054	30	
		2,4-Dichlorophenol	120-83-2	0.044	14	
		2,6-Dichlorophenol	87-65-0	0.044	14	
		1,2-Dichloropropane	78-87-5	0.85	18	
		cis-1,3-Dichloropropylene	10061-01-5	0.036	18	
		trans-1,3-Dichloropropylene	10061-02-6	0.036	18	
		Dieldrin	60-57-1	0.017	0.13	
		Diethyl phthalate	84-66-2	0.20	28	
		2-4-Dimethyl phenol	105-67-9	0.036	14	
		Dimethyl phthalate	131-11-3	0.047	28	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		1,4-Dinitrobenzene	100-25-4	0.32	2.3	
		4,6-Dinitro-o-cresol	534-52-1	0.28	160	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		2,4-Dinitrotoluene	121-14-2	0.32	140	
		2,6-Dinitrotoluene	606-20-2	0.55	28	
		Di-n-octyl phthalate	117-84-0	0.017	28	
		Di-n-propylnitrosamine	621-64-7	0.40	14	
		1,4-Dioxane	123-91-1	12.0	170	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine).	122-39-4	0.92	NA	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine).	86-30-6	0.92	NA	
		1,2-Diphenylhydrazine	122-66-7	0.087	NA	
		Disulfoton	298-04-4	0.017	6.2	
		Endosulfan I	939-98-8	0.023	0.066	
		Endosulfan II	33213-6-5	0.029	0.13	
		Endosulfan sulfate	1-31-07-8	0.029	0.13	
		Endrin	72-20-8	0.0028	0.13	
		Endrin aldehyde	7421-93-4	0.025	0.13	
		Ethyl acetate	141-78-6	0.34	33	
		Ethyl cyanide (Propanenitrile)	107-12-0	0.24	360	
		Ethyl benzene	100-41-4	0.057	10	
		Ethyl ether	60-29-7	0.12	160	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Ethyl methacrylate	97-63-2	0.14	160	
		Ethylene oxide	75-21-8	0.12	NA	
		Famphur	52-85-7	0.017	15	
		Fluoranthene	206-44-0	0.068	3.4	
		Fluorene	86-73-7	0.059	3.4	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		Hexachloroethane	67-72-1	0.055	30	
		Hexachloropropylene	1888-71-7	0.035	30	
		Indeno (1,2,3-c,d) pyrene	193-39-5	0.0055	3.4	
		Iodomethane	74-88-4	0.19	65	
		Isobutyl alcohol	78-83-1	5.6	170	
		Isodrin	465-73-6	0.021	0.066	
		Isosafrole	120-58-1	0.081	2.6	
		Kepone	143-50-8	0.0011	0.13	
		Methacrylonitrile	126-98-7	0.24	84	
		Methanol	67-56-1	5.6	NA	
		Methapyrilene	91-80-5	0.081	1.5	
		Methoxychlor	72-43-5	0.25	0.18	
		3-Methylcholanthrene	56-49-5	0.0055	15	
		4,4-Methylene bis(2-chloroaniline)	101-14-4	0.50	30	
		Methylene chloride	75-09-2	0.089	30	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Methyl methacrylate	80-62-6	0.14	160	
		Methyl methansulfonate	66-27-3	0.018	NA	
		Methyl parathion	298-00-0	0.014	4.6	
		Naphthalene	91-20-3	0.059	5.6	
		2-Naphthylamine	91-59-8	0.52	NA	
		p-Nitroaniline	100-01-6	0.028	28	
		Nitrobenzene	98-95-3	0.068	14	
		5-Nitro-o-toluidine	99-55-8	0.32	28	
		p-Nitrophenol	100-02-7	0.12	29	
		N-Nitrosodiethylamine	55-18-5	0.40	28	
		N-Nitrosodimethylamine	62-75-9	0.40	NA	
		N-Nitroso-di-n-butylamine	924-16-3	0.40	17	
		N-Nitrosomethylethylamine	10595-95-6	0.40	2.3	
		N-Nitrosomorpholine	59-89-2	0.40	2.3	
		N-Nitrosopiperidine	100-75-4	0.013	35	
		N-Nitrosopyrrolidine	930-55-2	0.013	35	
		Parathion	56-38-2	0.014	4.6	
		Total PCBs
(sum of all PCB isomers, or all Aroclors)	1336-36-3	0.10	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		Pentachloronitrobenzene	82-68-8	0.055	4.8	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenacetin	62-44-2	0.081	16	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Phorate	298-02-2	0.021	4.6	
		Phthalic anhydride	85-44-9	0.055	NA	
		Pronamide	23950-58-5	0.093	1.5	
		Pyrene	129-00-0	0.067	8.2	
		Pyridine	110-86-1	0.014	16	
		Safrole	94-59-7	0.081	22	
		Silvex (2,4,5-TP)	93-72-1	0.72	7.9	
		2,4,5-T	93-76-5	0.72	7.9	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		TCDDs (All Tetrachlorodibenzo-p-dioxins).	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Toluene	108-88-3	0.080	10	
		Toxaphene	8001-35-2	0.0095	2.6	
		Bromoform (Tribromomethane)	75-25-2	0.63	15	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Trichloromonofluoromethane	75-69-4	0.020	30	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		1,2,3-Trichloropropane	96-18-4	0.85	30	
		1,1,2-Trichloro-1,2,2-trifluoroethane	76-13-1	0.057	30	
		tris(2,3-Dibromopropyl) phosphate.	126-72-7	0.11	NA	
		Vinyl chloride	75-01-4	0.27	6.0	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Antimony	7440-36-0	1.9	2.1 mg/l TCLP	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Barium	7440-39-3	1.2	7.6 mg/l TCLP	
		Beryllium	7440-41-7	0.82	NA	
		Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)	57-12-5	0.86	NA	
		Fluoride	16964-48-8	35	NA	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Mercury	7439-97-6	0.15	0.025 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
		Sulfide	8496-25-8	14	NA	
		Thallium	7440-28-0	1.4	NA	
		Vanadium	7440-62-2	4.3	NA	
K001	Bottom sediment sludge from the treatment of wastewaters from wood preserving processes that use creosote and/or pentachlorophenol..	Naphthalene	91-20-3	0.059	5.6	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenanthrene	85-01-8	0.059	5.6	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations).	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K002	Wastewater treatment sludge from the production of chrome yellow and orange pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K003	Wastewater treatment sludge from the production of molybdate orange pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K004	Wastewater treatment sludge from the production of zinc yellow pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K005	Wastewater treatment sludge from the production of chrome green pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
K006	Wastewater treatment sludge from the production of chrome oxide green pigments (anhydrous).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
	Wastewater treatment sludge from the production of chrome oxide green pigments (hydrated).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K007	Wastewater treatment sludge from the production of iron blue pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
K008	Oven residue from the production of chrome oxide green pigments.	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K009	Distillation bottoms from the production of acetaldehyde from ethylene.	Chloroform	67-66-3	0.046	6.0	
K010	Distillation side cuts from the production of acetaldehyde from ethylene.	Chloroform	67-66-3	0.046	6.0	
K011	Bottom stream from the wastewater stripper in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	38	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K013	Bottom stream from the acetonitrile column in the production of acrylonitrile..	Acetonitrile	75-05-8	5.6	38	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K014	Bottoms from the acetonitrile purification column in the production of acrylonitrile.	Acetonitrile	75-05-8	5.6	38	
		Acrylonitrile	107-13-1	0.24	84	
		Acrylamide	79-06-1	19	23	
		Benzene	71-43-2	0.14	10	
		Cyanide (Total)	57-12-5	1.2	590	
K015	Still bottoms from the distillation of benzyl chloride.	Anthracene	120-12-7	0.059	3.4	
		Benzal chloride	98-87-3	0.055	6.0	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene.	205-99-2	0.11	6.8	
		Benzo(k)fluroanthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Phenanthrene	85-01-8	0.059	5.6	
		Toluene	108-88-3	0.080	10	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K016	Heavy ends or distillation residues from the production of carbon tetrachloride.	Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		Hexachloroethane	67-72-1	0.055	30	
		Tetrachloroethylene	127-18-4	0.056	6.0	
K017	Heavy ends (still bottoms) from the purification column in the production of epichlorohydrin.	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		1,2-Dichloropropane	78-87-5	0.85	18	
		1,2,3-Trichloropropane	96-18-4	0.85	30	
K018	Heavy ends from the fractionation column in ethyl chloride production.	Chloroethane	75-00-3	0.27	6.0	
		Chloromethane	74-87-3	0.19	NA	
		1,1-Dichloroethane	75-34-3	0.059	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	NA	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K019	Heavy ends from the distillation of ethylene dichloride in ethylene dichloride production..	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
		Chlorobenzene	108-90-7	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		p-Dichlorobenzene	106-46-7	0.090	NA	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		Fluorene	86-73-7	0.059	NA	
		Hexachloroethane	67-72-1	0.055	30	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	NA	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K020	Heavy ends from the distillation of vinyl chloride in vinyl chloride monomer production.	1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
K021	Aqueous spent antimony catalyst waste from fluoromethanes production.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Antimony	7440-36-0	1.9	2.1 mg/l TCLP	
K022	Distillation bottom tars from the production of phenol/acetone from cumene.	Toluene	108-88-3	0.080	10	
		Acetophenone	96-86-2	0.010	9.7	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine).	122-39-4	0.92	13	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine).	86-30-6	0.92	13	
		Phenol	108-95-2	0.039	6.2	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K023	Distillation light ends from the production of phthalic anhydride from naphthalene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	85-44-9	0.055	28	
K024	Distillation bottoms from the production of phthalic anhydride from naphthalene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	85-44-9	0.055	28	
K025	Distillation bottoms from the production of nitrobenzene by the nitration of benzene.	NA	NA	LLEXT fb SSTRP fb CARBN; or  CMBST	 CMBST	
K026	Stripping still tails from the production of methyl ethyl pyridines.	NA	NA	 CMBST	 CMBST	
K027	Centrifuge and distillation residues from toluene diisocyanate production.	NA	NA	CARBN; or  CMBST	CMBST	
K028	Spent catalyst from the hydrochlorinator reactor in the production of 1,1,1-trichloroethane.	1,1-Dichloroethane	75-34-3	0.059	6.0	
		trans-1,2-Dichloroethylene	156-60-5	0.054	30	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	NA	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Cadmium	7440-43-9	0.69	NA	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K029	Waste from the product steam stripper in the production of 1,1,1-trichloroethane.	Chloroform	67-66-3	0.046	6.0	
		1,2-Dichloroethane	107-06-2	0.21	6.0	
		1,1-Dichloroethylene	75-35-4	0.025	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		Vinyl chloride	75-01-4	0.27	6.0	
K030	Column bodies or heavy ends from the combined production of trichloroethylene and perchloroethylene.	o-Dichlorobenzene	95-50-1	0.088	NA	
		p-Dichlorobenzene	106-46-7	0.090	NA	
		Hexachlorobutadiene	87-68-3	0.055	5.6	
		Hexachloroethane	67-72-1	0.055	30	
		Hexachloropropylene	1888-71-7	NA	30	
		Pentachlorobenzene	608-93-5	NA	10	
		Pentachloroethane	76-01-7	NA	6.0	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K031	By-product salts generated in the production of MSMA and cacodylic acid.	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
K032	Wastewater treatment sludge from the production of chlordane.	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
		Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
K033	Wastewater and scrub water from the chlorination of cyclopentadiene in the production of chlordane.	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
K034	Filter solids from the filtration of hexachlorocyclopentadiene in the production of chlordane.	Hexachlorocylopentadiene	77-47-4	0.057	2.4	
K035	Wastewater treatment sludges generated in the production of creosote.	Acenaphthene	83-32-9	NA	3.4	
		Anthracene	120-12-7	NA	3.4	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Chrysene	218-01-9	0.059	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		Dibenz(a,h)anthracene	53-70-3	NA	8.2	
		Fluoranthene	206-44-0	0.068	3.4	
		Fluorene	86-73-7	NA	3.4	
		Indeno(1,2,3-cd)pyrene	193-39-5	NA	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
K036	Still bottoms from toluene reclamation distillation in the production of disulfoton.	Disulfoton	298-04-4	0.017	6.2	
K037	Wastewater treatment sludges from the production of disulfoton.	Disulfoton	298-04-4	0.017	6.2	
		Toluene	108-88-3	0.080	10	
K038	Wastewater from the washing and stripping of phorate production.	Phorate	298-02-2	0.021	4.6	
K039	Filter cake from the filtration of diethylphosphorodithioc acid in the production of phorate.	NA	NA	CARBN; or  CMBST	CMBST	
K040	Wastewater treatment sludge from the production of phorate.	Phorate	298-02-2	0.021	4.6	
K041	Wastewater treatment sludge from the production of toxaphene.	Toxaphene	8001-35-2	0.0095	2.6	
K042	Heavy ends or distillation residues from the distillation of tetrachlorobenzene in the production of 2,4,5-T.	o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K043	2,6-Dichlorophenol waste from the production of 2,4-D.	2,4-Dichlorophenol	120-83-2	0.044	14	
		2,6-Dichlorophenol	187-65-0	0.044	14	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
		2,3,4,6-Tetrachlorophenol	58-90-2	0.030	7.4	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		HxCDDs (All Hexachlorodibenzo-p-dioxins).	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans).	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins).	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans).	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins).	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans).	NA	0.000063	0.001	
K044	Wastewater treatment sludges from the manufacturing and processing of explosives.	NA	NA	DEACT	DEACT	
K045	Spent carbon from the treatment of wastewater containing explosives.	NA	NA	DEACT	DEACT	
K046	Wastewater treatment sludges from the manufacturing, formulation and loading of lead-based initiating compounds.	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K047	Pink/red water from TNT operations.	NA	NA	DEACT	DEACT	
K048	Dissolved air flotation (DAF) float from the petroleum refining industry.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	218-01-9	0.059	3.4	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-33	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations).	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K049	Slop oil emulsion solids from the petroleum refining industry.	Anthracene	120-12-7	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Carbon disulfide	75-15-0	3.8	NA	
		Chrysene	2218-01-9	0.059	3.4	
		2,4-Dimethylphenol	105-67-9	0.036	NA	
		Ethylbenzene	100-41-4	0.057	10	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-. and p-xylene concentrations)	1330-20-7	0.32	30	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K050	Heat exchanger bundle cleaning sludge from the petroleum refining industry.	Benzo(a)pyrene	50-32-8	0.061	3.4	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K051	API separator sludge from the petroleum refining industry.	Acenaphthene	83-32-9	0.059	NA	
		Anthracene	120-12-7	0.059	3.4	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		Chrysene	2218-01-9	0.059	3.4	
		Di-n-butyl phthalate	105-67-9	0.057	28	
		Ethylbenzene	100-41-4	0.057	10	
		Fluorene	86-73-7	0.059	NA	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.08	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Cyanides (Total)7	57-12-5	1.2	590	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K052	Tank bottoms (leaded) from the petroleum refining industry.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		o-Cresol	95-48-7	0.11	5.6	
		m-Cresol
(difficult to distinguish from p-cresol)	108-39-4	0.77	5.6	
		p-Cresol
(difficult to distinguish from m-cresol)	106-44-5	0.77	5.6	
		2,4-Dimethylphenol	105-67-9	0.036	NA	
		Ethylbenzene	100-41-4	0.057	10	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Toluene	108-88-3	0.08	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	NA	
		Nickel	7440-02-0	NA	5.0 mg/l TCLP	
K060	Ammonia still lime sludge from coking operations.	Benzene	71-43-2	0.14	10	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
K061	Emission control dust/sludge from the primary production of steel in electric furnaces.	Antimony	7440-36-0	NA	2.1 mg/l TCLP	
		Arsenic	7440-38-2	NA	5.0 mg/l TCLP	
		Barium	7440-39-3	NA	7.6 mg/l TCLP	
		Beryllium	7440-41-7	NA	0.014 mg/l TCLP	
		Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Mercury	7439-97-6	NA	0.025 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Selenium	7782-49-2	NA	0.16 mg/l TCLP	
		Silver	7440-22-4	NA	0.30 mg/l TCLP	
		Thallium	7440-28-0	NA	0.078 mg/l TCLP	
		Zinc	7440-66-6	NA	5.3 mg/l TCLP	
K062	Spent pickle liquor generated by steel finishing operations of facilities within the iron and steel industry (SIC Codes 331 and 332).	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K069	Emission control dust/sludge from secondary lead smelting. - Calcium Sulfate (Low Lead) Subcategory	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
	Emission control dust/sludge from secondary lead smelting. - Non-Calcium Sulfate (High Lead) Subcategory	NA	NA	NA	RLEAD	
K071	K071 (Brine purification muds from the mercury cell process in chlorine production, where separately prepurified brine is not used) nonwastewaters that are residues from RMERC.	Mercury	7439-97-6	NA	0.02 mg/l TCLP	
	K071 (Brine purification muds from the mercury cell process in chlorine production, where separately prepurified brine is not used) nonwastewaters that are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All K071 wastewaters.	Mercury	7439-97-6	0.15	NA	
K073	Chlorinated hydrocarbon waste from the purification step of the diaphragm cell process using graphite anodes in chlorine production.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachloroethane	67-72-1	0.055	30	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
K083	Distillation bottoms from aniline production.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		Cyclohexanone	108-94-1	0.36	NA	
		Diphenylamine (difficult to distinguish from diphenylnitrosamine)	122-39-4	0.92	13	
		Diphenylnitrosamine (difficult to distinguish from diphenylamine)	86-30-6	0.92	13	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
K084	Wastewater treatment sludges generated during the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
K085	Distillation or fractionation column bottoms from the production of chlorobenzenes.	Benzene	71-43-2	0.14	10	
		Chlorobenzene	108-90-7	0.057	6.0	
		m-Dichlorobenzene	541-73-1	0.036	6.0	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Total PCBs
(sum of all PCB isomers, or all Aroclors)	1336-36-3	0.10	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K086	Solvent wastes and sludges, caustic washes and sludges, or water washes and sludges from cleaning tubs and equipment used in the formulation of ink from pigments, driers, soaps, and stabilizers containing chromium and lead.	Acetone	67-64-1	0.28	160	
		Acetophenone	96-86-2	0.010	9.7	
		bis(2-Ethylhexyl) phthalate	117-81-7	0.28	28	
		n-Butyl alcohol	71-36-3	5.6	2.6	
		Butylbenzyl phthalate	85-68-7	0.017	28	
		Cyclohexanone	108-94-1	0.36	NA	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		Diethyl phthalate	84-66-2	0.20	28	
		Dimethyl phthalate	131-11-3	0.047	28	
		Di-n-butyl phthalate	84-74-2	0.057	28	
		Di-n-octyl phthalate	117-84-0	0.017	28	
		Ethyl acetate	141-78-6	0.34	33	
		Ethylbenzene	100-41-4	0.057	10	
		Methanol	67-56-1	5.6	NA	
		Methyl ethyl ketone	78-93-3	0.28	36	
		Methyl isobutyl ketone	108-10-1	0.14	33	
		Methylene chloride	75-09-2	0.089	30	
		Naphthalene	91-20-3	0.059	5.6	
		Nitrobenzene	98-95-3	0.068	14	
		Toluene	108-88-3	0.080	10	
		1,1,1-Trichloroethane	71-55-6	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations)	1330-20-7	0.32	30	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K087	Decanter tank tar sludge from coking operations.	Acenaphthylene	208-96-8	0.059	3.4	
		Benzene	71-43-2	0.14	10	
		Chrysene	218-01-9	0.059	3.4	
		Fluoranthene	206-44-0	0.068	3.4	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
		Naphthalene	91-20-3	0.059	5.6	
		Phenanthrene	85-01-8	0.059	5.6	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations).	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K088 	Spent potliners from primary aluminum reduction.	Acenaphthene	83_32_9	0.059	3.4	
		Anthracene 	120_12_7	0.059	3.4	
		Benz(a)anthracene 	56_55_3	0.059	3.4	
		Benzo(a)pyrene 	50_32_8	0.061	3.4	
		Benzo(b)fluoranthene 	205_99_2	0.11	6.8	
		Benzo(k)fluoranthene 	207_08_9	0.11	6.8	
		Benzo(g,h,i)perylene 	191_24_2	0.0055	1.8	
		Chrysene 	218_01_9	0.059	3.4	
		Dibenz(a,h)anthracene	53_70_3	0.055	8.2	
		Fluoranthene 	206_44_0	0.068	3.4	
		Indeno(1,2,3_c,d)pyrene 	193_39_5	0.0055	3.4	
		Phenanthrene 	85_01_8	0.059	5.6	
		Pyrene 	129_00_0	0.067	8.2	
		Antimony 	7440_36_0	1.9	2.1 mg/l TCLP	
		Arsenic 	7440_38_2	1.4	5.0 mg/l TCLP	
		Barium	7440_39_3	1.2	7.6 mg/l TCLP	
		Beryllium 	7440_41_7	0.82	0.014 mg/l TCLP	
		Cadmium 	7440_43_9	0.69	0.19 mg/l TCLP	
		Chromium (Total) 	7440_47_3	2.77	0.86 mg/l TCLP	
		Lead 	7439_92_1	0.69	0.37 mg/l TCLP	
		Mercury 	7439_97_6	0.15	0.025 mg/l TCLP	
		Nickel 	7440_02_0	3.98	5.0 mg/l TCLP	
		Selenium 	7782_49_2	0.82	0.16 mg/l TCLP	
		Silver 	7440_22_4	0.43	0.30 mg/l TCLP	
		Cyanide (Total) 	57_12_5	1.2	590	
		Cyanide (Amenable) 	57_12_5	0.86	30	
		Fluoride 	16984_48_8	35	48 mg/l TCLP	
K093	Distillation light ends from the production of phthalic anhydride from ortho-xylene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	85-44-9	0.055	28	
K094	Distillation bottoms from the production of phthalic anhydride from ortho-xylene.	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	100-21-0	0.055	28	
		Phthalic anhydride (measured as Phthalic acid or Terephthalic acid)	85-44-9	0.055	28	
K095	Distillation bottoms from the production of 1,1,1-trichloroethane.	Hexachloroethane	67-72-1	0.055	30	
		Pentachloroethane	76-01-7	0.055	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
K096	Heavy ends from the heavy ends column from the production of 1,1,1-trichloroethane.	m-Dichlorobenzene	541-73-1	0.036	6.0	
		Pentachloroethane	76-01-7	0.055	6.0	
		1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
		1,1,2,2-Tetrachloroethane	79-34-6	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
		1,1,2-Trichloroethane	79-00-5	0.054	6.0	
		Trichloroethylene	79-01-6	0.054	6.0	
K097	Vacuum stripper discharge from the chlordane chlorinator in the production of chlordane.	Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
		Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
		Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
K098	Untreated process wastewater from the production of toxaphene.	Toxaphene	8001-35-2	0.0095	2.6	
K099	Untreated wastewater from the production of 2,4-D.	2,4-Dichlorophenoxyacetic acid	94-75-7	0.72	10	
		HxCDDs (All Hexachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		HxCDFs (All Hexachlorodibenzofurans)	NA	0.000063	0.001	
		PeCDDs (All Pentachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		PeCDFs (All Pentachlorodibenzofurans)	NA	0.000035	0.001	
		TCDDs (All Tetrachlorodibenzo-p-dioxins)	NA	0.000063	0.001	
		TCDFs (All Tetrachlorodibenzofurans)	NA	0.000063	0.001	
K100	Waste leaching solution from acid leaching of emission control dust/sludge from secondary lead smelting.	Cadmium	7440-43-9	0.69	0.19 mg/l TCLP	
		Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
K101	Distillation tar residues from the distillation of aniline-based compounds in the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	o-Nitroaniline	88-74-4	0.27	14	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Cadmium	7440-43-9	0.69	NA	
		Lead	7439-92-1	0.69	NA	
		Mercury	7439-97-6	0.15	NA	
K102	Residue from the use of activated carbon for decolorization in the production of veterinary pharmaceuticals from arsenic or organo-arsenic compounds.	o-Nitrophenol	88-75-5	0.028	13	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Cadmium	7440-43-9	0.69	NA	
		Lead	7439-92-1	0.69	NA	
		Mercury	7439-97-6	0.15	NA	
K103	Process residues from aniline extraction from the production of aniline.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
K104	Combined wastewater streams generated from nitrobenzene/aniline production.	Aniline	62-53-3	0.81	14	
		Benzene	71-43-2	0.14	10	
		2,4-Dinitrophenol	51-28-5	0.12	160	
		Nitrobenzene	98-95-3	0.068	14	
		Phenol	108-95-2	0.039	6.2	
		Cyanides (Total)7	57-12-5	1.2	590	
K105	Separated aqueous stream from the reactor product washing step in the production of chlorobenzenes.	Benzene	71-43-2	0.14	10	
		Chlorobenzene	108-90-7	0.057	6.0	
		2-Chlorophenol	95-57-8	0.044	5.7	
		o-Dichlorobenzene	95-50-1	0.088	6.0	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Phenol	108-95-2	0.039	6.2	
		2,4,5-Trichlorophenol	95-95-4	0.18	7.4	
		2,4,6-Trichlorophenol	88-06-2	0.035	7.4	
K106	K106 (wastewater treatment sludge from the mercury cell process in chlorine production) nonwastewaters that contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	K106 (wastewater treatment sludge from the mercury cell process in chlorine production) nonwastewaters that contain less than 260 mg/kg total mercury that are residues from RMERC.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	Other K106 nonwastewaters that contain less than 260 mg/kg total mercury and are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All K106 wastewaters.	Mercury	7439-97-6	0.15	NA	
K107	Column bottoms from product separation from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	 CMBST; or CHOXD fb CARBN; or BIODG fb CARBN	 CMBST	
K108	Condensed column overheads from product separation and condensed reactor vent gases from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	 CMBST; or CHOXD fb CARBN; or BIODG fb CARBN	 CMBST	
K109	Spent filter cartridges from product purification from the production of 1,1-dimethyhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	 CMBST; or CHOXD fb CARBN; or BIODG fb CARBN	 CMBST	
K110	Condensed column overheads from intermediate separation from the production of 1,1-dimethylhydrazine (UDMH) from carboxylic acid hydrazides.	NA	NA	 CMBST; or CHOXD fb CARBN; or BIODG fb CARBN	 CMBST	
K111	Product washwaters from the production of dinitrotoluene via nitration of toluene	2,4-Dinitrotoluene	121-1-1	0.32	140	
		2,6-Dinitrotoluene	606-20-2	0.55	28	
K112	Reaction by-product water from the drying column in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	 CMBST; or CHOXD fb CARBN; or BIODG fb CARBN	 CMBST	
K113	Condensed liquid light ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	CARBN; or  CMBST	CMBST	
K114	Vicinals from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	NA	NA	CARBN; or  CMBST	CMBST	
K115	Heavy ends from the purification of toluenediamine in the production of toluenediamine via hydrogenation of dinitrotoluene.	Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		NA	NA	CARBN; or  CMBST	CMBST	
K116	Organic condensate from the solvent recovery column in the production of toluene diisocyanate via phosgenation of toluenediamine.	NA	NA	CARBN; or  CMBST	CMBST	
K117	Wastewater from the reactor vent gas scrubber in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane).	106-93-4	0.028	15	
K118	Spent absorbent solids from purification of ethylene dibromide in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K123	Process wastewater (including supernates, filtrates, and washwaters) from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	 CMBST; or CHOXD fb (BIODG or CARBN)	 CMBST	
K124	Reactor vent scrubber water from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	 CMBST; or CHOXD fb (BIODG or CARBN)	 CMBST	
K125	Filtration, evaporation, and centrifugation solids from the production of ethylenebisdithiocarbamic acid and its salts.	NA	NA	 CMBST; or CHOXD fb (BIODG or CARBN)	 CMBST	
K126	Baghouse dust and floor sweepings in milling and packaging operations from the production or formulation of ethylenebisdithiocarbamic acid and its salts.	NA	NA	 CMBST; or CHOXD fb (BIODG or CARBN)	 CMBST	
K131	Wastewater from the reactor and spent sulfuric acid from the acid dryer from the production of methyl bromide.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
K132	Spent absorbent and wastewater separator solids from the production of methyl bromide.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
K136	Still bottoms from the purification of ethylene dibromide in the production of ethylene dibromide via bromination of ethene.	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
		Chloroform	67-66-3	0.046	6.0	
		Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
K140	Waste solids and filter cartridges from the production of 2,4,6-tribromophenol.	2,4,6-Tribromophenol	118-79-6	0.035	7.4	
K141	Process residues from the recovery of coal tar, including, but not limited to, collecting sump residues from the production of coke or the recovery of coke by-products produced from coal.  This listing does not include K087 (decanter tank tar sludge from coking operations).	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-2-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene).	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene).	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K142	Tar storage tank residues from the production of coke from coal or from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K143	Process residues from the recovery of light oil, including, but not limited to, those generated in stills, decanters, and wash oil recovery units from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene)	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene)	207-08-9	0.11	6.8	
		Benzene	71-43-2	0.14	10	
		Chrysene	218-01-9	0.059	3.4	
K144	Wastewater sump residues from light oil refining, including, but not limited to, intercepting or contamination sump sludges from the recovery of coke by-products produced from coal.	Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene).	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene).	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
K145	Residues from naphthalene collection and recovery operations from the recovery of coke by-products produced from coal.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Naphthalene	91-20-3	0.059	5.6	
K147	Tar storage tank residues from coal tar refining.	Benzene	71-43-2	0.14	10	
		Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene).	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene).	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K148	Residues from coal tar distillation, including, but not limited to, still bottoms.	Benz(a)anthracene	56-55-3	0.059	3.4	
		Benzo(a)pyrene	50-32-8	0.061	3.4	
		Benzo(b)fluoranthene (difficult to distinguish from benzo(k)fluoranthene).	205-99-2	0.11	6.8	
		Benzo(k)fluoranthene (difficult to distinguish from benzo(b)fluoranthene).	207-08-9	0.11	6.8	
		Chrysene	218-01-9	0.059	3.4	
		Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
		Indeno(1,2,3-cd)pyrene	193-39-5	0.0055	3.4	
K149	Distillation bottoms from the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.  (This waste does not include still bottoms from the distillations of benzyl chloride.)	Chlorobenzene	108-90-7	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Chloromethane	74-87-3	0.19	30	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Toluene	108-88-3	0.080	10	
K150	Organic residuals, excluding spent carbon adsorbent, from the spent chlorine gas and hydrochloric acid recovery processes associated with the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.	Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Chloromethane	74-87-3	0.19	30	
		p-Dichlorobenzene	106-46-7	0.090	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		1,1,2,2- Tetrachlorotehane	79-34-5	0.057	6.0	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		1,2,4-Trichlorobenzene	120-82-1	0.055	19	
K151	Wastewater treatment sludges, excluding neutralization and biological sludges, generated during the treatment of wastewaters from the production of alpha- (or methyl-) chlorinated toluenes, ring-chlorinated toluenes, benzoyl chlorides, and compounds with mixtures of these functional groups.	Benzene	71-43-2	0.14	10	
		Carbon tetrachloride	56-23-5	0.057	6.0	
		Chloroform	67-66-3	0.046	6.0	
		Hexachlorobenzene	118-74-1	0.055	10	
		Pentachlorobenzene	608-93-5	0.055	10	
		1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
		Tetrachloroethylene	127-18-4	0.056	6.0	
		Toluene	108-88-3	0.080	10	
K156 	Organic waste (including heavy ends, still bottoms, light ends, spent solvents, filtrates, and decantates) from the production of carbamates and carbamoyl oximes.	Acetonitrile 	75_05_8	5.6	1.8	
		Acetophenone 	96_86_2	0.010	9.7	
		Aniline 	62_53_3	0.81	14	
		Benomyl 	17804_35_2	0.056	1.4	
		Benzene 	71_43_2	0.14	10	
		Carbaryl 	63_25_21	0.006	0.14	
		Carbenzadim 	10605_21_7	0.056	1.4	
		Carbofuran 	1563_66_2	0.006	0.14	
		Carbosulfan 	55285_14_8	0.028	1.4	
		Chlorobenzene 	108_90_7	0.057	6.0	
		Chloroform 	67_66_3	0.046	6.0	
		o_Dichlorobenzene	95_50_1	0.088	6.0	
		Methomyl 	16752_77_5	0.028	0.14	
		Methylene chloride 	75_09_2	0.089	30	
		Methyl ethyl ketone 	78_93_3	0.28	36	
		Naphthalene 	91_20_3	0.059	5.6	
		Phenol 	108_95_2	0.039	6.2	
		Pyridine 	110_86_1	0.014	16	
		Toluene 	108_88_3	0.080	10	
		Triethylamine 	121_44_8	0.081	1.5	
K157 	Wastewaters (including scrubber waters, condenser waters, washwaters, and separation waters) from the production of carbamates and carbamoyl oximes.	Carbon tetrachloride 	56_23_5	0.057	6.0	
		Chloroform 	67_66_3	0.046	6.0	
		Chloromethane 	74_87_3	0.19	30	
		Methomyl 	16752_77_5	0.028	0.14	
		Methylene chloride 	75_09_2	0.089	30	
		Methyl ethyl ketone 	78_93_3	0.28	36	
		o_Phenylenediamine 	95_54_5	0.056	5.6	
		Pyridine 	110_86_1	0.014	16	
		Triethylamine 	121_44_8	0.081	1.5	
K158 	Bag house dusts and  filter/separation solids from the production of carbamates and carbamoyl oximes.	Benomyl 	17804_35_2	0.056	1.4	
		Benzene 	71_43_2	0.14	10	
		Carbenzadim 	10605_21_7	0.056	1.4	
		Carbofuran 	1563_66_2	0.006	0.14	
		Carbosulfan 	55285_14_8	0.028	1.4	
		Chloroform 	67_66_3	0.046	6.0	
		Methylene chloride 	75_09_2	0.089	30	
		Phenol 	108_95_2	0.039	6.2	
K159 	Organics from the treatment of
thiocarbamate wastes.	Benzene 	71_43_2	0.14	10	
		Butylate 	2008_41_5	0.042	1.4	
		EPTC (Eptam) 	759_94_4	0.042	1.4	
		Molinate 	2212_67_1	0.042	1.4	
		Pebulate 	1114_71_2	0.042	1.4	
		Vernolate 	1929_77_7	0.042	1.4	
K160 	Solids (including filter wastes, separation solids, and spent  catalysts) from the production of thiocarbamates and solids from the  treatment of thiocarbamate wastes.	Butylate 	2008_41_5	0.042	1.4	
		EPTC (Eptam) 	759_94_4	0.042	1.4	
		Molinate 	2212_67_1	0.042	1.4	
		Pebulate 	1114_71_2	0.042	1.4	
		Toluene 	108_88_3	0.080	10	
		Vernolate 	1929_77_7	0.042	1.4	
K161 	Purification solids (including filtration, evaporation, and centrifugation solids), baghouse dust and floor sweepings, from the production of dithiocarbamate acids and their salts.	Antimony 	7440_36_0	1.9	2.1 mg/l TCLP	
		Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
		Carbon disulfide 	75_15_0	3.8	4.8 mg/l TCLP	
		Dithiocarbamates (total)	NA	0.028	28	
		Lead	7439_92_1	0.069	0.37 mg/l TCLP	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
		Selenium 	7782_49_2	0.82	0.16 mg/l TCLP	
P001	Warfarin, & salts, when present at concentrations greater than 0.3%.	Warfarin	81-81-2	(WETOX or CHOXD) fb CARBN; or  CBMST	CMBST	
P002	1-Acetyl-2-thiourea	1-Acetyl-2-thiourea	591-08-2	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P003	Acrolein	Acrolein	107-02-8	0.29	CMBST	
P004	Aldrin	Aldrin	309-00-2	0.021	0.066	
P005	Allyl alcohol	Allyl alcohol	107-18-6	(WETOX or CHOXD) fb CARBN; or  CBMST	CMBST	
P006	Aluminum phosphide	Aluminum phosphide	20859-73-8	CHOXD; CHRED; or  CMBST	CHOXD; CHRED; or CMBST	
P007	5-Aminomethyl 3-isoxazolol	5-Aminomethyl 3-isoxazolol	2763-96-4	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P008	4-Aminopyridine	4-Aminopyridine	504-24-5	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P009	Ammonium picrate	Ammonium picrate	131-74-8	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
P010	Arsenic acid	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P011	Arsenic pentoxide	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P012	Arsenic trioxide	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P013	Barium cyanide	Barium	7440-39-3	NA	7.6 mg/l TCLP	
		Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P014	Thiophenol (Benzene thiol)	Thiophenol (Benzene thiol)	108-98-5	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P015	Beryllium dust	Beryllium	7440-41-7	RMETL;or RTHRM	RMETL; or RTHRM	
P016	Dichloromethyl ether (Bis(chloromethyl)ether)	Dichloromethyl ether	542-88-1	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P017	Bromoacetone	Bromoacetone	598-31-2	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P018	Brucine	Brucine	357-57-3	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P020	2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	2-sec-Butyl-4,6-dinitrophenol (Dinoseb)	88-85-7	0.066	2.5	
P021	Calcium cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P022	Carbon disulfide	Carbon disulfide	75-15-0	3.8	 CMBST	
		Carbon disulfide; alternate6 standard for nonwastewaters only.	75-15-0	NA	4.8 mg/l TCLP	
P023	Chloroacetaldehyde	Chloroacetaldehyde	107-20-0	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P024	p-Chloroaniline	p-Chloroaniline	106-47-8	0.46	16	
P026	1-(o-Cholorphenyl)thiourea	1-(o-Cholorphenyl)thiourea	5344-82-1	(WETOX or CHOXD) fb CARBN; or  CBMST	CMBST	
P027	3-Chloropropionitrile	3-Chloropropionitrile	542-76-7	(WETOX or CHOXD) fb CARBN; or CBMST	INCIN	
P028	Benzyl chloride	Benzyl chloride	100-44-7	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P029	Copper cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P030	Cyanides (soluble salts and complexes)	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P031	Cyanogen	Cyanogen	460-19-5	CHOXD; WETOX; or CMBST	CHOXD; WETOX; or CMBST	
P033	Cyanogen chloride	Cyanogen chloride	506-77-4	CHOXD; WETOX; or CMBST	CHOXD; WETOX; or CMBST	
P034	2-Cyclohexly-4,6-dinitrophenol	2-Cyclohexly-4,6-dinitrophenol	131-89-5	(WETOX or CHOXD) fb CARBN; or  CBMST	 CMBST	
P036	Dichlorophenylarsine	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P037	Dieldrin	Dieldrin	60-57-1	0.017	0.13	
P038	Diethylarine	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
P039	Disulfoton	Disulfoton	298-04-4	0.017	6.2	
P040	0,0-Diethyl O-pyrazinyl phosphorothioate	0,0-Diethyl O-pyrazinyl phosphorothioate	297-97-2	CARBN; or  CMBST	CMBST	
P041	Diethyl-p-nitrophenyl phosphate	Diethyl-p-nitrophenyl phosphate	311-45-5	CARBN; or  CMBST	CMBST	
P042	Epinephrine	Epinephrine	51-43-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P043	Diisopropylfluorophosphate (DFP)	Diisopropylfluorophosphate (DFP)	55-91-4	CARBN; or  CMBST	CMBST	
P044	Dimethoate	Dimethoate	60-51-5	CARBN; or  CMBST	CMBST	
P045	Thiofanox	Thiofanox	39196-18-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P046	alpha, alpha-Dimethylphenethylamine	alpha, alpha-Dimethylphenethylamine	122-09-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P047	4,6-Dinitro-o-cresol	4,6-Dinitro-o-cresol	543-52-1	0.28	160	
	4,6-Dinitro-o-cresol salts	NA	NA	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P048	2,4-Dinitrophenol	2,4-Dinitrophenol	51-28-5	0.12	160	
P049	Dithiobiuret	Dithiobiuret	541-53-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P050	Endosulfan	Endosulfan I	939-98-8	0.023	0.066	
		Endosulfan II	33213-6-5	0.029	0.13	
		Endosulfan sulfate	1031-07-8	0.029	0.13	
P051	Endrin	Endrin	72-20-8	0.0028	0.13	
		Endrin aldehyde	7421-93-4	0.025	0.13	
P054	Aziridine	Aziridine	151-56-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P056	Fluorine	Fluoride (measured in wastewaters only).	16964-48-8	35	ADGAS fb NEUTR	
P057	Fluoroacetamide	Fluoroacetamide	640-19-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P058	Fluoroacetic acid, sodium salt	Fluoroacetic acid, sodium salt	62-74-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P059	Heptachlor	Heptachlor	76-44-8	0.0012	0.066	
		Heptachlor epoxide	1024-57-3	0.016	0.066	
P060	Isodrin	Isodrin	465-73-6	0.021	0.066	
P062	Hexaethyl tetraphosphate	Hexaethyl tetraphosphate	757-58-4	CARBN; or  CMBST	CMBST	
P063	Hydrogen cyanide	Cyandies (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P064	Isocyanic acid, ethyl ester	Isocyanic acid, ethyl ester	624-83-9	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P065	Mercury fulminate nonwastewaters, regardless of their total mercury content, that are not incinerator residues or are not residues from RMERC.	Mercury	7439-97-6	NA	IMERC	
	Mercury fulminate nonwastewaters that are either incinerator residues or are residues from RMERC; and contain greater than or equal to 260 mg/kg total mercury.	Mercury	7339-97-6	NA	RMERC	
	Mercury fulminate nonwastewaters that are residues from RMERC and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	Mercury fulminate nonwastewaters that are incinerator residues and contain less than 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All mercury fulminate wastewaters.	Mercury	7439-97-6	0.15	NA	
P066	Methomyl	Methomyl	16752-77-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P067	2-Methyl-aziridine	2-Methyl-aziridine	75-55-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P068	Methyl hydrazine	Methyl hydrazine	60-34-4	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED, or CMBST	
P069	2-Methyllactonitrile	2-Methyllactonitrile	75-86-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P070	Aldicarb	Aldicarb	116-06-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P071	Methyl parathion	Methyl parathion	298-00-0	0.014	4.6	
P072	1-Naphthyl-2-thiourea	1-Naphthyl-2-thiourea	86-88-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P073	Nickel carbonyl	Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
P074	Nickel-cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable7	57-12-5	0.86	30	
		Nickel	7440-02-0	3.98	5.0 mg/l TCLP	
P075	Nicotine and salts	Nicotine and salts	54-11-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P076	Nitric oxide	Nitric oxide	10102-43-9	ADGAS	ADGAS	
P077	p-Nitroaniline	p-Nitroaniline	100-01-6	0.028	28	
P078	Nitrogen dioxide	Nitrogen dioxide	10102-44-0	ADGAS	ADGAS	
P081	Nitroglycerin	Nitroglycerin	55-63-0	CHOXD; CHRED; CARBN; BIODG or CMBST	CHOXD; CHRED; or CMBST	
P082	N-Nitrosodimethylamine	N-Nitrosodimethylamine	62-75-9	0.40	2.3	
P084	N-Nitrosomethylvinylamine	N-Nitrosomethylvinylamine	4549-40-0	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P085	Octamethylpyrophosphoramide	Octamethylpyrophosphoramide	152-16-9	CARBN; or  CMBST	CMBST	
P087	Osmium tetroxide	Osmium tetroxide	20816-12-0	RMETL; or RTHRM	RMETL; or RTHRM	
P088	Endothall	Endothall	145-73-3	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
P089	Parathion	Parathion	56-38-2	0.014	4.6	
P092	Phenyl mercuric acetate nonwastewaters, regardless of their total mercury content, that are not incinerator residues or are not residues from RMERC.	Mercury	7439-97-6	NA	IMERC; or RMERC	
	Phenyl mercuric acetate nonwastewaters that are either incinerator residues or are residues from RMERC; and still contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	Phenyl mercuric acetate nonwastewaters that are residues from RMERC and contain less than 160 mg/kg total mercury.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	Phenyl mercuric acetate nonwastewaters that are incinerator residues and contain less then 260 mg/kg total mercury.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All phenyl mercuric acetate wastewaters.	Mercury	7439-97-6	0.15	NA	
P093	Phenylthiourea	Phenylthiourea	103-85-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P094	Phorate	Phorate	298-02-2	0.021	4.6	
P095	Phosgene	Phosgene	75-44-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P096	Phosphine	Phosphine	7803-51-2	CHOXD; CHRED; or CMBST	CHOXD; CHRED; or CMBST	
P097	Famphur	Famphur	52-85-7	0.017	15	
P098	Potassium cyanide.	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	.086	30	
P099		Cyanides (Amenable)7	57-12-5	0.86	30	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
P0101	Ethyl cyanide (Propanenitrile)	Ethyl cyanide (Propanenitrile)	107-12-0	0.24	360	
P0102	Propargyl alcohol	Propargyl alcohol	107-19-7	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
P0103	Selenourea	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
P0104	Silver cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
		Silver	7440-22-4	0.43	0.30 mg/l TCLP	
P0105	Sodium azide	Sodium azide	26628-22-8	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
P0106	Sodium cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P0108	Strychnine and salts	Strychnine and salts	57-24-9	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P109	Tetraethyldithiopyrophosphate	Tetraethyldithiopyrophosphate	3689-24-5	CARBN; or  CMBST	CMBST	
P110	Tetraethyl lead	lead	7439-92-1	0.69	0.37 mg/l TCLP	
P111	Tetraethylpyrophosphate	Tetraethylpyrophosphate	107-49-3	CARBN; or  CMBST	CMBST	
P112	Tetranitromethane	Tetranitromethane	509-14-8	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
P113	Thallic oxide	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
P114	Thallium selenite	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
P115	Thallium (I) sulfate	Thallium (measured in wastewaters only)	7440-28-0	1.4	RTHRM; or STABL	
P116	Thiosemicarbazide	Thiosemicarbazide	79-19-6	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P118	Trichloromethanethiol	Trichloromethanethiol	75-70-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
P119	Ammonium vanadate	Vanadium (measured in wastewaters only).	7440-62-2	4.3	STABL	
P120	Vanadium pentoxide	Vanadium (measured in wastewaters only).	7440-62-2	4.3	STABL	
P121	Zinc cyanide	Cyanides (Total)7	57-12-5	1.2	590	
		Cyanides (Amenable)7	57-12-5	0.86	30	
P122	Zinc phosphide Zn3P2, when present at concentrations greater than 10%	Zinc Phosphide	1314-84-7	CHOXD; CHRED; or CMBST	CHOXD; CHRED; or CMBST	
P123	Toxaphene	Toxaphene	8001-35-2	0.0095	2.6	
P127	Carbofuran 	Carbofuran 	1563_66_2	0.006	0.14	
P128	Mexacarbate 	Mexacarbate 	315_18_4	0.056	1.4	
P185 	Tirpate 	Tirpate 	26419_73_8	0.056	0.28	
P187 	Bendiocarb 	Bendiocarb 	22781_23_3	0.056	1.4	
P188 	Physostigimine salicylate 	Physostigmine salicylate 	57_64_7	0.056	1.4	
P189 	Carbosulfan 	Carbosulfan 	55285_14_8	0.028	1.4	
P190 	Metolcarb 	Metolcarb 	1129_41_5	0.056	1.4	
P191 	Dimetilan 	Dimetilan 	644_64_4	0.056	1.4	
P192 	Isolan 	Isolan 	119_38_0	0.056	1.4	
P193 	Thiophanate_methyl 	Thiophanate_methyl 	23564_05_8	0.056	1.4	
P194 	Oxamyl 	Oxamyl 	23135_22_0	0.056	0.28	
P195 	Thiodicarb 	Thiodicarb 	59669_26_0	0.019	1.4	
P196 	Manganese dimethyldithiocarbamate	Dithiocarbamates (total) 	NA	0.028	28	
P197 	Formparanate 	Formparanate 	17702_57_7	0.056	1.4	
P198 	Formetanate hydrochloride 	Formetanate hydrochloride 	23422_53_9	0.056	1.4	
P199 	Methiocarb 	Methiocarb 	2032_65_7	0.056	1.4	
P200 	Propoxur 	Propoxur 	114_26_1	0.056	1.4	
P201 	Promecarb 	Promecarb 	2631_37_0	0.056	1.4	
P202 	M-Cumenyl methylcarbamate	m-Cumenyl methylcarbamate	64_00_6	0.056	1.4	
P203 	Aldicarb sulfone 	Aldicarb sulfone 	1646_88_4	0.056	0.28	
P204 	Physostigmine 	Physostigmine 	57_47_6	0.056	1.4	
P205 	Ziram	Dithiocarbamates (total) 	NA	0.028	28	
U001	Acetaldehyde	Acetaldehyde	75-07-0	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U002	Acetone	Acetone	67-64-1	0.28	160	
U003	Acetonitrile	Acetonitrile	75-05-8	5.6	 CMBST	
		Acetonitrile; alternate6 standard for nonwastewaters only	75-05-8	NA	1.8	
U004	Acetophenone	Acetophenone	98-86-2	0.010	9.7	
U005	2-Acetylaminofluorene	2-Acetylaminofluorene	53-96-3	0.059	140	
U006	Acetyl chloride	Acetyl Chloride	75-36-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U007	Acrylamide	Acrylamide	79-06-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U008	Acrylic acid	Acrylic acid	79-10-7	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U009	Acrylonitrile	Acrylonitrile	107-13-1	0.24	84	
U010	Mitomycin C	Mitomycin C	50-07-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U011	Amitrole	Amitrole	61-82-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U012	Aniline	Aniline	62-53-3	0.81	14	
U014	Auramine	Auramine	492-80-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U015	Azaserine	Azaserine	115-02-6	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U016	Benz(c)acridine	Benz(c)acridine	225-51-4	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U017	Benzal chloride	Benzal chloride	98-87-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U018	Benz(a)anthracene	Benz(a)anthracene	56-55-3	0.059	3.4	
U019	Benzene	Benzene	71-43-2	0.14	10	
U020	Benzenesulfonyl chloride	Benzenesulfonyl chloride	98-09-9	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U021	Benzidine	Benzidine	92-87-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U022	Benzo(a)pyrene	Benzo(a)pyrene	50-32-8	0.061	3.4	
U023	Benzotrichloride	Benzotrichloride	98-07-7	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
U024	bis(2-Chloroethoxy)methane	bis(2-Chloroethoxy)methane	111-91-1	0.036	7.2	
U025	bis(2-Chloroethyl)ether	bis(2-Chloroethyl)ether	111-44-4	0.033	6.0	
U026	Chlornaphazine	Chlornaphazine	494-03-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U027	bis(2-Chloroisopropyl)ether	bis(2-Chloroisopropyl)ether	39638-32-9	(WETOX or CHOXD) fb CARBN; or  CMBST	7.2	
U028	bis(2-Ethylhexyl)phthalate	bis(2-Ethylhexyl)phthalate	117-81-7	0.28	28	
U029	Methyl bromide (Bromomethane)	Methyl bromide (Bromomethane)	74-83-9	0.11	15	
U030	4-Bromophenyl phenyl ether	4-Bromophenyl phenyl ether	101-55-3	0.055	15	
U031	n-Butyl alcohol	n-Butyl alcohol	71-36-3	5.6	2.6	
U032	Calcium chromate	Chromium (Total)	7440-47-3	2.77	0.86 mg/l TCLP	
U033	Carbon oxyfluoride	Carbon oxyfluoride	353-50-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U034	Trichloroacetaldehyde (Chloral)	Trichloroacetaldehyde (Chloral)	75-87-6	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U035	Chlorambucil	Chlorambucil	305-03-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U036	Chlordane	Chlordane (alpha and gamma isomers)	57-74-9	0.0033	0.26	
U037	Chlorobenzene	Chlorobenzene	108-90-7	0.057	6.0	
U038	Chlorobenzilate	Chlorobenzilate	510-15-6	0.10	 CMBEST	
U039	p-Chloro-m-cresol	p-Chloro-m-cresol	59-50-7	0.018	14	
U041	Epichlorohydrin (1-Chloro-2,3-epoxypropane)	Epichlorohydrin (1-Chloro-2,3-epoxypropane)	106-89-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U042	2-Chloroethyl vinyl ether	2-Chloroethyl vinyl ether	110-75-8	0.062	 CMBST	
U043	Vinyl chloride	Vinyl chloride	75-01-4	0.27	6.0	
U044	Chloroform	Chloroform	67-66-3	0.046	6.0	
U045	Chloromethane (Methyl chloride)	Chloromethane (Methyl chloride)	74-87-3	0.19	30	
U046	Chloromethyl methyl ether	Chloromethyl methyl ether	107-30-2	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U047	2-Chloronaphthalene	2-Chloronaphthalene	91-58-7	0.055	5.6	
U048	2-Chlorophenol	2-Chlorophenol	95-57-8	0.044	5.7	
U049	4-Chloro-o-toluidine hydrochloride	4-Chloro-o-toluidine hydrochloride	3165-93-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U050	Chrysene	Chrysene	218-01-9	0.059	3.4	
U051	Creosote	Naphthalene	91-20-3	0.059	5.6	
		Pentachlorophenol	87-86-5	0.089	7.4	
		Phenanthrene	85-01-8	0.059	5.6	
		Pyrene	129-00-0	0.067	8.2	
		Toluene	108-88-3	0.080	10	
		Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations).	1330-20-7	0.32	30	
		Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U052	Cresols (Cresylic acid)	o-Cresol	95-48-7	0.11	5.6	
		m-Cresol (difficult to distinguish from p-cresol).	108-39-4	0.77	5.6	
		p-Cresol (difficult to distinguish from m-cresol).	106-44-5	0.77	5.6	
		Cresol-mixed isomers (Cresylic acid)
(sum of o-, m-, and p-cresol concentrations).	1319-77-3	0.88	11.2	
U053	Crotonaldehyde	Crotonaldehyde	4170-30-3	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U055	Cumene	Cumene	98-82-8	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U056	Cyclohexane	Cyclohexane	110-82-7	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U057	Cyclohexanone	Cyclohexanone	108-94-1	0.36	CMBST	
		Cyclohexanone; alternate6 standard for nonwastewaters only	108-94-1	NA	0.75 mg/l TCLP	
U058	Cyclophosphamide	Cyclophosphamide	50-18-0	CARBN; or  CMBST	CMBST	
U059	Daunomycin	Daunomycin	20830-81-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U060	DDD	o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
U061	DDT	o,p'-DDT	789-02-6	0.0039	0.087	
		p,p'-DDT	50-29-3	0.0039	0.087	
		o,p'-DDD	53-19-0	0.023	0.087	
		p,p'-DDD	72-54-8	0.023	0.087	
		o,p'-DDE	3424-82-6	0.031	0.087	
		p,p'-DDE	72-55-9	0.031	0.087	
U062	Diallate	Diallate	2303-16-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U063	Dibenz(a,h)anthracene	Dibenz(a,h)anthracene	53-70-3	0.055	8.2	
U064	Dibenz(a,i)pyrene	Dibenz(a,i)pyrene	189-55-9	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U066	1,2-Dibromo-3-chloropropane	1,2-Dibromo-3-chloropropane	96-12-8	0.11	15	
U067	Ethylene dibromide (1,2-Dibromoethane)	Ethylene dibromide (1,2-Dibromoethane)	106-93-4	0.028	15	
U068	Dibromomethane	Dibromomethane	74-95-3	0.11	15	
U069	Di-n-butyl phthalate	Di-n-butyl phthalate	84-74-2	0.057	28	
U070	o-Dichlorobenzene	o-Dichlorobenzene	95-50-1	0.088	6.0	
U071	m-Dichlorobenzene	m-Dichlorobenzene	541-73-1	0.036	6.0	
U072	p-Dichlorobenzene	p-Dichlorobenzene	106-46-7	0.090	6.0	
U073	3,3'-Dichlorobenzidine	3,3'-Dichlorobenzidine	91-94-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U074	1,4-Dichloro-2-butene	cis-1,4-Dichloro-2-butene	1476-11-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
		trans-1,4-Dichloro-2-butene	764-41-0	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U075	Dichlorodifluoromethane	Dichlorodifluoromethane	75-71-8	0.23	7.2	
U076	1,1-Dichloroethane	1,1-Dichloroethane	75-34-3	0.059	6.0	
U077	1,2-Dichloroethane	1,2-Dichloroethane	107-06-2	0.21	6.0	
U078	1,1-Dichloroethylene	1,1-Dichloroethylene	75-35-4	0.025	6.0	
U079	1,2-Dichloroethylene	trans-1,2-Dichloroethylene	156-60-5	0.054	30	
U080	Methylene chloride	Methylene chloride	75-09-2	0.089	30	
U081	2,4-Dichlorophenol	2,4-Dichlorophenol	120-83-2	0.044	14	
U082	2,6-Dichlorophenol	2,6-Dichlorophenol	87-65-0	0.044	14	
U083	1,2-Dichloropropane	1,2-Dichloropropane	78-87-5	0.85	18	
U084	1,3-Dichloroproplyene	cis-1,3-Dichloroproplyene	10061-01-5	0.036	18	
		trans-1,3-Dichloroproplyene	10061-02-6	0.036	18	
U085	1,2:3,4-Diepoxybutane	1,2:3,4-Diepoxybutane	1464-53-5	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U086	N,N'-Diethylhydrazine	N,N'-Diethylhydrazine	1615-80-1	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
U087	O,O-Diethyl S-methyldithiophosphate	O,O-Diethyl S-methyldithiophosphate	3288-58-2	CARBN; CMBST	CMBST	
U088	Diethyl phthalate	Diethyl phthalate	84-66-2	0.20	28	
U089	Diethyl stilbestrol	Diethyl stilbestrol	56-53-1	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U090	Dihydrosafrole	Dihydrosafrole	94-58-6	(WETOX or CHOXD) fb CARBN; or CMBST	CMBST	
U091	3,3'-Dimethoxybenzidine	3,3'-Dimethoxybenzidine	119-90-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U092	Dimethylamine	Dimethylamine	124-40-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U093	p-Dimethylaminoazobenzene	p-Dimethylaminoazobenzene	60-11-7	0.13	CMBST	
U094	7,12-Dimethylibenz(a)anthracene	7,12-Dimethylbenz(a)anthracene	57-97-6	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U095	3,3'-Dimethylbenzidine	3,3'-Dimethylbenzidine	119-93-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U096	alpha, alpha-Dimethyl benzyl hydroperoxide	alpha, alpha-Dimethyl benzyl hydroperoxide	80-15-9	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
U097	Dimethylcarbamoyl chloride	Dimethylcarbamoyl chloride	79-44-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U098	1,1-Dimethylhydrazine	1,1-Dimethylhydrazine	57-14-7	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
U099	1,2-Dimethylhydrazine	1,2-Dimethylhydrazine	540-73-8	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST 
CHOXD; CHRED; or CMBST	
U101	2,4-Dimethylphenol	2,4-Dimethylphenol	105-67-9	0.036	14	
U102	Dimethyl phthalate	Dimethyl phthalate	131-11-3	0.047	28	
U103	Dimethyl sulfate	Dimethyl sulfate	77-78-1	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
U105	2,4-Dinitrotoluene	2,4-Dinitrotoluene	121-14-2	0.32	140	
U106	2,6-Dinitrotoluene	2,6-Dinitrotoluene	606-20-2	0.55	28	
U107	Di-n-octyl phthalate	Di-n-octyl phthalate	117-84-0	0.017	28	
U108	1,4-Dioxane	1,4-Dioxane	123-91-1	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
		1,4-Dioxane; alternate6 standard for nonwastewaters only.	123-91-1	NA	170	
U109	1,2-Diphenylhydrazine	1,2-Diphenylhydrazine	122-66-7	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
		1,2-Diphenylhydrazine; alternate6 standard for wastewaters only.	122-66-7	0.087	NA	
U110	Dipropylamine	Dipropylamine	142-84-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U111	Di-n-propylnitrosamine	Di-n-propylnitrosamine	621-64-7	0.40	14	
U112	Ethyl acetate	Ethyl acetate	141-78-6	0.34	33	
U113	Ethyl acrylate	Ethyl acrylate	140-88-5	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U114	Ethylenebisdithiocarbamic acid salts and esters	Ethylenebisdithiocarbamic acid	111-54-6	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U115	Ethylene oxide	Ethylene oxide 	75-21-8	(WETOX or CHOXD) fb CARBN; or  CMBST	CHOXD; or  CMBST	
		Ethylene oxide; alternate 6 standard for wastewaters only	75-21-8	0.12	NA	
U116	Ethylene thiourea	Ethylene thiourea	96-45-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U117	Ethyl ether	Ethyl ether	60-29-7	0.12	160	
U118	Ethyl methacrylate	Ethyl methacrylate	97-63-2	0.14	160	
U119	Ethyl methane sulfonate	Ethyl methane sulfonate	62-50-0	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U120	Fluoranthene	Fluoranthene	206-44-0	0.068	3.4	
U121	Trichloromonofluoromethane	Trichloromonofluoromethane	75-69-4	0.020	30	
U122	Formaldehyde	Formaldehyde	50-00-0	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U123	Formic acid	Formic acid	64-18-6	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U124	Furan	Furan	110-00-9	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U125	Furfural	Furfural	98-01-1	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U126	Glycidylaldehyde	Glycidylaldehyde	765-34-4	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U127	Hexachlorobenzene	Hexachlorobenzene	118-74-1	0.055	10	
U128	Hexachlorobutadiene	Hexachlorobutadiene	87-68-3	0.055	5.6	
U129	Lindane	alpha-BHC	319-84-6	0.00014	0.066	
		beta-BHC	319-85-7	0.00014	0.066	
		delta-BHC	319-86-8	0.023	0.066	
		gamma-BHC (Lindane)	58-89-9	0.0017	0.066	
U130	Hexachlorocyclopentadiene	Hexachlorocyclopentadiene	77-47-4	0.057	2.4	
U131	Hexachloroethane	Hexachloroethane	67-72-1	0.055	30	
U132	Hexachlorophene	Hexachlorophene	70-30-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U133	Hydrazine	Hydrazine	302-01-2	CHOXD; CHRED; CARBN; DIODG; or CMBST	CHOXD; CHRED; or CMBST	
U134	Hydrogen fluoride	Fluoride (measured in wastewaters only)	16964-48-8	35	ADGAS fb NEUTR; or NEUTR	
U135	Hydrogen Sulfide	Hydrogen Sulfide	7783-06-4	CHOXD; CHRED; or CMBST	CHOXD; CHRED; or CMBST	
U136	Cacodylic acid	Arsenic	7440-38-2	1.4	5.0 mg/l TCLP	
U137	Indeno(1,2,3-cd)pyrene	Indeno(1,2,3-c, d)pyrene	193-39-5	0.0055	3.4	
U138	Iodomethane	Iodomethane	74-88-4	0.19	65	
U140	Isobutyl alcohol	Isobutyl alcohol	78-83-1	5.6	170	
U141	Isosafrole	Isosafrole	120-58-1	0.081	2.6	
U142	Kepone	Kepone	143-50-8	0.0011	0.13	
U143	Lasiocarpine	Lasiocarpine	303-34-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U144	Lead acetate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U145	Lead phosphate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U146	Lead subacetate	Lead	7439-92-1	0.69	0.37 mg/l TCLP	
U147	Maleic anhydride	Maleic anhydride	108-31-6	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U148	Maleic hydrazide	Maleic hydrazide	123-33-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U149	Malononitrile	Malononitrile	109-77-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U150	Melphalan	Melphalan	148-82-3	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U151	U151 (mercury) nonwastewaters that contain greater than or equal to 260 mg/kg total mercury.	Mercury	7439-97-6	NA	RMERC	
	U151 (mercury) nonwastewaters that contain less than 260 mg/kg total mercury and that are residues from RMERC only.	Mercury	7439-97-6	NA	0.20 mg/l TCLP	
	U151 (mercury) nonwastewaters that contain less than 260 mg/kg total mercury and that are not residues from RMERC.	Mercury	7439-97-6	NA	0.025 mg/l TCLP	
	All U151 (mercury) wastewaters.	Mercury	7439-97-6	0.15	NA	
	Elemental Mercury Contaminated with Radioactive materials.	Mercury	7439-97-6	NA	AMLGM	
U152	Methacrylonitrile	Methacrylonitrile	126-98-7	0.24	84	
U153	Methanethiol	Methanethiol	74-93-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U154	Methanol	Methanol	67-56-1	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
		Methanol, alternate6 set of standards for both wastewaters and nonwastewaters	67-56-1	5.6	0.75 mg/l TCLP	
U155	Methapyrilene	Methapyrilene	91-80-5	0.081	1.5	
U156	Methyl chlorocarbonate	Methyl chlorocarbonate	79-22-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U157	3-Methylcholanthrene	3-Methylcholanthrene	56-49-5	0.0055	15	
U158	4,4'-Methylene bis(2-chloroaniline)	4,4'-Methylene bis(2-chloroaniline)	101-14-4	0.50	30	
U159	Methyl ethyl ketone	Methyl ethyl ketone	78-93-3	0.28	36	
U160	Methyl ethyl ketone peroxide	Methyl ethyl ketone peroxide	1338-23-4	CHOXD; CHRED; CARBN; BIODG; or CMBST	CHOXD; CHRED; or CMBST	
U161	Methyl isobutyl ketone	Methyl isobutyl ketone	108-10-1	0.14	33	
U162	Methyl methacrylate	Methyl methacrylate	80-62-6	0.14	160	
U163	N-Methyl N'-nitro N-nitrosoguanidine	N-Methyl N'-nitro N-nitrosoguanidine	70-25-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U164	Methylthiouracil	Methylthiouracil	56-04-2	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U165	Naphthalene	Naphthalene	91-20-3	0.059	5.6	
U166	1,4-Naphthoquinone	1,4-Naphthoquinone	130-15-4	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U167	1-Naphthlyamine	1-Naphthlyamine	134-32-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U168	2-Naphthlyamine	2-Naphthlyamine	91-59-8	0.52	 CMBST	
U169	Nitrobenzene	Nitrobenzene	98-95-3	0.068	14	
U170	p-Nitrophenol	p-Nitrophenol	100-02-7	0.12	29	
U171	2-Nitropropane	2-Nitropropane	79-46-9	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U172	N-Nitrosodi-n-butylamine	N-Nitrosodi-n-butylamine	924-16-3	0.40	17	
U173	N-Nitrosodiethanolamine	N-Nitrosodiethanolamine	1116-54-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U174	N-Nitrosodiethylamine	N-Nitrosodiethylamine	55-18-5	0.40	28	
U176	N-Nitroso-N-ethylurea	N-Nitroso-N-ethylurea	759-73-9	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U177	N-Nitroso-N-methylurea	N-Nitroso-N-methylurea	684-93-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U178	N-Nitroso-N-methylurethane	N-Nitroso-N-methylurethane	615-53-2	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U179	N-Nitrosopiperidine	N-Nitrosopiperidine	100-75-4	0.013	35	
U180	N-Nitrosopyrrolidine	N-Nitrosopyrrolidine	930-55-2	0.013	35	
U181	5-Nitro-o-toluidine	5-Nitro-o-toluidine	99-55-8	0.32	28	
U182	Paraldehyde	Paraldehyde	123-63-7	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U183	Pentachlorobenzene	Pentachlorobenzene	608-93-5	0.055	10	
U184	Pentachloroethane	Pentachloroethane	76-01-7	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
		Pentachloroethane; alternate6 standards for both wastewaters and nonwastewaters.	76-01-7	0.055	6.0	
U185	Pentachloronitrobenzene	Pentachloronitrobenzene	82-68-8	0.055	4.8	
U186	1,3-Pentadiene	1,3-Pentadiene	504-60-9	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U187	Phenacetin	Phenacetin	62-44-2	0.081	16	
U188	Phenol	Phenol	108-95-2	0.039	6.2	
U189	Phosphorus sulfide	Phosphorus sulfide	1314-80-3	CHOXD; CHRED; or CMBST	CHOXD; CHRED; or CMBST	
U190	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	Phthalic anhydride (measured as Phthalic acid or Terephthalic acid).	100-21-0	0.055	28	
		Phthalic anhydride	85-44-9	0.055	28	
U191	2-Picoline	2-Picoline	109-06-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U192	Pronamide	Pronamide	23950-58-5	0.093	1.5	
U193	1,3-Propane sultone	1,3-Propane sultone	1120-71-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U194	n-Propylamine	n-Propylamine	107-10-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U196	Pyridine	Pyridine	110-86-1	0.014	16	
U197	p-Benzoquinone	p-Benzoquinone	106-51-4	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U200	Reserpine	Reserpine	50-55-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U201	Resorcinol	Resorcinol	108-46-3	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U202	Saccharin and salts	Saccharin	81-07-2	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U203	Safrole	Safrole	94-59-7	0.081	22	
U204	Selenium dioxide	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
U205	Selenium sulfide	Selenium	7782-49-2	0.82	0.16 mg/l TCLP	
U206	Streptozotocin	Streptozotocin	18883-66-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U207	1,2,4,5-Tetrachlorobenzene	1,2,4,5-Tetrachlorobenzene	95-94-3	0.055	14	
U208	1,1,1,2-Tetrachloroethane	1,1,1,2-Tetrachloroethane	630-20-6	0.057	6.0	
U209	1,1,2,2-Tetrachloroethane	1,1,2,2-Tetrachloroethane	79-34-5	0.057	6.0	
U210	Tetrachloroethylene	Tetrachloroethylene	127-18-4	0.056	6.0	
U211	Carbon tetrachloride	Carbon tetrachloride	56-23-5	0.057	6.0	
U213	Tetrahydrofuran	Tetrahydrofuran	109-99-9	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U214	Thallium (I) acetate	Thallium (measured in wastewaters only).	7440-28-0	1.4	RTHRM; or STABL	
U215	Thallium (I) carbonate	Thallium (measured in wastewaters only).	7440-28-0	1.4	RTHRM; or STABL	
U216	Thallium (I) chloride	Thallium (measured in wastewaters only).	7440-28-0	1.4	RTHRM; or STABL	
U217	Thallium (I) nitrate	Thallium (measured in wastewaters only).	7440-28-0	1.4	RTHRM; or STABL	
U218	Thioacetamide	Thioacetamide	62-55-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U219	Thiourea	Thiourea	62-56-6	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U220	Toluene	Toluene	108-88-3	0.080	10	
U221	Toluenediamine	Toluenediamine	25376-45-8	CARBN; or  CMBST	CMBST	
U222	o-Toluidine hydrochloride	o-Toluidine hydrochloride	636-21-5	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U223	Toluene diisocyanate	Toluene diisocyanate	26471-62-5	CARBN; or  CMBST	CMBST	
U225	Bromoform (Tribromomethane)	Bromoform (Tribromomethane)	75-25-2	0.63	15	
U226	1,1,1-Trichloroethane	1,1,1-Trichloroethane	71-55-6	0.054	6.0	
U227	1,1,2-Trichloroethane	1,1,2-Trichloroethane	79-00-5	0.054	6.0	
U228	Trichloroethylene	Trichloroethylene	79-01-6	0.054	6.0	
U234	1,3,5-Trinitrobenzene	1,3,5-Trinitrobenzene	99-35-4	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U235	tris-(2,3-Dibromopropyl)-phosphate	tris-(2,3-Dibromopropyl)-phosphate	126-72-7	0.11	0.10	
U236	Trypan Blue	Trypan Blue	72-57-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U237	Uracil mustard	Uracil mustard	66-75-1	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U238	Urethane (Ethyl carbamate)	Urethane (Ethyl carbamate)	51-79-6	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U239	Xylenes	Xylenes-mixed isomers
(sum of o-, m-, and p-xylene concentrations).	1330-20-7	0.32	30	
U240	2,4-D (2,4-Dichlorophenoxyacetic acid)	2,4-D (2,4-Dichlorophenoxyacetic acid).	94-75-7	0.72	10	
	2,4-D (2,4-Dichlorophenoxyacetic acid) salts and esters		NA	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U243	Hexachloropropylene	Hexachloropropylene	1888-71-7	0.035	30	
U244	Thiram	Thiram	137-26-8	(WETOX or CHOXD) fb CARBN; or  CMBST	 CMBST	
U246	Cyanogen bromide	Cyanogen bromide	506-68-3	CHOXD; WETOX; or CMBST	CHOXD; WETOX; or CMBST	
U247	Methoxychlor	Methoxychlor	72-43-5	0.25	0.18	
U248	Warfarin, & salts, when present at concentrations of 0.3% or less.	Warfarin	81-81-2	(WETOX or CHOXD) fb CARBN; or  CMBST	CMBST	
U249	Zinc phosphide, Zn3P2, when present at concentrations of 10% or less.	Zinc Phosphide	1314-84-7	CHOXD; CHRED; or CMBST	CHOXD; CHRED; or CMBST	
U271	Benomyl	Benomyl	17804-35-2	0.056	1.4	
U277	Sulfallate	Dithiocarbamates (total).	NA	0.028	28	
U278	Bendiocarb	Bendiocarb	22781-23-3	0.056	1.4	
U279	Carbaryl	Carbaryl	63-25-2	0.006	0.14	
U280	Barban	Barban	101-27-9	0.056	1.4	
U328	o-Toluidine	o-Toluidine	95-53-4	 CMBST; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN.	CMBST	
U353	p-Toluidine	p-Toluidine	106-49-0	 CMBST; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN.	 CMBST	
U359	2-Ethoxyethanol	2-Ethoxyethanol	110-80-5	 CMBST; or CHOXD fb (BIODG or CARBN); or BIODG fb CARBN	CMBST	
U360	Carbamates, N.O.S.	Carbamates, N.O.S.	 NA	 0.056	 1.4	
U361	Carbamoyl Oximes, N.O.S.	Carbamoyl Oximes, N.O.S.	 NA	 0.056	0.28	
U362	Thiocarbamates, N.O.S.	Thiocarbamates, N.O.S.	 NA	 0.003	 1.4	
U363	Dithiocarbamates (total)	Dithiocarbamates (total)	 NA	 0.028	28	
	Antimony	Antimony	7440_36_0	 1.9	2.1 mg/l TCLP	
	Lead	Lead	7439_92_1	0.69	 0.37 mg/l TCLP	
	Nickel	Nickel	7440_02_0	3.98	5.0 mg/l TCLP	
	Selenium	Selenium	7782_49_2	0.82	 0.16 mg/l TCLP	
U364	Bendiocarb phenol	Bendiocarb phenol	 22961_82_6	 0.056	 1.4	
U365	Molinate	Molinate	2212_67_1	 0.042	1.4	
U366	Dazomet	Dithiocarbamates (total)	NA	0.028	28	
U367	Carbofuran phenol	Carbofuran phenol	1563_38_8	 0.056	 1.4	
U368	Dithiocarbamates (total)	Dithiocarbamates (total)	 NA	 0.028	28	
	Antimony	Antimony	7440_36_0	 1.9	2.1 mg/l TCLP	
U369	Dithiocarbamates (total)	Dithiocarbamates (total)	 NA	 0.028	28	
	Antimony	Antimony	7440_36_0	 1.9	2.1 mg/l TCLP	
U370	Dithiocarbamates (total)	Dithiocarbamates (total)	 NA	 0.028	28	
U371	Hexazinone intermediate	Hexazinone intermediate	 65086_85_3	 0.056	 1.4	
U372	Carbendazim	Carbendazim	 10605_21_7	 0.056	 1.4	
U373	Propham	Propham	 122_42_9	 0.056	 1.4	
U374	U9069	U9069	112006_94_7	 0.056	 1.4	
U375	3_Iodo_2_propynyl n_butylcarbamate	3_Iodo_2_propynyl n_butylcarbamate	55406_53_6	0.056	1.4	
U376	Selenium, tetrakis (dimethyldithio_carbamate)	Dithiocarbamates (total)	NA	0.028	28	
	Selenium	Selenium	7782_49_2	 0.82	0.16 mg/l TCLP	
U377	Pottasium n_methyldithiocarbamate	Dithiocarbamates (total)	NA	0.028	28	
U378	Potassium n_hydroxymethyl_n_methyldithiocarbamate	Dithiocarbamates (total)	NA	0.028	28	
U379	Sodium dibutyldithiocarbamate	Dithiocarbamates (total)	NA	0.028	28	
U381	Sodium diethyldithiocarbamate	Dithiocarbamates (total)	NA	0.028	28	
U382	Sodium dimethyldithiocarbamate	Dithiocarbamates (total)	NA	0.028	28	
U383	Potassium dimethyl dithiocarbamate	Dithiocarbamates (total)	NA	0.028	28	
U384	Metam Sodium	Dithiocarbamates (total)	NA	0.028	28	
U385	Vernolate	Vernolate	1929_77_7	 0.042	1.4	
U386	Cycloate	Cycloate	1134_23_2	 0.042	1.4	
U387	Prosulfocarb	Prosulfocarb	52888_80_9	0.042	1.4	
U389	Triallate	Triallate	2303_17_5	 0.042	1.4	
U390	EPTC	EPTC	759_94_4	0.042	1.4	
U391	Pebulate	Pebulate	1114_71_2	 0.042	1.4	
U392	Butylate	Butylate	2008_41_5	 0.042	1.4	
U393	Copper dimethyldithiocarbamate	Dithiocarbamates (total)	NA	0.028	28	
U394	A2213	A2213	30558_43_1	0.042	1.4	
U395	Diethylene glycol, dicarbamate	Diethylene glycol, dicarbamate	 5952_26_1	 0.056	1.4	
U396	Ferbam	Dithiocarbamates (total)	NA	0.028	28	
U400	Bis (pentamethylene) thiuram tetrasulfide	Dithiocarbamates (total)	NA	0.028	28	
U401	Tetramethyl thiuram monosulfide	Dithiocarbamates (total)	NA	0.028	28	
U402	Tetrabutylthiuram disulfide	 Dithiocarbamates (total)	NA	0.028	28	
U403	Disulfiram	Dithiocarbamates (total)	NA	0.028	28	
U404	Triethylamine	Triethylamine	101_44_8	0.081	1.5	
U407	Ethyl Ziram	Dithiocarbamates (total)	NA	0.028	28	
U409	Thiophanate_methyl	Thiophanate_methyl	23564_05_8	0.056	1.4	
U410	Thiodicarb	Thiodicarb	59669_26_0	0.019	1.4	
U411	Propoxur	Propoxur	114_26_1	0.056	1.4	
Notes to Table:
1	The waste descriptions provided in this table do not replace waste descriptions in 40 CFR part 261.  Descriptions of Treatment/Regulatory Subcategories are provided, as needed, to distinguish between applicability of different standards.
2	CAS means Chemical Abstract Services.  When the waste code and/or regulated constituents are described as a combination of a chemical with it's salts and/or esters, the CAS number is given for the parent compound only.
3	Concentration standards for wastewaters are expressed in mg/l and are based on analysis of composite samples.
4	All treatment standards expressed as a Technology Code or combination of Technology Codes are explained in detail in 40 CFR 268.42 Table 1 - Technology Codes and Descriptions of Technology-Based Standards.
5	Except for Metals (EP or TCLP) and Cyanides (Total and Amenable) the nonwastewater treatment standards expressed as a concentration were established, in part, based upon incineration in units operated in accordance with the technical requirements of 40 CFR part 264, Subpart O, or part 265, subpart O, or based upon combustion in fuel substitution units operating in accordance with applicable technical requirements.  A facility may comply with these treatment standards according to provisions in 40 CFR 268.40(d).  All concentration standards for nonwastewaters are based on analysis of grab samples.
6	Where an alternate treatment standard or set of alternate standards has been indicated, a facility may comply with this alternate standard, but only for the Treatment/Regulatory Subcategory or physical form (i.e., wastewater and/or nonwastewater) specified for that alternate standard.
7	Both Cyanides (Total) and Cyanides (Amenable) for nonwastewaters are to be analyzed using Method 9010 or 9012, found in "Test Methods for Evaluating Solid Waste, Physical/Chemical Methods", EPA Publication SW-846, as incorporated by reference in 40 CFR 260.11, with a sample size of 10 grams and a distillation time of one hour and 15 minutes.
8	These wastes, when rendered nonhazardous and then subsequently managed in CWA, CWA-equivalent, or Class I SDWA systems are not subject to treatment standards.  (See §148.1(d) and §268.1(c)(3) and (4)).
9	These wastes, when rendered nonhazardous and then subsequently injected in a Class I SDWA well are not subject to treatment standards.  (See §148.1(d)).

BILLING CODE 1505_01_D